3GPP TSG RAN WG1 Meeting #103-e R1-200xxxx

**e-Meeting, Oct. 26th – Nov. 13th, 2020**

**Source: Moderator (ZTE)**

Title: FL summary #3 on SRS enhancements

Agenda Item: 8.1.3

Document for: Discussion and Decision

# Introduction

In RAN#86, the Rel-17 WID of further enhancements on MIMO for NR is approved [1]. In the approved WID, a particular point is about SRS enhancements in terms of flexibility, coverage and capacity, targeting both FR1 and FR2. The detailed scope of the SRS enhancement is given as follows.

*3. Enhancement on SRS, targeting both FR1 and FR2:*

* 1. *Identify and specify enhancements on aperiodic SRS triggering to facilitate more flexible triggering and/or DCI overhead/usage reduction*
	2. *Specify SRS switching for up to 8 antennas (e.g., xTyR, x = {1, 2, 4} and y = {6, 8})*
	3. *Evaluate and, if needed, specify the following mechanism(s) to enhance SRS capacity and/or coverage: SRS time bundling, increased SRS repetition, partial sounding across frequency*

The relevant agreements made in previous RAN1 meetings are given in Appendix.

In this contribution, we summarize companies’ views on the above SRS enhancements submitted to RAN1#103e [2]-[27].

# Usage/overhead reduction

After Wednesday GTW session, the only left issue is a proposed conclusion for the discussion of Rel-17 SRS enhancement.

***Proposed conclusion:***

*For the purpose of Rel-17 SRS enhancement, the following is assumed:*

*A Rel-15/16 UE that supports nT=nR antenna switching with n={1,2,4} can be configured with an n port SRS resource that is in both an SRS resource set with usage=’codebook’ and another SRS resource set with usage=’antennaSwitching’, provided that the SRS resource sets have the same time domain behavior.*

* *The existing conclusions/agreements for Rel-15/16 is unchanged.*

Let’s focus on this nTnR case. Companies are encouraged to indicate whether the proposed conclusion is acceptable, or any suggestion to refine it.

Companies’ further views are collected as follows.

|  |  |
| --- | --- |
| Companies | Views |
|  |  |
|  |  |
|  |  |

# Further discussion in next meeting

This section is intended to give some general guidance on further discussion points in next meeting. These aspects are either relative hot discussion points in RAN1#103e without clear conclusion, or necessary components to complete the already agreed features. Companies are encouraged to share your views on these aspects in your contribution submitted to RAN1#104e.

For further discussion in next RAN1 meeting

SRS triggering flexibility enhancement

* Detailed definition of available slot
* Down-selection between Opt. 1 and Opt. 2 for reference slot
* Detailed mechanism on DCI indication of t
* Whether/how to re-purpose unused fields in DCI format 0\_1 and 0\_2, when aperiodic SRS is triggered without data and without CSI
* Whether to support group-common DCI enhancements for SRS triggering
* Whether to support specification enhancement for SRS resource reuse between the usages of nTmR antenna switching and codebook based UL, where n<m
* Whether to support relevant enhancement for indicating a subset of Tx/Rx antennas in SRS antenna switching

SRS antenna switching for up to 8Rx

* Whether 4T6R is supported in addition
* Detailed SRS resource set configuration for each xTyR in the agreed set of {1T6R, 1T8R, 2T6R, 2T8R, 4T8R}

SRS capacity and coverage enhancements

* Down-selection from Scheme 2-0 to Scheme 2-3 in Class 2, and/or Scheme 3-1 to Scheme 3-5 in Class 3

# Conclusion

# Appendix

## Previous agreements

|  |
| --- |
| **RAN1#102e****Agreement**Enhance the determination of aperiodic SRS triggering offset, with at least one of the following alternatives* + Alt 1: Delay the SRS transmission to an available slot later than the triggering offset defined in current specification, including possible re-definition of the triggering offset
	+ Alt 2: Indicate triggering offset in DCI explicitly or implicitly
	+ Alt 3: Update triggering offset in MAC CE
	+ Further consideration aspects may include the cost v.s. the total combinations PDCCH and SRS locations for gNB to choose, DCI overhead, multi-UE SRS multiplexing, CA aspect, whether to have multiple opportunities to transmit SRS, etc.

**Agreement**Study the following two alternatives in the scope to enhance at least one DCI format for aperiodic SRS triggering * + Alt 1: Use UE-specific DCI, e.g., extending DCI 0\_1 without uplink data and without CSI
	+ Alt 2: Use group-common DCI, e.g., extending DCI 2\_3 for cases other than carrier switching
	+ Further consideration aspects may include simultaneous or CC-specific SRS triggering for multiple CCs, dynamic indication of SRS frequency resources, etc..

**Agreement**For SRS overhead reduction, study reusing same resources among multiple usages, at least for “codebook” and “antenna switching”. Study aspects include* + Whether implementation approach based on legacy SRS configuration is sufficient
		- If not, and if there are benefits other than RRC overhead reduction, study further on the case that antenna switching and PUSCH have different number of Tx antennas, whether UL BWP for different SRS usages is the same or different, whether and how to ensure UE to use same virtualization, the set of applicable usages, UE implementation complexity and overhead, etc..

**Agreement**For SRS antenna switching up to 8Rx, study the configuration of {1T6R, 1T8R, 2T6R, 2T8R, 4T6R, 4T8R}.* + Study points may include CSI latency, performance considering aspects like insertion loss, use cases, antenna structure, UE power saving, SRS resource configuration, etc..

**Agreement**For SRS coverage/capacity enhancements, evaluate and, if needed, specify one or more from three categories based on the following definition. * + Class 1 (Time bundling): Utilize relationship among two or more occasions of one or more SRS resources in one or more slots to enable joint processing within time domain.
		- Study aspects include the issue of phase discontinuity, interruption of SRS transmission by other UL signals, etc..
	+ Class 2 (Increase repetition): Change the legacy SRS pattern in one resource and one occasion from time domain by increasing SRS symbols for repetition.
		- Study aspects include to use TD-OCC to compensate the negative impact on SRS capacity, inter-cell interference randomization, whether these SRS symbols are in one slot or consecutive slots, etc..
	+ Class 3 (Partial frequency sounding): Support more flexibility on SRS frequency resources to allow SRS transmission on partial frequency resources within the legacy SRS frequency resources.
		- Study aspects include the partial frequency resources are with RB level or subcarrier level (e.g., larger comb, partial bandwidth), PAPR issue, etc..

**RAN1#103e****Agreement**A given aperiodic SRS resource set is transmitted in the (t+1)-th available slot counting from a reference slot, where t is indicated from DCI, or RRC (if only one value of t is configured in RRC), and the candidate values of t at least include 0. Adopt at least one of the following options for the reference slot.* Opt. 1: Reference slot is the slot with the triggering DCI.
* Opt. 2: Reference slot is the slot indicated by the legacy triggering offset.
* FFS the detailed definition of “available slot” considering UE processing complexity and timeline to determine available slot, potential co-existence with collision handling, etc., e.g.,
	+ Based on only RRC configuration, “available slot” is the slot satisfying: there are UL or flexible symbol(s) for the time-domain location(s) for all the SRS resources in the resource set and it satisfies the minimum timing requirement between triggering PDCCH and all the SRS resources in the resource set
* FFS explicit or implicit indication of t
* FFS whether updating candidate triggering offsets in MAC CE may be beneficial

**Agreement**Support at least DCI 0\_1 and 0\_2 to trigger aperiodic SRS without data and without CSI.* FFS whether/how to re-purpose the unused fields, e.g., the triggering offset(s) and the frequency resources for triggering A-SRS on one or more component carriers, SFI-index, etc.
* FFS UL/DL DCI with data for aperiodic SRS
* FFS group common DCI

**Agreement**In Rel-17 SRS coverage and capacity enhancement, support at least one scheme from Class 2 and Class 3, and deprioritize Class 1.* Note: Extensions of Rel-15/16 frequency hopping are included in Classes 2 and 3, e.g. where UE hops once per symbol within a Rel-17 SRS resource.

**Agreement**Candidate schemes for Class 2:* Scheme 2-0: Increase the number of repetition symbols in one slot
* Scheme 2-1: Inter-slot repetition on consecutive symbols or non-consecutive symbols across slots
* Scheme 2-2: Repetition with TD-OCC
* Scheme 2-3: Repetition with CS hopping

Candidate schemes for Class 3:* Scheme 3-1: RB-level partial frequency sounding
* Scheme 3-2: Subcarrier-level partial frequency sounding
* Scheme 3-3: Subband-level partial frequency sounding
* Scheme 3-4: Partial-frequency sounding schemes assisted with CSI-RS, where SRS is transmitted in a subset of RBs of the original SRS frequency resource
* Scheme 3-5: Dynamic change of SRS bandwidth with RB-level subband size scaling
* Note: Consider issues like gNB receiver complexity, PAPR, etc., with above schemes
* Note: Joint operation between Class 2 and Class 3 schemes can be considered

**Agreement**For antenna switching up to 8Rx, support SRS resource configurations for {1T6R, 1T8R, 2T6R, 2T8R, [4T6R], 4T8R}. |

# References

[1] RP-193133, New WID: Further enhancements on MIMO for NR, Samsung

[2] R1-2007544, Enhancements on SRS flexibility, coverage and capacity, FUTUREWEI

[4] R1-2007591, Discussion on SRS enhancements for Rel-17, Huawei, HiSilicon

[5] R1-2007631, Discussion on SRS Enhancements, InterDigital, Inc.

[6] R1-2007649, Further discussion on SRS enhancement, vivo

[7] R1-2007768, Enhancements on SRS flexibility, coverage and capacity, ZTE

[8] R1-2007829, On enhancements on SRS flexibility, coverage and capacity, CATT

[9] R1-2008005, Enhancements on SRS flexibility, coverage and capacity, CMCC

[10] R1-2008153, Enhancements on SRS, Samsung

[11] R1-2008222, Enhancements on SRS flexibility, coverage and capacity, OPPO

[12] R1-2008351, Considerations on SRS flexibility, coverage and capacity, Sony

[13] R1-2008443, Views on Rel-17 SRS enhancement, Apple

[14] R1-2008578, Enhancements on SRS flexibility, coverage and capacity, LG Electronics

[15] R1-2008900, Enhancements on SRS for coverage and capacity, Fraunhofer IIS, Fraunhofer HHI

[16] R1-2008908, Enhancements on SRS flexibility, coverage and capacity, Nokia, Nokia Shanghai Bell

[17] R1-2008914, Enhancements on SRS, Lenovo, Motorola Mobility

[18] R1-2008948, Discussion on SRS enhancement, NEC

[19] R1-2008959, Enhancements on SRS flexibility, coverage and capacity, MediaTek Inc.

[20] R1-2008982, Discussion on SRS enhancements, Intel Corporation

[21] R1-2009031, Discussion on SRS enhancements, Xiaomi

[22] R1-2009131, Enhancements on SRS, Sharp

[23] R1-2009146, Considerations on SRS enhancement, Spreadtrum Communications

[24] R1-2009179, Discussion on SRS enhancement, NTT DOCOMO, INC.

[25] R1-2009211, SRS Performance and Potential Enhancements, Ericsson LM

[26] R1-2009255, Enhancements on SRS flexibility, coverage and capacity, Qualcomm Incorporated

[27] R1-2009286, Discussion on enhancement of SRS in Rel. 17 further enhanced MIMO, CEWiT