**3GPP TSG RAN WG1 #104-e R1-200XXXX**

**e-Meeting, January 25th – February 5th, 2021**

**Agenda item: 8.12.3**

**Source:** Moderator (BBC)

**Title:** Summary # 2 on RAN basic functions for broadcast/multicast for UEs in RRC\_IDLE/ RRC\_INACTIVE states

**Document for:** Discussion and Decision

# Introduction

RAN1#104-e is the second meeting that discusses the AI 8.12.3 on Basic functions for broadcast/multicast for RRC\_IDLE/ RRC\_INACTIVE UEs. The information of the email thread on this topic and the check points on the discussion provided by RAN1 Chairman is shown below:

[104-e-NR-MBS-03] Email discussion/approval on basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs with checkpoints for agreements on Jan-28, Feb-02, Feb-05 – David (BBC)

A summary of the analysis and key issues identified from the technical inputs to this meeting to AI 8.12.3 can be found in R1-2101721 ([Inbox](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_104-e/Inbox/R1-2101721.zip)).

Section 2 includes an initial proposal of High Priority issues for discussion at RAN1#104-e. Section 3 includes an initial proposal on Medium Priority issues for discussion at RAN1#104-e. Each Issue includes Initial FL proposals where companies are welcomed to provide their inputs.

Please use the “Navigation Pane” of Word to quickly find the proposals and the different rounds of discussions in this document.

Section 4 will include any agreements reached from the discussions.

# Discussion on High Priority Issues

## Issue 1: MBS Common Frequency Resource: relation to the Initial BWP

### **Initial FL proposals for Issue 1**

**Proposal 1**: For RRC\_IDLE/RRC\_INACTIVE UEs, the defined/configured common frequency resource for group-common PDCCH/PDSCH contains the initial BWP and has the same SCS and CP as the initial BWP.

**Proposal 2**: For RRC\_IDLE/RRC\_INACTIVE UEs, the initial BWP contains the defined/configured common frequency resource for group-common PDCCH/PDSCH.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 2: Number of MBS Common Frequency Resources

### **Initial FL proposal for Issue 2**

**Proposal 3**: For RRC\_IDLE/RRC\_INACTIVE UEs, one common frequency resource for group-common PDCCH/PDSCH can be defined/configured.

* FFS: whether to define/configure more than one common frequency resources
* FFS: if more than one common frequency resource are configured, either the common frequency resource can be fully confined within the initial BWP and other configured common frequency resources, or the common frequency resource can be configured to contain the entire initial BWP and other common frequency resources**.**

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 3: Configuration/Definition of MBS Common Frequency Resources

### **Initial FL proposals for Issue 3**

**Proposal 4**: For RRC\_IDLE/RRC\_INACTIVE UEs, for the case that the common frequency resource for group-common PDCCH/PDSCH is larger than the Initial BWP (if supported), define a MBS specific BWP.

* FFS: details on start PRB, length PRB and reuse of SILV indication mechanisms.

**Proposal 5**: For RRC\_IDLE/RRC\_INACTIVE UEs, for the case that the Initial BWP contains the common frequency resource for group-common PDCCH/PDSCH (if supported), configure a MBS frequency resource within the Initial BWP.

* FFS: details on start PRB, length PRB and reuse of SILV indication mechanisms.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 4: CORESET configuration for group-common PDCCH/PDSCH

### **Initial FL proposals for Issue 4**

**Proposal 6**: For RRC\_IDLE/RRC\_INACTIVE UEs, network can configure the common CORESET configured by RRC signalling *commonControlResourceSet* for group-common PDCCH/PDSCH if the common frequency resource is the initial BWP and a CORESET is not configured.

**Proposal 7**: For RRC\_IDLE/RRC\_INACTIVE UEs, multiple CORESETs can be configured for the defined/configured common frequency resource for group-common PDCCH/PDSCH.

* the same configured CORESET can be used to schedule MBS control information reception, broadcast, multicast and unicast.
* multiple CORESETs can be configured to independently schedule different MBS services and/or channels for control and traffic.
* FFS: definition of new RRC parameters to configure CORESET in a common frequency resource larger than Initial BWP (if supported).

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 5: Search Space (SS) for group-common PDCCH/PDSCH

### **Initial FL proposal for Issue 5**

**Proposal 8**: For RRC\_IDLE/RRC\_INACTIVE UEs, a new CSS type is defined for group-common PDCCH.

* FFS: monitoring priority with respect to existing CSS and USS.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 6: Beam Sweeping for group-common PDCCH/PDSCH

### **Initial FL proposal for Issue 6**

**Proposal 9**: For RRC\_IDLE/RRC\_INACTIVE UEs, the UE may assume that group-common PDCCH/PDSCH is QCL’d with SSB if configured.

* UE monitoring occasions are associated with a subset of the total SSB indexes in a timing window.
	+ FFS: definition details of timing window such as periodicity and offset
	+ FFS: association rules between SSB indexes and UE monitoring occasions.
* for broadcast reception, full beam sweeping is supported.
* FFS: (re)use of RRC\_CONNECTED beam configuration for RRC\_IDLE/RRC\_INACTIVE UEs states.
* FFS: group-common PDCCH/PDSCH is QCL’d with TRS if configured.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 7: HARQ feedback for RRC\_IDLE/RRC\_INACTIVE UE states

### **Initial FL proposal for Issue 7**

**Proposal 10**: For RRC\_IDLE/RRC\_INACTIVE UEs, study the potential support of HARQ feedback.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

# Discussion on Medium Priority Issues

## Issue 8: PDSCH repetition

### **Initial FL proposals for Issue 8**

**Proposal 11**: For RRC\_IDLE/RRC\_INACTIVE UEs, support slot-level repetition for group-common PDSCH.

* semi-static and dynamic slot-level repetition number configured by higher layer signalling.
* FFS: support of consecutive slot-level and RV-based time-interleaving for group-common PDSCH.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 9: PDSCH Semi Persistent Scheduling

### **Initial FL proposals for Issue 9**

**Proposal 12**: Support SPS group-common PDSCH for MBS for RRC\_IDLE/RRC\_INACTIVE UEs.

* FFS: whether to support more than one SPS group-common PDSCH configuration per UE

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 10: MBS Common Frequency Resource: relation with Unicast BWP

### **Initial FL proposals for Issue 10**

**Proposal 13**:for broadcast reception, the same group-common PDCCH and the corresponding scheduled group-common PDSCH can be received by both RRC\_IDLE/RRC\_INACTIVE UEs and RRC\_CONNECTED UEs when UE-specific active BWP of RRC\_CONNECTED UE contains the common frequency resource of RRC\_IDLE/INACTIVE UEs.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

## Issue 11: Multicast reception by UEs in IDLE/INACTIVE states

### **Initial FL proposals for Issue 11**

**Proposal 14**:For RRC\_IDLE/RRC\_INACTIVE UEs, Multicast reception with high QoS requirement (reliability, latency) is not supported for UEs in RRC\_IDLE/RRC\_INACTIVE states.

* FFS: multicast reception with low QoS requirement (reliability, latency) for For RRC\_IDLE/RRC\_INACTIVE UEs, subject to final RAN2 confirmation.

Please provide your company’s views and comments in the table below:

|  |  |
| --- | --- |
| **company** | **comments** |
|  |  |

# Summary

# References

1. RP-201038 Revised Work Item on NR Multicast and Broadcast Services, Huawei, HiSilicon
2. R1-2100108 Discussion on basic Functions for Broadcast or Multicast for RRC\_IDLE or RRC\_INACTIVE UEs, ZTE
3. R1-2100146 Discussion on support for IDLE and INACTIVE state UEs, OPPO
4. R1-2100191 Discussion on multicast support for IDLE/INACTIVE UEs, Huawei, HiSilicon
5. R1-2100356 Discussion on basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs, CATT, CBN
6. R1-2100471 Discussion on basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE Ues, vivo
7. R1-2100512 Basic Functions for Broadcast / Multicast for RRC\_IDLE / RRC\_INACTIVE Ues, Nokia, Nokia Shanghai Bell
8. R1-2100615 Common frequency resource for NR PTM transmission, MediaTek Inc.
9. R1-2100676 NR-MBS for RRC\_IDLE/INACTIVE UEs, Intel Corporation
10. R1-2100770 Basic functions for broadcast/multicast in idle/inactive states, Lenovo, Motorola Mobility
11. R1-2100873 Considerations on MBS functions for RRC\_IDLE UEs, Sony
12. R1-2100908 Basic function for broadcast/multicast, LG Electronics
13. R1-2101065 Discussion on NR MBS in RRC\_IDLE/ RRC\_INACTIVE states, CMCC
14. R1-2101236 On basic functions for broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs, Samsung
15. R1-2101361 Discussion on MBS for RRC\_IDLE/RRC\_INACTIVE UEs, Apple
16. R1-2101426 On NR multicast and broadcast for RRC\_IDLE/RRC\_INACTIVE UEs, Convida Wireless
17. R1-2101489 Views on group scheduling for Multicast RRC\_IDLE/INACTIVE UEs, Qualcomm Incorporated
18. R1-2101638 Basic functions for MBS for RRC\_IDLE/RRC\_INACTIVE UEs, CHENGDU TD TECH LTD.
19. R1-2101728 Support for NR multicast reception in RRC Inactive/Idle, Ericsson
20. R1-2009276 *Discussion on broadcast/multicast for RRC\_IDLE/RRC\_INACTIVE UEs*, Qualcomm Incorporated
21. R1-2009307 *Support for NR multicast reception in RRC Inactive/Idle*, Ericsson