**3GPP TSG RAN WG2 Meeting #117-e**   **R2-220xxxx**

**E-Meeting, 21st February – 3rd March 2022**

**Agenda Item:** **6.1.4.3**

**Source:**  **Intel Corporation**

**Title:** **Summary report of [AT117-e][034][NR16] UE capabilities I (Intel)**

**Document for:** **Discussion/Decision**

# Introduction

This is to kick-off the following offline discussion:

* [AT117-e][034][NR16] UE capabilities I (Intel)

 Scope: Treat R2-2202146, R2-2202107, R2-2202665, R2-2203163, R2-2203167, R2-22002195, R2-2202196, R2-2203488, R2-2202293. Ph1 Determine agreeable parts, Ph2 for agreeable parts, progress CRs.

 Intended outcome: Report, Agreed CRs.

 Deadline: Schedule 1

For Schedule 1:

A **first round** with **Deadline for comments W1 Thur Feb 24th 1200 UTC** to settle scope what is agreeable etc

A Final round with **Final deadline W2 Wed March 2nd 1200 UTC** to settle details / agree CRs etc.

# Companies’ point of contact

|  |  |  |
| --- | --- | --- |
| **Company** | **Point of contact** | **Email address** |
| Intel Corporation | Seau Sian Lim | seau.s.lim@intel.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Leftover issues for DAPS capability

The following papers are for DAPS remaining issues:

|  |
| --- |
| DAPSR2-2202195 Left issues on DAPS capability OPPO discussion Rel-16 NR\_Mob\_enh-CoreR2-2203488 Discussion on DAPS capabilities and configuration Huawei, HiSilicon discussion Rel-15 NR\_newRAT-CoreR2-2202293 Correction on DAPS capability OPPO CR Rel-16 38.306 16.7.0 0677 - F NR\_Mob\_enh-Core |

In Ph1, we could focus on proposals in discussion papers, and leave the CR part to Ph2.

**Signalling structure:**

**In RAN2#116, the following agreements were made:**

|  |
| --- |
| * [012] The capability for source/target cell in intra-frequency DAPS handover is derived based on a pair of per-CC feature-set ID in the same band-entry, and  the capability for source/target cell in inter-frequency DAPS handover is derived from a pair of per-CC feature-set ID in the same or different band entries. Correction in TS 38.306 is needed to clarify this.
 |

In R2-2203488, a further proposal is made to discuss whether the same two FSPC IDs can be reported for a band intra-frequency DAPS capability within DAPS FSC, while in case of CA normally different FSPC IDs are included for a band.

|  |
| --- |
| **Observation1: The DAPS capability should be derived from a pair of FSPCs for both intra-freq and inter-freq DAPS.**For the FSPC IDs reported by UE in a DAPS FeatureSetCombination, there is network coordination between the source and target cell. The target can determine which one of FSPC ID to use based on the received source configuration. This principle should be applicable for both intra-freq DAPS and inter-freq DAPS. Thus, for a band with intra-freq DAPS capability, same or different FSPC IDs should be allowed to report within DAPS FSC. **Proposal 1: Same or different FSPC IDs are allowed to report for a band with intra-frequency DAPS capability within DAPS FSC.**  |

**Question 3-1: Whether the following proposals can be agreeable?**

|  |
| --- |
| **Proposal 1: Same or different FSPC IDs are allowed to report for a band with intra-frequency DAPS capability within DAPS FSC.** |

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
| Intel | Y | it’s possible that source cell and target cell have the same FSPC capabilities. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Applicability of legacy CA BC capabilities:**

In RAN2#116 meeting, the following agreement was made, and one discussion point was postponed:

|  |
| --- |
| * [012] RAN2 confirms: the legacy reported field of 1) frequency-separation and 2) BCS is not applicable for intra-frequency DAPS handover.
* [012] RAN2 further discuss that, for inter-frequency DAPS HO cases where the BW of source and target cells are NOT overlapping with each other, the 1) BW-class, 2) frequency-separation and 3) BCS restriction reported in the same BC-entry are all applicable to DAPS FSC.
 |

In R2-2203488, a general proposal regarding this leftover issue is made as below:

|  |
| --- |
| **Proposal 2: For inter-frequency DAPS HO cases where the BW of source and target cells are not overlapping with each other, the 1) BW-class, 2) frequency-separation and 3) BCS restriction reported in the same BC-entry are all applicable to DAPS FSC.** |

While in R2-2202195, the proposals with a detailed differentiation between BWC D/E, BWC B/C and BWC A are provided as follows:

|  |
| --- |
| **Proposal 1 R2 discuss that BWC of D/E and above (and BCS, frequency separation in case of BWC D/E and above) are 1) not applicable to DAPS FSC for inter-frequency DAPS, or 2) applicable to DAPS FSC for inter-frequency DAPS based on 2-CC fallback BC.****Proposal 2 R2 discuss that BWC of B/C (and BCS, frequency separation in case of BWC B/C) for intra-band non-continguous BC or inter-band BC are 1) not applicable to DAPS FSC for inter-frequency DAPS HO, or 2) applicable to DAPS FSC for inter-frequency DAPS based on 2-CC fallback BC.****Proposal 3 R2 clarify BWC of B/C and BCS in case of BWC B/C for intra-band continguous BC is applicable to DAPS FSC for inter-frequency DAPS HO.****Proposal 4 R2 clarify for intra-band non-continguous BC and inter-band BC limited to BWC A, frequency separation (only valid for intra-band non-continguous BC) and BCS is applicable to DAPS FSC for inter-frequency DAPS HO.** |

In Ph1, at least some general question can be asked, and companies can provide exceptions if any.

**Question 3-2: Whether the following proposal can be agreeable? And please indicate the exception if any.**

|  |
| --- |
| **Proposal 2: For inter-frequency DAPS HO cases where the BW of source and target cells are not overlapping with each other, the 1) BW-class, 2) frequency-separation and 3) BCS restriction reported in the same BC-entry are all applicable to DAPS FSC.** |

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
| Intel | Y | The basic principle is to reuse CA UE capability for DAPS, and consider DAPS as a two-CC CA. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Synchronous DAPS capability:**

In R2-2203488, the following proposals are made to clarify the synchronous DAPS capability:

|  |
| --- |
| In our view, if there is the case that syncDAPS only capability is supported, one possible way is to report the intrafreqDAPS-r16 or interfreqDAPS-r16 IE without any sub-field included. Besides, in this case, the intra-freq and inter-freq syncDAPS capability should be understood separately by including corresponding IE.**Proposal 3: If the intraFreqDAPS-r16 is included and no sub-fields are included inside, it indicates support of intra-frequency syncDAPS handover.****Proposal 4: If the interFreqDAPS-r16 is included and no sub-fields are included inside, it indicates support of inter-frequency syncDAPS handover.** |

**Question 3-3: Whether the following proposals can be agreeable?**

|  |
| --- |
| **Proposal 3: If the intraFreqDAPS-r16 is included and no sub-fields are included inside, it indicates support of intra-frequency syncDAPS handover.****Proposal 4: If the interFreqDAPS-r16 is included and no sub-fields are included inside, it indicates support of inter-frequency syncDAPS handover.** |

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
| Intel | Y | sub-fields are optional, and they don’t affect the support of syncDAPS. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Clarifications on multi-TRP configuration for DAPS:**

In R2-2203488, the following proposals are made to clarify the mTRP restriction on DAPS:

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| We think it is worth to figure out the detailed configuration so that the network is clear on the restrictions, and our suggestions are as below (details can be found in section 5.3):

|  |  |  |
| --- | --- | --- |
| **Feature** | **Configurations** | **Note** |
| Multi-DCI based multi-TRP | *coresetPoolIndex-r16* in *ControlResourceSet* | RRC configuration(defined in TS 38.331) |
| TDM/FDM based Single-DCI based multi-TRP | *repetitionSchemeConfig-r16/ repetitionSchemeConfig-v1630* in *PDSCH-Config* | RRC configuration(defined in TS 38.331) |
| SDM based Single-DCI based multi-TRP | Enhanced TCI States Activation/Deactivation for UE-specific PDSCH MAC CE | MAC configuration(defined in section 6.1.3.24 in TS 38.321) |

**Proposal 5: For DAPS configuration, the terminology multi-DCI/single-DCI based multi-TRP refers to the following definitions:****- Multi-DCI based multi-TRP: configured via the coresetPoolIndex-r16 IE in the ControlResourceSet IE****- TDM/FDM based Single-DCI based multi-TRP: configured via the repetitionSchemeConfig-r16/repetitionSchemeConfig-v1630 IE in the PDSCH-Config IE****- SDM based Single-DCI based multi-TRP: configured via the enhanced TCI States Activation/Deactivation for UE-specific PDSCH MAC CE, as specified in TS 38.321** |

**Question 3-4: Whether the following proposal can be agreeable?**

|  |
| --- |
| **Proposal 5: For DAPS configuration, the terminology multi-DCI/single-DCI based multi-TRP refers to the following definitions:****- Multi-DCI based multi-TRP: configured via the coresetPoolIndex-r16 IE in the ControlResourceSet IE****- TDM/FDM based Single-DCI based multi-TRP: configured via the repetitionSchemeConfig-r16/repetitionSchemeConfig-v1630 IE in the PDSCH-Config IE****- SDM based Single-DCI based multi-TRP: configured via the enhanced TCI States Activation/Deactivation for UE-specific PDSCH MAC CE, as specified in TS 38.321** |

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
| Intel | Probably No | This is not related to UE capability, but more about DAPS configuration. It would be better to discuss this as part of RRC configuration discussion. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Miscellaneous updates on TR38.822

The CR [4] has the following reason for change:

Updates the feature list tables in TS38.822 based on the following:

* R2-2109178 Miscellaneous corrections to 38.306
* R4-2118537 R4 feature list – The corresponding 38.306/331 CRs are already agreed in R2-2111502 and R2-2111503 on TX diversity
* R1-2112777 R1 feature list

**Q5 Do companies agree with the proposed changes in the CR? For companies agreeing to the proposed changes, please also comment on the contents of the CR, if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Intel | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Rename of field extendedBand-n77

The CR [6] has the following reason for change:

* Field extendedBand-n77 has the suffix of r16 based on RP decision (RP-212598). After the ASN.1 frozen for the release, the suffix should use the version number (i.e. v1660, not r16 in this case) to track when the change occurs.

**Q6-1 Do companies agree with the proposed changes in the CR? For companies agreeing to the proposed changes, please also comment on the contents of the CR, if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Intel | No | As the field is not a non-critical extension of an existing field, the suffix of ‘-r16’ should be used. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

The CR [5] has the following reason for change:

* Field extendedBand-n77 has the suffix of r16 based on RP decision (RP-212597). However suffix is not specified in TS 38.306 unless it has to be distinguished explicitly.

As TS38.306 rapporteur point of view, unlike in TS38.331, suffix of a release (e.g. xxxx-r16) is included in field name in the field description to allow fast knowledge of the release of a UE capability. Hence the change is not correct.

**Q6-2 Do companies agree with the proposed changes in the CR? For companies agreeing to the proposed changes, please also comment on the contents of the CR, if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Intel | No | Agree with the rapporteur. The actual field name should be the same as the TS38.331 including the suffix. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

To be added latter

# References

[1] R2-2202195 Left issues on DAPS capability OPPO discussion Rel-16 NR\_Mob\_enh-Core

[2] R2-2202293 Correction on DAPS capability OPPO CR Rel-16 38.306 16.7.0 0677 - F NR\_Mob\_enh-Core

[3] R2-2203488 Discussion on DAPS capabilities and configuration Huawei, HiSilicon discussion Rel-15 NR\_newRAT-Core

[4] R2-2202665 Miscellaneous updates on TR38.822 Intel Corporation CR Rel-16 38.822 16.2.0 0009 - F NR\_pos-Core, NR\_RF\_TxD-Core, NR\_unlic-Core, NR\_IAB-Core

[5] R2-2203163 Rename of field extendedBand-n77 Samsung R&D Institute UK CR Rel-16 38.306 16.7.0 0691 - D NR\_RF\_FR1-Core

[6] R2-2203167 Rename of field extendedBand-n77 Samsung R&D Institute UK CR Rel-16 38.331 16.7.0 2931 - D NR\_RF\_FR1-Core

[7] R2-2202107 LS on updated Rel-16 RAN1 UE features lists for NR after RAN1#107-e (R1-2112778; contact: NTT DOCOMO) RAN1 LS in Rel-16 To:RAN2 Cc:RAN4

[8] R2-2202146 LS on Rel-16 updated RAN4 UE features lists for LTE and NR (R4-2118536; contact: CMCC) RAN4 LS in Rel-16 To:RAN2 Cc:RAN1