3GPP TSG-RAN WG3 Meeting #107-e draft R3-201234

E-meeting, 24 Feb – 6 Mar 2020

**Agenda item: 9.2**

**Source: Nokia, Nokia Shanghai Bell**

**Title: Summary of the email discussion #101bis (ReviseProcTxtX2AP)**

**Document for: Endorsement**

# 1 Introduction

At RAN3 #107-e meeting, an email discussion was initiated to clarify correction to the description of the usage of the RRC container in the SN-initiated release procedure.

The paper summarises the discussion and proposes conclusions.

# 2 Discussion

During the email exchange, the scenario was clarified to concern SN change situation with delta configuration, where SCG configuration is not released in the UE.

Following text is proposed to be used in the CRs:

If the*SgNB to MeNBContainer* IE is included in the SGNB RELEASE REQUIRED message the MeNB / M-NG-RAN node may use the contained information to apply delta configuration.

# 3 Conclusions

It is proposed to agree the corresponding CRs in [1] and [2].

# References

1. R3-201235, RAN3 #107-e
2. R3-201236, RAN3 #107-e