**3GPP TSG-RAN WG3 Meeting #117-e *R3-22xxxx***

***E-meeting, 15-24 Aug 2022***

**Title:** [draft] **Reply LS on QoE configuration and reporting related issues**

**Response to:** **LS S5-223518**

**Release: Release 17**

**Work Item: eQoE**

**Source: Huawei [will be RAN3]**

**To: SA5, SA4**

**Cc: RAN2**

**Contact person: Jingcong Sun**

**Sunjingcong@huawei.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** **None**

1 Overall description

RAN3 thanks to SA5 for the LS on QoE configuration and reporting related issues.

RAN3 would like to inform that in current RAN3 specification, it is supported to configure multiple different slices for the same service type but only with the same *QMC MCE* address. In order to configure different *QMC MCE* IP addresses for the different slices of the same service type, it can be realized by configuring multiple different QoE measurements, where each QoE configuration contains one or moreslices and the corresponding *QMC MCE* IP address, without any specification changes.

2 Actions

**To SA5 and SA4:**

**ACTION: RAN3 kindly asks SA5 and SA4 to take the feedback above into account.**

3 Dates of next RAN3 meetings

RAN3#117-bis-e 2022-10-10 - 2022-10-18

RAN3#118 2022-11-14 - 2022-11-18 TBD