**3GPP TSG RAN WG3 Meeting #127bis R3-25xxxx**

**Wuhan, China, 07-11 April, 2025**

**Title: LS on Average Window for Alternative QoS**

**Response to: -**

**Release: REL-18**

**Work Item: NR\_XR\_enh-Core**

**Source: RAN3**

**To: SA2**

**Cc: -**

**Contact person: liuziqiao@catt.cn**

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** -

# 1 Overall description

RAN3 notices the misalignment on Average Window between RAN3 and SA2 specifications.

Current SA2 specification has following statement but RAN3 specifications do not include Averaging Window in the Alternative QoS Parameters.

*An* ***Alternative QoS Profile*** *represents a combination of QoS parameters PDB, PER,* ***Averaging Window*** *and GFBR to which the application traffic is able to adapt.*

RAN3 would like to ask SA2 to clarify why the SA2 specification above includes Averaging Window in Alternative QoS Profile, and to reply whether the Averaging Window in QoS Flow level QoS parameters can be used for Alternative QoS.

# 2 Actions

**To SA2**

**ACTION:** RAN3 kindly asks SA2 to provide feedback on above question.

# 3 Dates of next TSG RAN WG3 meetings

RAN3#128 19 - 23 May 2025 Malta, MT

RAN3#129 25 - 29 August 2025 Bangalore, IN