**3GPP TSG-RAN WG3 Meeting #128R3-253835**

**Malta, MT, 19-23 April 2025**

Agenda Item: 21.3

Source: ZTE Corporation, China Telecom, Nokia, Nokia Shanghai Bell

Title: [TP to XR BL CR for 38.473] Fix for the FFS

Document for: Other & Approval

# 1 Introduction

This TP adds the following changes:

1. **define available bitrate and threshold as a 32-bit integer with unit kbps.**
2. **Use value “8” for maxnoofThresholds for available data rate reporting**
3. **Remove FFS on MMSID octet string size.**

This annex below provides the TP to BLCR for TS38.473.

TP to BL CR for TS 38.473

9.3.1.26 QoS Flow Level QoS Parameters

This IE defines the QoS parameters to be applied to a QoS Flow.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| CHOICE *QoS Characteristics* | M |  |  |  | - |  |
| *>Non-dynamic 5QI* |  |  |  |  |  |  |
| >>Non Dynamic 5QI Descriptor | M |  | 9.3.1.27 |  | - |  |
| *>Dynamic 5QI* |  |  |  |  |  |  |
| >>Dynamic 5QI Descriptor | M |  | 9.3.1.28 |  | - |  |
| NG-RAN Allocation and Retention Priority | M |  | 9.3.1.29 |  | - |  |
| GBR QoS Flow Information | O |  | 9.3.1.30 | This IE shall be present for GBR QoS Flows and is ignored otherwise. | - |  |
| Reflective QoS Attribute | O |  | ENUMERATED (subject to, …) | Details in TS 23.501 [20]. This IE applies to Non-GBR flows only and is ignored otherwise. | - |  |
| Additional QoS Flow Information | O |  | ENUMERATED (more likely, …) | This IE indicates that traffic for this QoS flow is likely to appear more often than traffic for other flows established for the PDU Session. | - |  |
| Paging Priority Index | O |  | INTEGER(1.. 8, …) | This IE is not used in this version of the specification. | - |  |
| RDI | O |  | ENUMERATED (enabled, …) | Indicates whether Reflective QoS flow to DRB mapping should be applied. | - |  |
| QoS Monitoring Request | O |  | ENUMERATED (UL, DL, Both, …) | Indicates to measure UL, or DL, or both UL/DL delays for the associated QoS flow. | YES | ignore |
| MCG Offered GBR QoS Flow Information | O |  | GBR QoS Flow Information 9.3.1.30 | This IE contains M-Node offered GBR QoS Flow Information. | YES | ignore |
| QoS Monitoring Reporting Frequency | O |  | INTEGER (1..1800, …) | Indicates the Reporting Frequency for RAN part delay for Qos monitoring.Units: second | YES | ignore |
| QoS Monitoring Disabled | O |  | ENUMERATED (true, ...) | Indicates to stop the QoS monitoring. | YES | ignore |
| Data Forwarding Source IP Address | O |  | Transport Layer Address9.3.2.4 | Identifies the TNL address used by the source node for data forwarding. | YES | ignore |
| **PDU Set QoS Parameters** |  | *0..1* |  |  | YES | ignore |
| >UL PDU Set QoS Information | O |  | PDU Set QoS Information9.3.1.143 |  | - |  |
| >DL PDU Set QoS Information | O |  | PDU Set QoS Information9.3.1.143 |  | - |  |
| MMSID | O |  | OCTET STRING (SIZE(1)) | Multi-modal service ID from the application, used to indicate QoS flows are related to a multi-modal service, as specified in TS 23.501 [20] and TS 38.300 [4]. | YES | ignore |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

9.3.1.x Available Data Rate Report Threshold List

This IE contains a list of available data rate report thresholds. It is used for available data rate report for UL and DL as specified in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **Available Data Rate Report Threshold Item** |  | *1..<maxnoofThresholds>* |  |  |
| >Reporting Threshold | M |  | INTEGER (0..4,000,000,000) | This IE indicates the Reporting threshold as specified in TS 23.501 [20]. The unit is Kbps. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofThresholds | Maximum no. of thresholds allowed to be provided by the CN. Value is 8. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

>>>>>>>>>>>>>>>>>>>Unchanged parts are skipped<<<<<<<<<<<<<<<<<<<

MBS-ServiceAreaInformation-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

MBS-ServiceAreaCellList ::= SEQUENCE (SIZE(1.. maxnoofCellsforMBS)) OF NR-CGI

MBS-ServiceAreaTAIList ::= SEQUENCE (SIZE(1.. maxnoofTAIforMBS)) OF MBS-ServiceAreaTAIList-Item

MBS-ServiceAreaTAIList-Item ::= SEQUENCE {

 plmn-ID PLMN-Identity,

 fiveGS-TAC FiveGS-TAC,

 iE-Extensions ProtocolExtensionContainer { {MBS-ServiceAreaTAIList-Item-ExtIEs} } OPTIONAL,

 ...

}

MBS-ServiceAreaTAIList-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

MBS-ServiceAreaInformationList ::= SEQUENCE (SIZE(1..maxnoofMBSServiceAreaInformation)) OF MBS-ServiceAreaInformationItem

MBS-ServiceAreaInformationItem ::= SEQUENCE {

 mBS-AreaSessionID MBSAreaSessionID,

 mBS-ServiceAreaInformation MBS-ServiceAreaInformation,

 iE-Extensions ProtocolExtensionContainer { { MBS-ServiceAreaInformationItem-ExtIEs} } OPTIONAL,

 ...

}

MBS-ServiceAreaInformationItem-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

MonitoringRequestonAvailableDataRate ::= SEQUENCE{

 monitoringRequest MonitoringRequest,

 dlAvailableDataRateReportThresholds AvailableDataRateReportThresholdList OPTIONAL,

-- The above IE shall be present if the Monitoring Request IE is set to the value “dl” or “both”

 ulAvailableDataRateReportThresholds AvailableDataRateReportThresholdList OPTIONAL,

-- The above IE shall be present if the Monitoring Request IE is set to the value “ul” or “both”

 iE-Extensions ProtocolExtensionContainer { { MonitoringRequestonAvailableDataRate-ExtIEs} } OPTIONAL,

 ...

}

MonitoringRequestonAvailableDataRate-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

MonitoringRequest ::= ENUMERATED {ul, dl, both, stop,...}

MMSID ::= OCTET STRING (SIZE (1))

-- N

NetworkInstance ::= INTEGER (1..256, ...)

New-UL-TNL-Information-Required::= ENUMERATED {

 required,

 ...

}

NGRANAllocationAndRetentionPriority ::= SEQUENCE {

 priorityLevel PriorityLevel,

 pre-emptionCapability Pre-emptionCapability,

 pre-emptionVulnerability Pre-emptionVulnerability,

 iE-Extensions ProtocolExtensionContainer { {NGRANAllocationAndRetentionPriority-ExtIEs} } OPTIONAL

}

NGRANAllocationAndRetentionPriority-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

>>>>>>>>>>>>>>>>>>>Unchanged parts are skipped<<<<<<<<<<<<<<<<<<<

ReportCharacteristics ::= BIT STRING (SIZE(36))

ReportingPeriodicity ::= ENUMERATED {

 ms500, ms1000, ms2000, ms5000, ms10000, ms20000, ms30000, ms40000, ms50000, ms60000, ms70000, ms80000, ms90000, ms100000, ms110000, ms120000,

 ...

}

ReportingThreshold ::= INTEGER(0..4000000000)

RequestedAction4AvailNGUTermination ::= ENUMERATED {

 apply-available-configuration,

 apply-requested-configuration,

 ...,

 apply-available-configuration-if-same-as-requested

}

RLC-Mode ::= ENUMERATED {

 rlc-tm,

 rlc-am,

 rlc-um-bidirectional,

 rlc-um-unidirectional-ul,

 rlc-um-unidirectional-dl,

 ...

}

>>>>>>>>>>>>>>>>>>>Unchanged parts are skipped<<<<<<<<<<<<<<<<<<<

9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM E1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-reset ProcedureCode ::= 0

id-errorIndication ProcedureCode ::= 1

id-privateMessage ProcedureCode ::= 2

id-gNB-CU-UP-E1Setup ProcedureCode ::= 3

id-gNB-CU-CP-E1Setup ProcedureCode ::= 4

id-gNB-CU-UP-ConfigurationUpdate ProcedureCode ::= 5

id-gNB-CU-CP-ConfigurationUpdate ProcedureCode ::= 6

id-e1Release ProcedureCode ::= 7

id-bearerContextSetup ProcedureCode ::= 8

id-bearerContextModification ProcedureCode ::= 9

id-bearerContextModificationRequired ProcedureCode ::= 10

id-bearerContextRelease ProcedureCode ::= 11

id-bearerContextReleaseRequest ProcedureCode ::= 12

>>>>>>>>>>>>>>>>>>>Unchanged parts are skipped<<<<<<<<<<<<<<<<<<<

maxnoofSMBRValues INTEGER ::= 8

maxnoofMBSAreaSessionIDs INTEGER ::= 256

maxnoofSharedNG-UTerminations INTEGER ::= 8

maxnoofMRBs INTEGER ::= 32

maxnoofMBSSessionIDs INTEGER ::= 512

maxnoofCellsforMBS INTEGER ::= 512

maxnoofTAIforMBS INTEGER ::= 512

maxnoofMBSServiceAreaInformation INTEGER ::= 256

maxnoofDUs INTEGER ::= 512

maxnoofThresholds INTEGER ::= 8

<<<<<<<<<<<<<<<<<<<< End of Change >>>>>>>>>>>>>>>>>>