**3GPP TSG-RAN WG3 Meeting #128R3-253878**

**Malta, MT, 19th – 23rd May, 2025**

**Agenda Item: 19.2**

**Source: CATT, Ericsson**

**Title: (TP to BL CR for 38.470) introduction of Evolution of NR duplex operation Sub-band full duplex (SBFD)**

**Document for: Other**

1. 1 Introduction

This TP adds the following change:

**Change “CLI MITIGATION UPDATE” to “CLI INDICATION” and remove Editor’s Note.**

1. TP to BL CR for TS 38.423

<<<< Start of change >>>

5.2 F1-C functions

<<<Unchanged part omitted>>>

5.2. x CLI mitigation function

The CLI mitigation function enables the transfer of CLI measurements and CLI mitigation request between gNB-DU and gNB-CU.

<<<Next change>>>

## 6.1 Control plane procedures

<<<Unchanged part omitted>>>

6.1. x CLI mitigation function

The following procedure is used to report the result of CLI measurements and to request CLI mitigation:

- CLI INDICATION

<<<< End of change >>>