**3GPP TSG- Meeting #104-e**

**, - , 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Big CR for TS 38.141-2 Maintenance Demod part (Rel-15, CAT F)  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | This big CR merges endorsed draft CR to 38.141-2 in RAN4#104-e. The reason for change in endorsed draft CR is copied below* R4-2214863

SNR description in Clause 8 General section has mis-leading expression which could leads to higher SNR than defined requirement. For N (noise energy) to calculate SNR, it needs to take noise energy where wanted signal (S) exists. However, current text can be interpret as total noise energy of entire one slot which, in some cases, is longer period than where wanted signal exists especially cases like PRACH as example. This interpretation makes noise energy density lower than defined requirement.* R4-2214551

There is no intra slot frequency hopping configured in PF2 test with ACK miss detection requirements, but the test parameters of intra slot hopping are still existing |
|  |  |
| ***Summary of change:*** | The summary of change in endorsed draft CR is copied as below:* R4-2214863

Description of N is updated to clarify noise energy to calculate SNR is where wanted signal energy exists in time domain as well as frequency domain.* R4-2214551:

Delate all the test parameters and description about intra slot frequency hopping for PF2 test with ACK miss detection requirements |
|  |  |
| ***Consequences if not approved:*** | The consequences if not approved for endorsed draft CR are coppied as below.* R4-2214863

Without this clarification, it’s possible to misinterpret requirement then resulted noise density lower than requirement value (higher SNR).* R4-2214551

The test parameters of PF2 are confusing. |
|  |  |
| ***Clauses affected:*** | 8.1.0, 8.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start Of Change R4-2214863>

### 8.1.0 Scope and definitions

Radiated performance requirements specify the ability of the *BS type 1-O* or *BS type 2-O* to correctly demodulate radiated signals in various conditions and configurations. Radiated performance requirements are specified at the RIB.

Radiated performance requirements for the BS are specified for the fixed reference channels and propagation conditions defined in TS 38.104 [2] annex A and annex J, respectively. The requirements only apply to those FRCs that are supported by the BS.

The radiated performance requirements for *BS type 1-O* and for the *BS type 2-O* are limited to two OTA *demodulations branches* as described in clause 8.1.1. Conformance requirements can only be tested for 1 or 2 *demodulation branches* depending on the number of polarizations supported by the BS, with the required SNR applied separately per polarization.

NOTE 1: BS can support more than 2 *demodulation branches*, however OTA conformance testing can only be performed for 1 or 2 *demodulation branches*.

Unless stated otherwise, radiated performance requirements apply for a single carrier only. Radiated performance requirements for a BS supporting CA are defined in terms of single carrier requirements.

For *BS type 1-O* in FDD operation the requirements in clause 8 shall be met with the transmitter units associated with the RIB in the *operating* *band* turned ON.

NOTE 2: *BS type 1-O* in normal operating conditions in FDD operation is configured to transmit and receive at the same time. The transmitter unit(s) associated with the RIB may be OFF for some of the tests.

In tests performed with signal generators a synchronization signal may be provided between the BS and the signal generator, to enable correct timing of the wanted signal.

The SNR used in this clause is specified based on a single carrier and defined as:

 SNR = S / N

 Where:

S is the total signal energy in a slot on a RIB.

N is the noise energy in a bandwidth corresponding to the transmission bandwidth over the same duration where signal energy exists.

<End of Change R4-2214863>

<Start Of Change R4-2214551>

### Performance requirements for PUCCH format 2

#### 8.3.3.1 ACK missed detection performance requirements

##### 8.3.3.1.1 Definition and applicability

The performance requirement of PUCCH format 2 for ACK missed detection is determined by the two parameters: probability of false detection of the ACK and the probability of detection of ACK on the wanted signal. The performance is measured by the required SNR at probability of detection equal to 0.99. The probability of false detection of the ACK shall be 0.01 or less.

The probability of false detection of the ACK is defined as a probability of erroneous detection of the ACK when input is only noise.

The probability of detection of ACK is defined as probability of detection of the ACK when the signal is present.

Which specific test(s) are applicable to BS is based on the test applicability rules defined in clause 8.1.2.

##### 8.3.3.1.2 Minimum Requirement

For *BS type 1-O*, the minimum requirement is in TS 38.104 [2] clause 11.3.1.4.

For *BS type 2-O*, the minimum requirement is in TS 38.104 [2] clause 11.3.2.4.

##### 8.3.3.1.3 Test Purpose

The test shall verify the receiver's ability to detect ACK bits under multipath fading propagation conditions for a given SNR.

##### 8.3.3.1.4 Method of test

8.3.3.1.4.1 Initial conditions

Test environment: Normal, see clause B.2.

RF channels to be tested for single carrier; M; see clause 4.9.1

Direction to be tested: OTA REFSENS *receiver target reference direction* (see D.54 in table.4.6-1).

8.3.3.1.4.2 Procedure

1) Place the BS with its manufacturer declared coordinate system reference point in the same place as calibrated point in the test system, as shown in annex E.3.

2) Align the manufacturer declared coordinate system orientation of the BS with the test system.

3) Set the BS in the declared direction to be tested.

4) Connect the BS tester generating the wanted signal, multipath fading simulators and AWGN generators to a test antenna via a combining network in OTA test setup, as shown in annex E.3. Each of the demodulation branch signals should be transmitted one polarization of the test antenna(s).

5) The characteristics of the wanted signal shall be configured according to TS 38.211 [20], and according to additional test parameters listed in table 8.3.3.1.4.2-1.

Table 8.3.3.1.4.2-1: Test parameters

|  |  |
| --- | --- |
| Parameter | Value |
| Modulation order | QPSK |
| Starting RB location | 0 |
| Intra-slot frequency hopping | N/A |
|  |  |
| Number of PRBs | 4 |
| Number of symbols | 1 |
| The number of UCI information bits | 4 |
| First symbol | 13 |
| DM-RS sequence generation | *NID*0=0 |

6) The multipath fading emulators shall be configured according to the corresponding channel model defined in annex J.

7) Adjust the test signal mean power so the calibrated radiated SNR value at the BS receiver is as specified in clause 8.3.3.1.5.1 and 8.3.3.1.5.2 for *BS type 1-O* and *BS type 2-O* respectively, and that the SNR at the BS receiver is not impacted by the noise floor.

 The power level for the transmission may be set such that the AWGN level at the RIB is equal to the AWGN level in table 8.3.3.1.4.2-2.

Table 8.3.3.1.4.2-2: AWGN power level at the BS input

|  |  |  |  |
| --- | --- | --- | --- |
| BS type | Sub-carrier spacing(kHz) | Channel bandwidth(MHz) | AWGN power level |
| BS type 1-O (Note 4) | 15 kHz | 5 | -83.5 - ΔOTAREFSENS dBm / 4.5 MHz |
|  |  | 10 | -80.3 - ΔOTAREFSENS dBm / 9.36 MHz |
|  |  | 20 | -77.2 -ΔOTAREFSENS dBm / 19.08 MHz |
|  | 30 kHz | 10 | -80.6 - ΔOTAREFSENS dBm / 8.64 MHz |
|  |  | 20 | -77.4 - ΔOTAREFSENS dBm / 18.36 MHz |
|  |  | 40 | -74.2 - ΔOTAREFSENS dBm / 38.16 MHz |
|  |  | 100 | -70.1 - ΔOTAREFSENS dBm / 98.28 MHz |
| BS type 2-O (Note 5) | 60 kHz | 50 | EISREFSENS\_50M + ΔFR2\_REFSENS + 15 dBm / 47.52MHz |
|  |  | 100 | EISREFSENS\_50M + ΔFR2\_REFSENS + 18 dBm / 95.04 MHz  |
|  | 120 kHz | 50 | EISREFSENS\_50M + ΔFR2\_REFSENS + 15 dBm / 46.08 MHz  |
|  |  | 100 | EISREFSENS\_50M + ΔFR2\_REFSENS + 18 dBm / 95.04 MHz  |
|  |  | 200 | EISREFSENS\_50M + ΔFR2\_REFSENS + 21 dBm / 190.08 MHz  |
| NOTE 1: ΔOTAREFSENS as declared in D.53 in table 4.6-1 and clause 7.1.NOTE 2: ΔFR2\_REFSENS = -3 dB as declared in clause 7.1, since the OTA REFSENS receiver target reference direction (as declared in D.54 in table 4.6-1) is used for testing.NOTE 3: EISREFSENS\_50M as declared in D.28 in table 4.6-1.NOTE 4: The AWGN power level contains an AWGN offset of 16dB by default. If needed for test purposes, the AWGN level can be reduced from the default by any value in the range 0dB to 16dB. Changing the AWGN level does not impact the validity of the test, as it reduces the effective base band SNR level.NOTE 5: The AWGN power level contains an AWGN offset of 15dB by default. If needed for test purposes, the AWGN level can be reduced from the default by any value in the range 0dB to 15dB. Changing the AWGN level does not impact the validity of the test, as it reduces the effective base band SNR level. |

8) The signal generator sends a test pattern with pattern outlined in figure 8.3.3.1.4.2-1. The following statistics are kept: the number of ACK bits detected in the idle periods and the number of missed ACKs.



Figure 8.3.3.1.4.2-1: Test signal pattern for PUCCH format 2 demodulation tests

##### 8.3.3.1.5 Test requirement

8.3.3.1.5.1 Requirements for BS type 1-O

The fraction of falsely detected ACKs shall be less than 1% and the fraction of correctly detected ACKs shall be larger than 99% for the SNR listed in table 8.3.3.1.5.1-1 and table 8.3.3.1.5.1-2.

Table 8.3.3.1.5.1-1: Required SNR for PUCCH format 2 with 15 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of | Number of | Cyclic | Propagation | Channel bandwidth / SNR (dB) |
| TX antennas | demodulation branches | Prefix | conditions and correlation matrix (annex J) | 5 MHz | 10 MHz | 20 MHz |
| 1 | 2 | Normal | TDLC300-100 Low | 6.4 | 6.2 | 6.5 |

Table 8.3.3.1.5.1-2: Required SNR for PUCCH format 2 with 30 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of | Number of | Cyclic | Propagation | Channel bandwidth/ SNR (dB) |
| TX antennas | demodulation branches | Prefix | conditions and correlation matrix (annex J) | 10MHz | 20MHz | 40MHz | 100MHz |
| 1 | 2 | Normal | TDLC300-100 Low | 6.1 | 6.2 | 6.1 | 6.3 |

8.3.3.1.5.2 Requirements for BS type 2-O

The fraction of falsely detected ACKs shall be less than 1% and the fraction of correctly detected ACKs shall be larger than 99% for the SNR listed in table 8.3.3.1.5.2-1 and table 8.3.3.1.5.2.-2

Table 8.3.3.1.5.2-1: Required SNR for PUCCH format 2 with 60 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of | Number of | Cyclic | Propagation | Channel bandwidth / SNR (dB) |
| TX antennas | demodulation branches | Prefix | conditions and correlation matrix (annex J) | 50 MHz | 100 MHz |
| 1 | 2 | Normal | TDLA30-300 Low | 7.3 | 7.8 |

Table 8.3.3.1.5.2-2: Required SNR for PUCCH format 2 with 120 kHz SCS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Number of | Number of | Cyclic | Propagation | Channel bandwidth / SNR (dB) |
| TX antennas | demodulation branches | Prefix | conditions and correlation matrix (annex J) | 50 MHz | 100 MHz | 200 MHz |
| 1 | 2 | Normal | TDLA30-300 Low | 7.2 | 6.9 | 7.2 |

<End of Change R4-2214551>