**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |   |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | S4 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | The conclusion of KI#9 and Ki#14 (traffic detection of multiplexed media flows) from TR 26.822 are as below The following aspects are concluded as principles for normative work:- Based on response from SA2, normative work on multiplexed RTP streams may be needed. Furthermore, it is recommended to add guidelines to TS 26.522 [2] for RTP senders that use multiplexing. There may be potential normative aspects to be added to TS 26.510 [50].When multiple RTP media streams are multiplexed in an RTP session, each media stream can be identified using the identification-tag (the values of "mid" attribute) in the SDP information. The RTP SDES header extension for MID make it possible for a 5G System or an RTP receiver to associate each PDU or PDU Set to a media stream when the the PDUs in a PDU Set carry the RTP SDES header extension for MID. To enable the traffic detection in 5G System, the mediaTransportParameters paremetr in the Application‌Flow‌Description object shall be updated to include the information of the RTP SDES header extension for MID. |
|  |  |
| ***Summary of change:*** | Updated the Dynamic Policy API to include the details of *SDES RTP Compact Header Extension for MID* in protocol description*.*  |
|  |  |
| ***Consequences if not approved:*** | Recommendations from work item description are not met, key 5GA features are not supported |
|  |  |
| ***Clauses affected:*** | 10.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

First change

## 10.3 Dynamic Policy API

The Dynamic Policy API allows the RTC Media Session Handler of the RTC Client or the ICE Function of the RTC AS or the WebRTC Signalling Function of the RTC AS to request a specific QoS and/or charging policy to be applied to the application flows of an RTC session. The Dynamic Policy API is invoked as a result of SDP negotiation during the WebRTC signalling phase of the RTC session.

The relevant procedures are specified in clause 5.3.3 of TS 26.510 [3].

The resource structure and the data model are specified in clause 9.3 of TS 26.510 [3].

If specific QoS with PDU Set parameters is desired, and PDU Set marking is not enabled for the selected Policy Template as specified in clause 5.3.3.2 of TS 26.510 [3], the Media Session Handler shall additionally populate the mediaTransportParameters property of the Application‌Flow‌Description object (see clause 5.5.4.13 of TS 29.571 [36]) as follows when creating or updating a Dynamic Policy Instance based on that Policy Template:

- The transportProto property shall be set to the value SRTP.

- The rtpHeaderExtInfo object (see clause 5.5.4.14 of TS 29.571 [36]) shall be omitted.

- The rtpPayloadInfoList property shall contain a single member populated as follows:

- rtpPayloadTypeList shall be set to the *RTP Payload Type* value(s) to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) for the negotiated SRTP session(s) to be carried by the application flow in question.

- rtpPayloadFormat shall be populated as appropriate in the absence of RTP header extensions.

If PDU Set marking is enabled for the selected Policy Template as specified in clause 5.3.3.2 of TS 26.510 [3], the Media Session Handler shall additionally populate the mediaTransportParameters property of the Application‌Flow‌Description object (see clause 5.5.4.13 of TS 29.571 [36]) as follows when creating or updating a Dynamic Policy Instance based on that Policy Template:

- The transportProto property shall be set to the value SRTP.

- The properties of the rtpHeaderExtInfo object (see clause 5.5.4.14 of TS 29.571 [36]) shall be populated as follows:

- rtpHeaderExtType shall be set to PDU\_SET\_MARKINGorSDES\_INFORMATION.

- rtpHeaderExtId shall be set to the value of the *ID* field to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) in the *RTP Header Extension for PDU Set Marking* or *SDES RTP Compact Header Extension for MID* on the application flow in question, as specified in clause 4.2 or clause 4.6 respectively of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- longFormat shall be set according to the use of the one- or two-byte *RTP Header Extension for PDU Set Marking* or *SDES RTP Compact Header Extension for MID*, as specified in clause 4.2.1 or clause 4.6.2 respectively of TS 26.522 [37]. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

- pduSetSizeActive shall be set to reflect the presence of the *PDU Set Size* field in the *RTP Header Extension for PDU Set Marking*, as specified in clause 4.2.4 of TS 26.522 [37]. This field shall be set to false for *SDES RTP Compact Header Extension for MID*. The value of this parameter is negotiated via the SDP offer/answer procedure during the WebRTC signalling phase of the RTC session.

NOTE: The intention of the RTC Access Function of the RTC Client to include the optional NPDS (Number of PDUs in the PDU Set) field in the *RTP Header Extension for PDU Set Marking* is not yet signalled in advance to the 5G Core by means of a Boolean flag in the RtpHeaderExtInfo specified in clause 5.5.4.14 of TS 29.571 [36].

- The rtpPayloadInfoList property shall contain a single member populated as follows:

- rtpPayloadTypeList shall be set to the *RTP Payload Type* value(s) to be used by the RTC endpoint (e.g., the RTC Access Function of an RTC Client) for the negotiated SRTP session(s) to be carried by the application flow in question.

- rtpPayloadFormat shall be omitted because RTP header extensions are present.

In all PDUs it contributes at reference point RTC‑4m or RTC‑12 that fall within the scope of the application flow description, the RTC Access Function (Media Access Function) shall use the protocol indicated in transportProto; it shall set the SRTP header fields in accordance with rtpPayloadInfoList; and it shall include a one- or two- byte (consistent with the signalled length) *RTP Header Extension for PDU Set Marking* or *SDES RTP Compact Header Extension for MID* in the SRTP header with fields set according to the values declared in the rtpHeaderExtInfo property per above.End of changes