**3GPP TSG-CT Meeting #88eCP-201345-v10**

**E-Meeting, 29th June – 1st July 2020**

Title: LS on human-readable network name (HRNN)

Release: Rel-16

Work Item: Vertical\_LAN

Source: CT

To: SA1

Cc: CT1, CT4, SA2

**Contact Person:**

Name: Ivo Sedlacek

E-mail Address: Ivo dot sedlacek at ericsson dot com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

Attachments: approved revision of CR 23.122 CR#0518, CP-201172

**1. Overall Description:**

CT approved CR 23.122 CR#0518 which contains the following editor's note:

Editor's note: It is FFS whether human-readable network name can be configured for a CAG-ID in a PLMN’s entry in the CAG Information list, to be provided to the upper layer during manual CAG selection. This is subject to SA2 decision.

Furthermore, CT approved the exception sheet for Vertical\_LAN WI (CP-201172) stating the following:

1. *TS 23.122 does not clearly reflect a requirement to obtain a human-readable network name via system information broadcast.* *It remains open whether there is a requirement for a UE to obtain a human-readable network name via other means than the system information broadcast and if so by what other way(s) the UE can obtain a human-readable network name.*

Finally, CT1 noticed that in TS 23.501, subclauses 5.30.2.1, 5.30.2, 5.30.2.4, 5.30.3.2, it is indicated that the HRNN (if broadcasted) is only used for presentation in case of manual NPN selection.

**2. Actions:**

**To** SA1 **group.**

**ACTION:** CT would like to ask SA1:

Question-1) What is the stage-1 requirement for a UE to obtain a human-readable network name other than the system information broadcast for the manual NPN selection?

Question-2) If there is another requirement, what is the precedence between the HRNN obtained via other means and HRNN broadcasted in the system information?

**3. Date of Next CT Meetings:**

3GPP TSG CT September 2020 e-Meeting