**3GPP TSG-CT Meeting #93-eCP-212262**

**E-Meeting, 13th – 15th September 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.301** | **CR** | **3532** | **rev** | **6** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | C2 pairing authorization at bearer resource modification |
|  |  |
| ***Source to WG:*** | Lenovo, Motorola Mobility, Qualcomm Incorporated |
| ***Source to TSG:*** | Lenovo, Motorola Mobility, Qualcomm Incorporated |
|  |  |
| ***Work item code:*** | ID-UAS |  | ***Date:*** | 2021-09-03 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Stage 2 of C2 pairing authorization at the time of bearer resource modification is defined in clause 5.2.5.3.2 of TS 23.256. Stage 3 implementation is currently missing. |
|  |  |
| ***Summary of change:*** | Adding abbreviations.Adding UE requirements for C2 pairing authorization when modifying resource bearer. |
|  |  |
| ***Consequences if not approved:*** | Stage 3 of a feature is not implemented |
|  |  |
| ***Clauses affected:*** | 3.2, 6.4.3.3, 6.5.4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | * Added "with the length of two octets" after C2 aviation container and service-level AA container.
* Editorial change:

From:Upon receipt the MODIFY EPS BEARER CONTEXT REQUEST message with an extended protocol configuration options IE containing the C2 aviation container IE (or service-level AA container IE), the C2 aviation container IE (or service-level AA container IE):To:The MODIFY EPS BEARER CONTEXT REQUEST message can include an extended protocol configuration options IE containing the C2 aviation container with the length of two octets (or service-level AA container with the length of two octets). The C2 aviation container with the length of two octets (or service-level AA container with the length of two octets): |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5G-GUTI 5G-Globally Unique Temporary Identifier

5GMM 5GS Mobility Management

5GS 5G System

ACDC Application specific Congestion control for Data Communication

AKA Authentication and Key Agreement

AMBR Aggregate Maximum Bit Rate

APN Access Point Name

APN-AMBR APN Aggregate Maximum Bit Rate

ARP Allocation Retention Priority

BCM Bearer Control Mode

CIoT Cellular IoT

CP-CIoT Control Plane CIoT

CP-EDT Control Plane EDT

CSG Closed Subscriber Group

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRAN Evolved Universal Terrestrial Radio Access Network

EAB Extended Access Barring

ECM EPS Connection Management

eDRX Extended idle-mode DRX cycle

EDT Early Data Transmission

EENLV Extended Emergency Number List Validity

eKSI Key Set Identifier for E-UTRAN

EMM EPS Mobility Management

eNode B Evolved Node B

EPC Evolved Packet Core Network

EPS Evolved Packet System

ESM EPS Session Management

GBR Guaranteed Bit Rate

GUMMEI Globally Unique MME Identifier

GUTI Globally Unique Temporary Identifier

HeNB Home eNode B

HRPD High Rate Packet Data

IoT Internet of Things

IP-CAN IP-Connectivity Access Network

ISR Idle mode Signalling Reduction

kbps Kilobits per second

KSI Key Set Identifier

L-GW Local PDN Gateway

LHN-ID Local Home Network Identifier

LIPA Local IP Access

M-TMSI M-Temporary Mobile Subscriber Identity

Mbps Megabits per second

MBR Maximum Bit Rate

MME Mobility Management Entity

MMEC MME Code

MT-EDT Mobile Terminated-Early Data Transmission

MUSIM Multi-USIM

NB-IoT Narrowband IoT

NR New Radio

NSSAI Network Slice Selection Assistance Information

PD Protocol Discriminator

PDN GW Packet Data Network Gateway

ProSe Proximity-based Services

PSM Power Saving Mode

PTI Procedure Transaction Identity

QCI QoS Class Identifier

QoS Quality of Service

RACS Radio Capability Signalling Optimisation

RLOS Restricted Local Operator Services

ROHC RObust Header Compression

RRC Radio Resource Control

S-NSSAI Single NSSAI

S-TMSI S-Temporary Mobile Subscriber Identity

S101-AP S101 Application Protocol

S1AP S1 Application Protocol

SAE System Architecture Evolution

SCEF Service Capability Exposure Function

SGC Service Gap Control

SIPTO Selected IP Traffic Offload

TA Tracking Area

TAC Tracking Area Code

TAI Tracking Area Identity

TFT Traffic Flow Template

TI Transaction Identifier

TIN Temporary Identity used in Next update

UAV Uncrewed Aerial Vehicle

URN Uniform Resource Name

USS UAS Service Supplier

V2X Vehicle-to-Everything

WUS Wake-Up Signal

\* \* \* Next Change \* \* \* \*

#### 6.4.3.3 EPS bearer context modification accepted by the UE

Upon receipt of the MODIFY EPS BEARER CONTEXT REQUEST message, if the UE provided an APN for the establishment of the PDN connection, the UE shall stop timer T3396, if it is running for the APN provided by the UE. If the UE did not provide an APN for the establishment of the PDN connection and the request type was different from "emergency" and from "handover of emergency bearer services", the UE shall stop the timer T3396 associated with no APN if it is running. If the MODIFY EPS BEARER CONTEXT REQUEST message was received for an emergency PDN connection, the UE shall not stop the timer T3396 associated with no APN if it is running. For any case, the UE shall then check the received TFT before taking it into use and send a MODIFY EPS BEARER CONTEXT ACCEPT message to the MME.

If the MODIFY EPS BEARER CONTEXT REQUEST message contains a PTI value other than "no procedure transaction identity assigned" and "reserved" (see 3GPP TS 24.007 [12]), the UE uses the PTI to identify the UE requested bearer resource allocation procedure or the UE requested bearer resource modification procedure to which the EPS bearer context modification is related (see clause 6.5.3 and clause 6.5.4).

If the MODIFY EPS BEARER CONTEXT REQUEST message contains a PTI value other than "no procedure transaction identity assigned" and "reserved" (see 3GPP TS 24.007 [12]) and the PTI is associated to a UE requested bearer resource allocation procedure or a UE requested bearer resource modification procedure, the UE shall release the traffic flow aggregate description associated to the PTI value provided.

If the EPS bearer context that is modified is a GBR bearer and the MODIFY EPS BEARER CONTEXT REQUEST message does not contain the Guaranteed Bit Rate (GBR) and the Maximum Bit Rate (MBR) values for uplink and downlink, the UE shall continue to use the previously received values for the Guaranteed Bit Rate (GBR) and the Maximum Bit Rate (MBR) for the corresponding bearer.

The UE shall use the received TFT to apply mapping of uplink traffic flows to the radio bearer if the TFT contains packet filters for the uplink direction.

If a WLAN offload indication information element is included in the MODIFY EPS BEARER CONTEXT REQUEST message, the UE shall store the WLAN offload acceptability values for this PDN connection and use the E-UTRAN offload acceptability value to determine whether this PDN connection is offloadable to WLAN or not.

If the UE receives an APN rate control parameters container in the protocol configuration options IE or extended protocol configuration options IE in the MODIFY EPS BEARER CONTEXT REQUEST message, the UE shall store the APN rate control parameters value and use the stored APN rate control parameters value as the maximum allowed limit of uplink user data related to the corresponding APN in accordance with 3GPP TS 23.401 [10]. If the UE has a previously stored APN rate control parameters value for this APN, the UE shall replace the stored APN rate control parameters value for this APN with the received APN rate control parameters value.

If the UE receives an additional APN rate control parameters for exception data container in the protocol configuration options IE or extended protocol configuration options IE in the MODIFY EPS BEARER CONTEXT REQUEST message, the UE shall store the additional APN rate control parameters for exception data value and use the stored additional APN rate control parameters for exception data value as the maximum allowed limit of uplink exception data related to the corresponding APN in accordance with 3GPP TS 23.401 [10]. If the UE has a previously stored additional APN rate control parameters for exception data value for this APN, the UE shall replace the stored additional APN rate control parameters for exception data value for this APN with the received additional APN rate control parameters for exception data value.

If the UE receives a small data rate control parameters container in the protocol configuration options IE or the extended protocol configuration options IE in the MODIFY EPS BEARER CONTEXT REQUEST message, the UE shall store the small data rate control parameters value and use the stored small data rate control parameters value as the maximum allowed limit of uplink user data for the corresponding PDU session that becomes transferred after inter-system change from S1 mode to N1 mode in accordance with 3GPP TS 23.501 [58]. If the UE has a previously stored small data rate control parameters value for this PDU session, the UE shall replace the stored small data rate control parameters value for this PDU Session with the received small data rate control parameters value.

If the UE receives an additional small data rate control parameters for exception data container in the protocol configuration options IE or the extended protocol configuration options IE in the MODIFY EPS BEARER CONTEXT REQUEST message, the UE shall store the additional small data rate control parameters for exception data value and use the stored additional small data rate control parameters for exception data value as the maximum allowed limit of uplink exception data for the corresponding PDU session that becomes transferred after inter-system change from S1 mode to N1 mode in accordance with 3GPP TS 23.501 [58]. If the UE has a previously stored additional small data rate control parameters for exception data value for this PDU session, the UE shall replace the stored additional small data rate control parameters for exception data value for this PDU session with the received additional small data rate control parameters for exception data value.

Upon receipt of the MODIFY EPS BEARER CONTEXT REQUEST message with a session-AMBR and QoS rule(s) in the protocol configuration options IE or the extended protocol configuration options IE, the UE stores the session-AMBR and QoS rule(s) for use during inter-system change from S1 mode to N1 mode.

The MODIFY EPS BEARER CONTEXT REQUEST message can include an extended protocol configuration options IE containing the C2 aviation container with the length of two octets (or service-level AA container with the length of two octets). The C2 aviation container with the length of two octets (or service-level AA container with the length of two octets):

- contains C2 authorization result;

- can contain C2 session security information;

- can contain a new CAA-level UAV ID; and

- can contain the flight authorization information.

If the C2 aviation container with the length of two octets (or service-level AA container with the length of two octets) contains a CAA-level UAV ID, the UE supporting UAS services, shall replace its currently stored CAA-level UAV ID with the new CAA-level UAV ID.

Editor's note: Whether the new C2 aviation container with the length of two octets is adopted for C2 authorization or the service-level AA container with the length of two octets is re-used, is FFS.

Upon receipt of the MODIFY EPS BEARER CONTEXT ACCEPT message, the MME shall stop the timer T3486 and enter the state BEARER CONTEXT ACTIVE.

\* \* \* Next Change \* \* \* \*

#### 6.5.4.2 UE requested bearer resource modification procedure initiation

In order to request the modification of bearer resources for one traffic flow aggregate, the UE shall send a BEARER RESOURCE MODIFICATION REQUEST message to the MME, start timer T3481 and enter the state PROCEDURE TRANSACTION PENDING (see example in figure 6.5.4.2.1).

The UE shall include the EPS bearer identity of the EPS bearer associated with the traffic flow aggregate in the EPS bearer identity for packet filter IE.

To request a change of the GBR without changing the packet filter(s), the UE shall set the TFT operation code in the Traffic flow aggregate IE to "no TFT operation" and include the packet filter identifier(s) to which the change of the GBR applies in the Packet filter identifier parameter in the parameters list. The UE shall indicate the new GBR requested for the EPS bearer context in the Required traffic flow QoS IE.

To request a modification of a traffic flow aggregate, the UE shall set the TFT operation code in the Traffic flow aggregate IE to "Replace packet filters in existing TFT" or "Add packet filters to existing TFT". If the TFT operation code is set to "Add packet filters to existing TFT", the UE shall include in the parameter list one existing packet filter identifier to which the newly added packet filter(s) is linked. If the EPS bearer is a GBR bearer and the UE also wishes to request a change of GBR, the UE shall indicate the new GBR requested for the EPS bearer context in the Required traffic flow QoS IE.

To request a release of bearer resources, the UE shall set the TFT operation code in the Traffic flow aggregate IE to "Delete packet filters from existing TFT". If the EPS bearer is a GBR bearer and the UE does not request the release of all bearer resources, the UE shall indicate the new GBR requested for the EPS bearer context in the Required traffic flow QoS IE.

To request re-negotiation of header compression configuration associated to an EPS bearer context, the UE shall include the Header compression configuration IE in the BEARER RESOURCE MODIFICATION REQUEST message if the network indicated "Control plane CIoT EPS optimization supported" and "Header compression for control plane CIoT EPS optimization supported" in the EPS network feature support IE.

After an inter-system change from N1 mode to S1 mode, if:

a) the UE is operating in single-registration mode and has received the interworking without N26 interface indicator set to "interworking without N26 interface not supported" from the network;

b) the PDN type value of the PDN type IE is set to "IPv4", "IPv6" or "IPv4v6";

c) the UE indicates "Control plane CIoT EPS optimization supported" and "Header compression for control plane CIoT EPS optimization supported" in the UE network capability IE of the TRACKING AREA UPDATE REQUEST message; and

d) the network indicates "Control plane CIoT EPS optimization supported" and "Header compression for control plane CIoT EPS optimization supported" in the EPS network feature support IE of the TRACKING AREA UPDATE ACCEPT message;

the UE shall send a BEARER RESOURCE MODIFICATION REQUEST message to the MME and include the Header compression configuration IE to negotiate the header compression configuration.

To indicate a change of 3GPP PS data off UE status associated to a PDN connection, the UE shall include the protocol configuration options IE in the BEARER RESOURCE MODIFICATION REQUEST message and set the 3GPP PS data off UE status only if:

- the network included the 3GPP PS data off support indication in the protocol configuration options IE in the ACTIVATE DEFAULT EPS BEARER CONTEXT REQUEST message when the PDN connection was established; or

- the PDU session was established when in N1 mode.

The UE behaves as described in clause 6.3.10.

If the UE requests the modification of a traffic flow aggregate, which is assigned to a dedicated EPS bearer context, it shall ensure that at least one packet filter applicable for the uplink direction remains among the packet filters created on request from the UE in that TFT, or no own packet filters.

NOTE: If the UE requests the release of all bearer resources of a GBR bearer and includes a Required traffic flow QoS IE in the BEARER RESOURCE MODIFICATION REQUEST message, the network ignores the Required traffic flow QoS IE.

If the UE includes the Required traffic flow QoS IE, the UE shall set the QCI to the current QCI value of the EPS bearer context.

If the UE requests the release of bearer resources, the ESM cause value typically indicates one of the following:

#36: regular deactivation.

To perform C2 authorization of UAV operation for the C2 communication when a PDN connection is already established for the USS communication, the UE shall include the extended protocol configuration options IE in the BEARER RESOURCE MODIFICATION REQUEST message containing the C2 aviation container with the length of two octets (or service-level AA container with the length of two octets). In the C2 aviation container with the length of two octets (or service-level AA container with the length of two octets), the UE:

- shall include CAA-level UAV ID of the UE;

- if available, shall include the identification information of UAV-C to pair; and

- may include the flight authorization information.

NOTE: The CAA-Level UAV ID, pairing information and flight authorization information are coded as described in 3GPP TS 24.501 [54].

Editor's note: Whether the new C2 aviation container with the length of two octets is adopted for C2 authorization or the service-level AA container with the length of two octets is re-used, is FFS.

Editor's note: Whether the identification information of UAV-C to pair is mandatory or optional if it is available is FFS.



Figure 6.5.4.2.1: UE requested bearer resource modification procedure

For the NBIFOM procedures as defined in 3GPP TS 24.161 [36], the UE may send a BEARER RESOURCE MODIFICATION REQUEST message to the MME.

It is possible that the traffic flow aggregate IE is not needed in the following procedures:

- re-negotiation of header compression configuration associated to an EPS bearer context;

- indicating a change of 3GPP PS data off UE status associated to a PDN connection; or

- NBIFOM procedures.

If the traffic flow aggregate IE is not needed, the UE shall set:

- the length indicator of the Traffic flow aggregate IE to the value 1;

- the TFT operation code to "000";

- the E bit to zero; and

- the number of packet filters to zero.

\* \* \* End of Changes \* \* \* \*