**3GPP TSG-CT WG1 Meeting #125-eC1-205089**

**Electronic meeting, 20-28 August 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.587** | **CR** | **0114** | **rev** | **-** | **Current version:** | **16.1.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Encoding for direct link establishment reject message |
|  |  |
| ***Source to WG:*** | Samsung, CATT |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | eV2XARC |  | ***Date:*** | 2020-08-12 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)* |
|  |  |
| ***Reason for change:*** | As per clause 6.1.2.2.5 (PC5 unicast link establishment procedure not accepted by the target UE), If the DIRECT LINK ESTABLISHMENT REQUEST message cannot be accepted, the target UE shall send a DIRECT LINK ESTABLISHMENT REJECT message.The encoding for DIRECT LINK ESTABLISHMENT REJECT message is missing. |
|  |  |
| ***Summary of change:*** | Add the encoding of DIRECT LINK ESTABLISHMENT REJECT message. |
|  |  |
| ***Consequences if not approved:*** | No encoding of DIRECT LINK ESTABLISHMENT REJECT message. |
|  |  |
| ***Clauses affected:*** | 7.3.x(new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* Next change \*\*\*\*\*

### 7.3.x Direct link establishment reject

#### 7.3.x.1 Message definition

This message is sent by the UE to another peer UE to indicate that the link establishment request is not accepted. See table 7.3.x.1.1.

Message type: DIRECT LINK ESTABLISHMENT REJECT

Significance: dual

Direction: UE to peer UE

Table 7.3.x.1.1: DIRECT LINK ESTABLISHMENT REJECT message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | DIRECT LINK ESTABLISHMENT REJECT message identity | PC5 signalling message type8.4.1 | M | V | 1 |
|  | Sequence number | Sequence number8.4.2 | M | V | 1 |
|  | PC5 signalling protocol cause | PC5 signalling protocol cause8.4.9 | M | V | 1 |

\*\*\*\*\* Next change \*\*\*\*\*