**3GPP TSG-CT WG1 Meeting #125-e C1-20xxxx**

**Electronic meeting, 20-28 August 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.501** | **CR** | **xxxx** | **rev** | **x** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | | |
| ***Title:*** | The requirements of Rejected NSSAI for unknown cause value | | | | | | | | | | |
|  |  | | | | | | | | | | |
| ***Source to WG:*** | China Mobile,ZTE, Huawei, HiSilicon | | | | | | | | | | |
|  |  | | | | | | | | | | |
| ***Work item code:*** | 5GProtoc16 | | | | | |  | ***Date:*** | | | 2020-08-06 |
|  |  | | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | | |
| ***Reason for change:*** | | | The Rejected NSSAI IE contains multiple rejected S-NSSAIs, and each rejected S-NSSAI consists of one S-NSSAI and an associated cause value.  Considering that:   1. An early version UE may not know a cause value defined in late version. 2. The cause value indicates the associated S-NSSAI belonging to VPLMN or HPLMN. 3. It’s not proper for UE to store a rejected S-NSSAI with an unknown cause, although the S-NSSAI is rejected by the network for some reason. 4. Each rejected S-NSSAI can be decoded independently. 5. It’s not proper for UE to ignore a whole Rejected NSSAI IE due to a reserved cause value within in one of the rejected S-NSSAIs, since other rejected S-NSSAIs can be decoded normally.   It is suggested that the UE shall not ignore the whole IE but skip the Rejected S-NSSAI with the reserved value. That is, UE can keep other rejected S-NSSAIs with a known cause value. | | | | | | | | |
|  | | |  | | | | | | | | |
| ***Summary of change:*** | | | Specify that UE ignores the rejected S-NSSAI with an unknown cause value, and keeps other rejected S-NSSAIs in the Rejected NSSAI IE. | | | | | | | | |
|  | | |  | | | | | | | | |
| ***Consequences if not approved:*** | | | 1. UE may store a rejected S-NSSAI without knowing it belongs to VPLMN or HPLMN. 2. UE may ignore a whole Rejected NSSAI IE due to an unknown cause value, which could impact other rejected S-NSSAIs decoded normally. | | | | | | | | |
|  | | |  | | | | | | | | |
| ***Clauses affected:*** | | | 9.11.3.46 | | | | | | | | |
|  | | |  | | | | | | | | |
|  | | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | | |  | | | | | | | | |
| ***Other comments:*** | | |  | | | | | | | | |
|  | | |  | | | | | | | | |
| ***This CR's revision history:*** | | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* NEXT CHANGE \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### 9.11.3.46 Rejected NSSAI

The purpose of the Rejected NSSAI information element is to identify a collection of rejected S-NSSAIs.

The Rejected NSSAI information element is coded as shown in figure 9.11.3.46.1, figure 9.11.3.46.2 and table 9.11.3.46.1.

The Rejected NSSAI is a type 4 information element with a minimum length of 4 octets and a maximum length of 42 octets.

NOTE: The number of rejected S-NSSAI(s) cannot exceed eight.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Rejected NSSAI IEI | | | | | | | | octet 1 |
| Length of Rejected NSSAI contents | | | | | | | | octet 2 |
| Rejected S-NSSAI 1 | | | | | | | | octet 3  octet m |
| Rejected S-NSSAI 2 | | | | | | | | octet m+1\*  octet n\* |
| … | | | | | | | | octet n+1\*  octet u\* |
| Rejected S-NSSAI n | | | | | | | | octet u+1\*  octet v\* |

Figure 9.11.3.46.1: Rejected NSSAI information element

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Length of rejected S-NSSAI | | | | Cause value | | | | octet 1 |
| SST | | | | | | | | octet 2 |
| SD | | | | | | | | octet 3\*  octet 5\* |

Figure 9.11.3.46.2: Rejected S-NSSAI

Table 9.11.3.46.1: Rejected NSSAI information element

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Value part of the Rejected NSSAI information element (octet 3 to v) | | | | | |
|  | | | | | |
| The value part of the Rejected NSSAI information element consists of one or more rejected S-NSSAIs. Each rejected S-NSSAI consists of one S-NSSAI and an associated cause value. The length of each rejected S-NSSAI can be determined by the 'length of rejected S-NSSAI' field in the first octet of the rejected S-NSSAI. | | | | | |
| The UE shall store the complete list received. If more than 8 rejected S-NSSAIs are included in this information element, the UE shall store the first 8 rejected S-NSSAIs and ignore the remaining octets of the information element. | | | | | |
|  | | | | | |
| Rejected S-NSSAI: | | | | | |
|  | | | | | |
| Cause value (octet 1) | | | | | |
| Bits | | | | | |
| 4 | 3 | 2 | 1 |  |  |
| 0 | 0 | 0 | 0 |  | S-NSSAI not available in the current PLMN or SNPN |
| 0 | 0 | 0 | 1 |  | S-NSSAI not available in the current registration area |
| 0 | 0 | 1 | 0 |  | S-NSSAI not available due to the failed or revoked network slice-specific authentication and authorization. |
| All other values are reserved. The UE shall ignore the rejected S-NSSAI associated with a reserved cause value. | | | | | |
|  | | | | | |
| Slice/service type (SST) (octet 2) | | | | | |
| This field contains the 8 bit SST value. The coding of the SST value part is defined in 3GPP TS 23.003 [4]. (NOTE 2) | | | | | |
|  | | | | | |
| Slice differentiator (SD) (octet 3 to octet 5) | | | | | |
| This field contains the 24 bit SD value. The coding of the SD value part is defined in 3GPP TS 23.003 [4]. (NOTE 3) | | | | | |
| NOTE 1: If octet 3 is included, then octet 4 and octet 5 shall be included.  NOTE 2: If the Cause value is “S-NSSAI not available due to the failed or revoked network slice-specific authentication and authorization”, this field shall contain the 8 bit SST value of an S-NSSAI in the S-NSSAI(s) of the HPLMN.  NOTE 3: If the Cause value is “S-NSSAI not available due to the failed or revoked network slice-specific authentication and authorization”, this field shall contain the 24 bit SD value of an S-NSSAI in the S-NSSAI(s) of the HPLMN. | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* END of CHANGE \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*