**3GPP TSG-CT WG1 Meeting #126-eC1-20xxxx**

**Electronic meeting, 15-23 October 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.501** | **CR** | **2733** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | PDU SESSION RELEASE COMPLETE message not forwarded due to routing failure |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | 5GProtoc17 |  | ***Date:*** | 2020-10-21 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)* |
|  |  |
| ***Reason for change:*** | If a PDU SESSION RELEASE COMMAND message is not forwarded due to routing failure, the UE will receive an indication that the 5GSM message was not forwarded due to routing failure along with a PDU SESSION RELEASE COMPLETE message with the PDU session ID IE set to the same value as the PDU session ID that was sent by the UE.However, currently the TS is missing how the UE operates in this case. |
|  |  |
| ***Summary of change:*** | UE operation is clarified for the case where a UE receives an indication that the 5GSM message was not forwarded due to routing failure along with a PDU SESSION RELEASE COMPLETE message with the PDU session ID IE set to the same value as the PDU session ID that was sent by the UE. |
|  |  |
| ***Consequences if not approved:*** | How the UE behaves in case a routing failure occurs for a PDU SESSION RELEASE COMMAND message. |
|  |  |
| ***Clauses affected:*** | 6.3.3.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 6.3.3.6 Abnormal cases in the UE

The following abnormal cases can be identified:

a) PDU session inactive for the received PDU session ID.

 If the PDU session ID in the PDU SESSION RELEASE COMMAND message belongs to any PDU session in state PDU SESSION INACTIVE in the UE, the UE shall include the 5GSM cause #43 "Invalid PDU session identity" in the 5GSM STATUS message, and set the PDU session ID to the received PDU session ID in the UL NAS TRANSPORT message as specified in subclause 5.4.5.

b) User-plane resources of the MA PDU session on the access indicated in the Access type IE not established.

 If the PDU session is an MA PDU session and has user-plane resources established on a single access different from the access indicated in the Access type IE, the UE shall not diagnose an error, further process the release command and consider the user-plane resources of the MA PDU session on the access indicated in the Access type IE as successfully released.

c) Upon receiving an indication that the 5GSM message was not forwarded due to routing failure along with a PDU SESSION RELEASE COMPLETE message with the PDU session ID IE set to the same value as the PDU session ID that was sent by the UE, the UE shall neither diagnose an error nor further process the release command and shall consider the PDU session as released.