**3GPP TSG-CT WG1 Meeting #129-eC1-21xxxx**

**Electronic meeting, 19-23 April 2021 was C1-212352**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.486** | **CR** | **0078** | **rev** | **-** | **Current version:** | **16.3.0**  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | VAE server initiated on network dynamic group information update procedure |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | eV2XAPP |  | ***Date:*** | 2021-04-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The specification needs to define the stage 3 details of the VAE server initiated on network dynamic group information update procedure defined in 3GPP TS 23.286 clause 9.12.6.3. |
|  |  |
| ***Summary of change:*** | 1. Add the VAE server initiated on network dynamic group information update procedure. |
|  |  |
| ***Consequences if not approved:*** | The VAE server initiated on network dynamic group information update procedure is missing |
|  |  |
| ***Clauses affected:*** | 6.8.XX(New) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

## 6.8.XX VAE server initiated on network dynamic group information update procedure

#### 6.8.XX.1 Client procedure

Upon receiving an HTTP POST request message containing:

a) a Content-Type header field set to "application/vnd.3gpp.vae-info +xml"; and

b) an application/vnd.3gpp.vae-info+xml MIME body with an <dynamic-group-info-update-indication> element in the <VAE-info> root element;

the VAE-C:

a) shall notify the V2X application specific client about the possible update to group information.

#### 6.8.XX.2 Server procedure

In oder to update dynamic group information of an on-network V2X dynamic group, if the update in group information requires consent from the group member(s), the VAE-S shall obtain the consent from the user as specified in clause 6.8.XXX and shall generate an HTTP POST request according to procedures specified in IETF RFC 2616 [19]. In the HTTP POST request, the VAE-S:

a) shall include a Request-URI set to the URI corresponding to the identity of the VAE-C;

b) shall include a Content-Type header field set to "application/vnd.3gpp.vae-info +xml";

c) shall include an application/vnd.3gpp.vae-info+xml MIME body with a <dynamic-group-info-update-indication> element in the <VAE-info> root element which shall include:

1) a <dynamic-group-info> element which shall include:

i) a <dynamic-group-id> element set to the identity of the dynamic group;

ii) a <group-definition> element set to information about the V2X group; and

iii) a <group-leader-id> element set to the identity of the new group leader;

d) shall send the HTTP POST request message towards the VAE-C according to IETF RFC 2616 [19]; and

e) shall update the group document as specified in clause 6.2.5.1 of TS 24.544 [9].

\* \* \* End of Change \* \* \* \*