**3GPP TSG-CT WG1 Meeting #129-eC1-21xxxx was C1-212163**

**Electronic meeting, 19-23 April 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.301** | **CR** |  **3508** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Multi-USIM introduction in EPS |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, InterDigital |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | MUSIM |  | ***Date:*** | 2021-04-06 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | SA2 has started to introduce the Multi-USIM (MUSIM) requirements in stage-2 specifications such as in S2-2102042. Hence in stage-3 specs, it is required to start reflecting that and indicate to the network if the UE supports MUSIM, as per stage-2 requirements. |
|  |  |
| ***Summary of change:*** | Adding an introductory section about MUSIM. |
|  |  |
| ***Consequences if not approved:*** | Unclarity in stage-3 about the meaning of MUSIM and its support stay in the spec. |
|  |  |
| ***Clauses affected:*** | 4.x (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* First change \*\*\*\*\*

## 4.x Support of Multi-USIM (MUSIM) capability

The UE may support MUSIM capability. The UE supporting MUSIM capability shall support one or more of the features related to MUSIM that are described in this specification.

The network may support one or more of the features related to MUSIM that are described in this specification.

Editor’s note: What is meant by "supporting MUSIM capability" and similar statements is for FFS.

\*\*\*\*\* End of changes \*\*\*\*\*