**3GPP TSG-CT WG1 Meeting #130-eC1-21xxxx**

**Electronic meeting, 20-28 May 2021 Revision of C1-213088**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.501** | **CR** |  | **rev** | **3** | **Current version:** | **17.2.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | MCC list for 5GMM message |
|  |  |
| ***Source to WG:*** | China Mobile, Nokia, Nokia Shanghai Bell, OPPO |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | 5GSAT\_ARCH-CT |  | ***Date:*** | 2021-05-09 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | SA2 clarifies in the TS 23.502 CR#2482 (S2-2101667) that indicated MCC(s) are intended to inform the UE of the country or international area in which the UE is determined to be currently located by the network. And informing the UE of the country or international area by the AMF is specified in Registration procedure, Network-initiated Deregistration procedure and Service Request procedure in the TS 23.502 after SA2#143e meeting.Therefore, it is suggested to define the MCC list in TS 24.501 to be aligned with stage 2. |
|  |  |
| ***Summary of change:*** | To define the MCC list in TS 24.501 to be aligned to stage 2. |
|  |  |
| ***Consequences if not approved:*** | Informing the UE of the country or international area by the AMF will not be supported in stage 3. |
|  |  |
| ***Clauses affected:*** | 8.2.9.1, 8.2.9.x(new), 8.2.14.1, 8.2.14.x(new), 8.2.18.1, 8.2.18.x(new), 9.11.3.xx(new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | 1. Correct the refered Tdoc number of TS 23.502 CR#2482 in the “Reason for change” part on the cover sheet.
2. Remove the “international area” in the text to be aligned to TS 23.502.and add ENs for the consideration of “international area”.
 |

\*\*\* First change \*\*\*

#### 8.2.9.1 Message definition

The REGISTRATION REJECT message is sent by the AMF to the UE. See table 8.2.9.1.1.

Message type: REGISTRATION REJECT

Significance: dual

Direction: network to UE

Table 8.2.9.1.1: REGISTRATION REJECT message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | Extended protocol discriminator | Extended protocol discriminator9.2 | M | V | 1 |
|  | Security header type | Security header type9.3 | M | V | 1/2 |
|  | Spare half octet | Spare half octet9.5 | M | V | 1/2 |
|  | Registration reject message identity | Message type9.7 | M | V | 1 |
|  | 5GMM cause | 5GMM cause9.11.3.2 | M | V | 1 |
| 5F | T3346 value | GPRS timer 29.11.2.4 | O | TLV | 3 |
| 16 | T3502 value | GPRS timer 29.11.2.4 | O | TLV | 3 |
| 78 | EAP message | EAP message9.11.2.2 | O | TLV-E | 7-1503 |
| 69 | Rejected NSSAI | Rejected NSSAI9.11.3.46 | O | TLV | 4-42 |
| 75 | CAG information list | CAG information list9.11.3.18A | O | TLV-E | 3-n |
| 68 | Extended rejected NSSAI | Extended rejected NSSAI9.11.3.75 | O | TLV | 4-74 |
| xx | MCC list | MCC list9.11.3.xx | O | TLV | 4-TBD |

\*\*\* Next change \*\*\*

#### 8.2.9.x MCC list

The AMF may include this IE to inform the UE of the country where the UE is located.

Editor's note: Whether and how the AMF uses the MCC list to indicate to the UE it is located in international area are FFS.

\*\*\* Next change \*\*\*

#### 8.2.14.1 Message definition

The DEREGISTRATION REQUEST message is sent by the AMF to the UE. See table 8.2.14.1.1.

Message type: DEREGISTRATION REQUEST

Significance: dual

Direction: network to UE

Table 8.2.14.1.1: DEREGISTRATION REQUEST message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | Extended protocol discriminator | Extended protocol discriminator9.2 | M | V | 1 |
|  | Security header type | Security header type9.3 | M | V | 1/2 |
|  | Spare half octet | Spare half octet9.5 | M | V | 1/2 |
|  | De-registration request message identity | Message type9.7 | M | V | 1 |
|  | De-registration type | De-registration type9.11.3.20 | M | V | 1/2 |
|  | Spare half octet | Spare half octet9.5 | M | V | 1/2 |
| 58 | 5GMM cause | 5GMM cause9.11.3.2 | O | TV | 2 |
| 5F | T3346 value | GPRS timer 29.11.2.4 | O | TLV | 3 |
| 6D | Rejected NSSAI | Rejected NSSAI9.11.3.46 | O | TLV | 4-42 |
| 75 | CAG information list | CAG information list9.11.3.18A | O | TLV-E | 3-n |
| 68 | Extended rejected NSSAI | Extended rejected NSSAI9.11.3.75 | O | TLV | 4-74 |
| xx | MCC list | MCC list9.11.3.xx | O | TLV | 4-TBD |

\*\*\* Next change \*\*\*

#### 8.2.14.x MCC list

The AMF may include this IE to inform the UE of the country where the UE is located.

Editor's note: Whether and how the AMF uses the MCC list to indicate to the UE it is located in international area are FFS.

\*\*\* Next change \*\*\*

#### 8.2.18.1 Message definition

The SERVICE REJECT message is sent by the AMF to the UE in order to reject the service request procedure. See table 8.2.18.1.1.

Message type: SERVICE REJECT

Significance: dual

Direction: network to UE

Table 8.2.18.1.1: SERVICE REJECT message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | Extended protocol discriminator | Extended protocol discriminator9.2 | M | V | 1 |
|  | Security header type | Security header type9.3 | M | V | 1/2 |
|  | Spare half octet | Spare half octet9.5 | M | V | 1/2 |
|  | Service reject message identity | Message type9.7 | M | V | 1 |
|  | 5GMM cause | 5GMM cause9.11.3.2 | M | V | 1 |
| 50 | PDU session status | PDU session status9.11.3.44 | O | TLV | 4-34 |
| 5F | T3346 value | GPRS timer 29.11.2.4 | O | TLV | 3 |
| 78 | EAP message | EAP message9.11.2.2 | O | TLV-E | 7-1503 |
| 6B | T3448 value | GPRS timer 29.11.2.4 | O | TLV | 3 |
| 75 | CAG information list | CAG information list9.11.3.18A | O | TLV-E | 3-n |
| xx | MCC list | MCC list9.11.3.xx | O | TLV | 4-TBD |

\*\*\* Next change \*\*\*

#### 8.2.18.x MCC list

The AMF may include this IE to inform the UE of the country where the UE is located.

Editor's note: Whether and how the AMF uses the MCC list to indicate to the UE it is located in international area are FFS.

\*\*\* Next change \*\*\*

#### 9.11.3.xx MCC list

The purpose of the MCC list information element is to inform the UE of the country where the UE is located.

Editor's note: Whether and how the AMF uses the MCC list to indicate to the UE it is located in international area are FFS.

The MCC list information element is coded as shown in figures 9.11.3.x.1 and 9.11.3.x.2 and table 9.11.3.x.1.

The MCC list is a type 4 information element, with a minimum length of 4 octets.

Editor's note: The maximum number of MCCs which can be included in the IE is FFS.

Editor's note: Whether there should be only a single MCC in the IE is FFS. If there are more than one MCC in the IE, the abnormal cases when all MCCs do not correspond to the same country are needed.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| MCC list IEI | octet 1 |
| Length of MCC list contents | octet 2 |
| MCC 1 | octet 3octet 4 |
| MCC 2 | octet 5\*octet 6\* |
| … | octet 7\*octet 2n\* |
| MCC n | octet 2n+1\*octet 2n+2\* |

Figure 9.11.3.x.1: MCC list information element

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| MCC digit 2 | MCC digit 1 | octet 2n+1 |
| MCC Indication | 0Spare | 0Spare | 0Spare | MCC digit 3 | octet 2n+2 |

Figure 9.11.3.x.2: MCC n

Table 9.11.3.x.1: MCC list information element

|  |
| --- |
| MCC, Mobile country code (octet 2n+1 and bits 1 to 4 in octet 2n+2)The field is coded as in ITU-T Recommendation E.212 [42], annex A. |
|  |
| MCC indication(bit 8 of octet 2n+2) |
| Bit |
| **8** |  |
| 0 | MCC of a country |
| 1 | spare |
|  |

Editor's note: How international area is indicated and whether MCC field could be not applicable when it is indicated are FFS.

\*\*\* End of changes \*\*\*