**3GPP TSG-CT WG1 Meeting #130-eC1-21XXXX**

**Electronic meeting, 20-28 May 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.913** | **CR** | **0048** | **rev** | **1** | **Current version:** | **17.0.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Measurement performance per QoS flow |
|  |  |
| ***Source to WG:*** | Lenovo, Motorola Mobility |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | ATSSS\_Ph2 |  | ***Date:*** | 2021-05-13 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Stage 2 has recently defined access performance measurements based on target QoS flow used by the service data flow (SDF) traffic, if the UE is capable of it. This is an addition to what which has been used i.e. default QoS flow. |
|  |  |
| ***Summary of change:*** | Added requirements to describe the behavior of the UE and the UPF about when to perform the access performance measurements based on target QoS flow or default QoS flow.Added a new indicator for the measurement assistance information that the UE performs the measurements based on target QoS flow.Added SMF providing the UE by the MAI, a QoS flow list for the access performance measurements per target QoS flow. In this implementation, already existing authorized QoS flow descriptions as described in TS24.501 has been employed as the QoS flow list. Corrected a reference (outside the scope of the intention for this CR). |
|  |  |
| ***Consequences if not approved:*** | Stage 3 has not been implemented for the new feature based on target QoS flow. |
|  |  |
| ***Clauses affected:*** | 4.4,6.1.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 23.501 ... CR #2720  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---------------------------------- NEXT CHANGE -----------------------------------

## 4.4 Support of access performance measurements

A performance measurement function (PMF) in the ATSSS capable UE and a PMF in the UPF can perform access performance measurements to decide how to distribute traffic over 3GPP access and non-3GPP access. The access performance measurements is performed based the default QoS flow. The access performance measuremets can also be performed based on target QoS flow, that is used by the service data flow (SDF) traffic, if the UE is capable of performing the measurements based on target QoS flow.

An ATSSS capable UE receives measurement assistance information from the SMF during the PDU session establishment procedure for an MA PDU session as described in clause 5.32.5 of 3GPP TS 23.501 [2]. The measurement assistance information (MAI) can contain the addressing information of the PMF in the UPF, as well as indicator on whether access availability/unavailability reports need to be sent to the network. If the UE is capable UE of performing the measurements based on target QoS flow, the MAI can also contain an indicator that the UE is to perform access performance messaurements based on target QoS flow and the MAI therefore includes a target QoS flow list. The encoding of the measurement assistance information is specified in clause 6.1.5.

An ATSSS capable UE that supports the MPTCP steering functionality can use the measurements available at the MPTCP layer.

The following PMF protocol messages can be exchanged between the PMF in the UE and the PMF in the UPF:

a) messages for RTT measurements, only applicable for the ATSSS-LL steering functionality; or

b) messages for reporting access availability/unavailability by the UE to the UPF.

An ATSSS capable UE does not apply the ATSSS rules to the PMF protocol messages.

The performance measurement function protocol procedures are specified in clause 5. 4.3 and 5.4.4 including the procedures for:

a) UE-initiated RTT measurement; and

b) Network-initiated RTT measurement.

The access availability/unavailability procedures are specified in clause 5.4.5.

---------------------------------- NEXT CHANGE -----------------------------------

---------------------------------- NEXT CHANGE -----------------------------------

#### 6.1.5.2 Encoding of measurement assistance information

The measurement assistance information contains addressing information for the PMF in the UPF and is encoded as shown in figure 6.1.5.2-1 and figure 6.1.5.2-2 and table 6.1.5.2-1 and table 6.1.5.2-2.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| PMF IP address type | octet a+1 |
| PMF IP address | octet a+2octet b-5 |
| PMF 3GPP port | octet b-4octet b-3 |
| PMF non-3GPP port | octet b-2octet b-1 |
| 0Spare | 0Spare | 0Spare | 0Spare | 0Spare | 0Spare | Target QoS | AARI | octet b |
| Target QoS flow list | octet b+1\*octet c\* |

Figure 6.1.5.2-1: ATSSS parameter contents including one PMF IP address information

Table 6.1.5.2-1: PMF IP address type

|  |
| --- |
| PMF IP address type (octet a+1) is set as follows:Bits |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |  |
| 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 |  | IPv4 |
| 0 | 0 | 0 | 0 | 0 | 0 | 1 | 0 |  | IPv6 |
| 0 | 0 | 0 | 0 | 0 | 0 | 1 | 1 |  | IPv4IPv6 |
| All other values are spare. |
|  |
| If the PMF IP address type indicates IPv4, then the PMF IP address field contains an IPv4 address in 4 octets. |
|  |
| If the PMF IP address type indicates IPv6, then the PMF IP address field contains an IPv6 address in 16 octets. |
|  |
| If the PMF IP address type indicates IPv4IPv6, then the PMF IP address field contains two IP addresses. The first PMF IP address is an IPv4 address in 4 octets and the second PMF IP address is an IPv6 address in 16 octets. |
|  |
| PMF 3GPP port (octets b-4 – b-3) is allocated port number associated with the 3GPP access network. |
|  |
| PMF non-3GPP port (octets b-2 – b-1) is allocated port number associated with the non-3GPP access network. |
|  |
| AARI (access availability reporting indicator) (octet b, bit 1) is set as follows:Bit |
| **1** |  |
| 0 | Do not report the access availability |
| 1 | Report the access availability |
|  |
| Target QoS (octet b, bit 2) is set as follows:Bit |
| **1** |  |
| 0 | Do not perform access performance measurements based on target QoS flow |
| 1 | Perform access performance measurements based on target QoS flow |
|  |
| Target QoS flow list is according to QoS flow descriptions as defined in subclause 9.11.4.12 of 3GPP TS 24.501 [6]. |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| PMF 3GPP MAC address | octet a+1octet a+6 |
| PMF non-3GPP MAC address | octet a+7octet a+12 |
| 0Spare | 0Spare | 0Spare | 0Spare | 0Spare | 0Spare | Target QoS | AARI | octet a+13 |
| Target QoS flow list | octet a+14\*octet b\* |

Figure 6.1.5.2-2: ATSSS parameter contents including one PMF MAC address information

Table 6.1.5.2-2: PMF MAC address type

|  |
| --- |
| PMF 3GPP MAC address contains a 6 octets MAC address associated with the 3GPP access network. |
|  |
| PMF non-3GPP MAC address contains a 6 octets MAC address associated with the non-3GPP access network. |
|  |
| AARI (access availability reporting indicator) (octet a+13, bit 1) is set as follows:Bit |
| **1** |  |
| 0 | Do not report the access availability |
| 1 | Report the access availability |
|  |
| Target QoS (octet b, bit 2) is set as follows:Bit |
| **1** |  |
| 0 | Do not perform access performance measurements based on target QoS flow |
| 1 | Perform access performance measurements based on target QoS flow |
|  |
|  |
|  |

Editor's note: The enconding of target QoS flow list is FFS.

---------------------------------- NEXT CHANGE -----------------------------------