**3GPP TSG-CT WG1 Meeting #130-eC1-21xxxx**

**Electronic meeting, 20-28 May 2021 (was C1-213266)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.501** | **CR** | **3262** | **rev** | **1** | **Current version:** | **17.2.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Storage of 5GMM information for UEs in SNPN access operation mode | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | vivo | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNPN | | | | |  | ***Date:*** | | | 2021-05-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **C** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) ... Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In CR 2550 to TS 23.501 (S2-2101079) approved at SA#91-e, SA2 introduced enhancements to enable SNPN selection for access to SNPNs, which includes: when a UE in SNPN access mode supports access to an SNPN using credentials from a credentials holder and the UE is configured with the prioritized lists of preferred SNPNs, then  1) the UE can select a SNPN which is in one of the following lists:  - User controlled prioritized list of preferred SNPNs;  - Credentials Holder controlled prioritized list of preferred SNPNs;  Therefore, the current specification in subclause c.2, "the SNPN in the "list of subscriber data"", can be misleading that the SNPN can be among the above preferred SNPNs.  Quote from subclause c.2:  *" The following 5GMM parameters shall be stored per SNPN in a non-volatile memory in the ME together with the subscriber identifier associated with the SNPN identity of the SNPN in the "list of subscriber data" configured in the ME "*  As the definition of "subscribed SNPN" is added by agreed TS 23.122 CR0663(C1-212448), it is proposed to change "the SNPN" to "the subscribed SNPN" in the above highlighted part.    2) the UE may register in a "preferred SNPN" using the PLMN subscription  Quote:  *" An SNPN-enabled UE that supports access to an SNPN using credentials from a Credentials Holder and that is equipped with a PLMN subscription may additionally be configured with the following information for SNPN selection and registration using the PLMN subscription in SNPN access mode:*  *- User controlled prioritized list of preferred SNPNs;*  *- Credentials Holder controlled prioritized list of preferred SNPNs;*  *- Credentials Holder controlled prioritized list of preferred GINs."*  Therefore, it is proposed to update subclause c.2 to align with SA2 changes. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The storing of information for UE in SNPN access mode is updated to align with the SA2 changes:  1) "the SNPN" is changed to "the subscribed SNPN";  2) the 5GMM parameters may be associated with the selected PLMN subscription | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | 1) "the SNPN" may be mistakenly regarded as one of the preferred SNPN.  2)The 5GMM parameters cannot be associated with the selected PLMN subscription. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.1 C.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The first Change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**5GMM-IDLE mode:** In this specification, if the term is used standalone, a UE in 5GMM-IDLE mode means the UE can be either in 5GMM-IDLE mode over 3GPP access or in 5GMM-IDLE mode over non-3GPP access.

**5GMM-CONNECTED mode:** In this specification, if the term is used standalone, a UE in 5GMM-CONNECTED mode means the UE can be either in 5GMM-CONNECTED mode over 3GPP access or in 5GMM-CONNECTED mode over non-3GPP access.

**5GMM-IDLE mode over 3GPP access:** A UE is in 5GMM-IDLE mode over 3GPP access when no N1 NAS signalling connection between the UE and network over 3GPP access exists. The term 5GMM-IDLE mode over 3GPP access used in the present document corresponds to the term CM-IDLE state for 3GPP access used in 3GPP TS 23.501 [8].

**5GMM-CONNECTED mode over 3GPP access:** A UE is in 5GMM-CONNECTED mode over 3GPP access when an N1 NAS signalling connection between the UE and network over 3GPP access exists. The term 5GMM-CONNECTED mode over 3GPP access used in the present document corresponds to the term CM-CONNECTED state for 3GPP access used in 3GPP TS 23.501 [8].

**5GMM-IDLE mode over non-3GPP access:** A UE is in 5GMM-IDLE mode over non-3GPP access when no N1 NAS signalling connection between the UE and network over non-3GPP access exists. The term 5GMM-IDLE mode over non-3GPP access used in the present document corresponds to the term CM-IDLE state for non-3GPP access used in 3GPP TS 23.501 [8].

**5GMM-CONNECTED mode over non-3GPP access:** A UE is in 5GMM-CONNECTED mode over non-3GPP access when an N1 NAS signalling connection between the UE and network over non-3GPP access exists. The term 5GMM-CONNECTED mode over non-3GPP access used in the present document corresponds to the term CM-CONNECTED state for non-3GPP access used in 3GPP TS 23.501 [8].

**5GS services:** Services provided by PS domain. Within the context of this specification, 5GS services is used as a synonym for EPS services.

**5G-EA:** 5GS encryption algorithms. The term 5G-EA, 5G-EA0, 128-5G-EA1, 128-5G-EA2, 128-5G-EA3, 5G-EA4, 5G-EA5, 5G-EA6 and 5G-EA7 used in the present document corresponds to the term NEA, NEA0, 128-NEA1, 128-NEA2, 128-NEA3, NEA4, NEA5, NEA6 and NEA7 defined in 3GPP TS 33.501 [24].

**5G-IA:** 5GS integrity algorithms. The term 5G-IA, 5G-IA0, 128-5G-IA1, 128-5G-IA2, 128-5G-IA3, 5G-IA4, 5G-IA5, 5G-IA6 and 5G-IA7 used in the present document corresponds to the term NIA, NIA0, 128-NIA1, 128-NIA2, 128-NIA3, NIA4, NIA5, NIA6 and NIA7 defined in 3GPP TS 33.501 [24].

**Access stratum connection:** A peer to peer access stratum connection:

- between the UE and the NG-RAN for 3GPP access;

- between the UE and the N3IWF for untrusted non-3GPP access;

- between the UE and the TNGF for trusted non-3GPP access used by the UE;

- within the TWIF acting on behalf of the N5CW device for trusted non-3GPP access used by the N5CW device;

- between the 5G-RG and the W-AGF for wireline access used by the 5G-RG;

- within the W-AGF acting on behalf of the FN-RG for wireline access used by the FN-RG; or

- within the W-AGF acting on behalf of the N5GC device for wireline access used by the N5GC device.

The access stratum connection for 3GPP access corresponds to an RRC connection via the Uu reference point. The creation of the access stratum connection for untrusted non-3GPP access corresponds to the completion of the IKE\_SA\_INIT exchange (see IETF RFC 7296 [41]) via the NWu reference point. The creation of the access stratum connection for trusted non-3GPP access used by the UE corresponds to the UE reception of an EAP-request/5G-start via NWt reference point (see 3GPP TS 23.502 [9]). The creation of the access stratum connection for trusted non-3GPP access used by the N5CW device corresponds to the TWIF's start of acting on behalf of the N5CW device. The creation of the access stratum connection for wireline access used by the 5G-RG corresponds to the 5G-RG reception of an EAP-request/5G-packet over the W-CP EAP connection via the Y4 reference point (see 3GPP TS 23.316 [6D]). The creation of the access stratum connection for wireline access used by the FN-RG corresponds to the W-AGF's start of acting on behalf of the FN-RG. The creation of the access stratum connection for wireline access used by the N5GC device corresponds to the W-AGF's start of acting on behalf of the N5GC device.

**Access to SNPN services via a PLMN/To access SNPN services via a PLMN:** A UE is accessing SNPN services via a PLMN when the UE is connecting to the 5GCN of the SNPN using the 3GPP access of the PLMN.

**Aggregate maximum bit rate:** The maximum bit rate that limits the aggregate bit rate of a set of non-GBR bearers of a UE. Definition derived from 3GPP TS 23.501 [8].

**Always-on PDU session:** A PDU session for which user-plane resources have to be established during every transition from 5GMM-IDLE mode to 5GMM-CONNECTED mode. A UE requests a PDU session to be established as an always-on PDU session based on indication from upper layers and the network decides whether a PDU session is established as an always-on PDU session.

NOTE 1: How the upper layers in the UE are configured to provide an indication is outside the scope of the present document.

**Applicable UE radio capability ID for the current UE radio configuration in the selected network:** The UE has an applicable UE radio capability ID for the current UE radio configuration in the selected network if:

a) the UE supports RACS; and

b) the UE has:

1) a stored network-assigned UE radio capability ID which is associated with the PLMN ID or SNPN identity of the serving network and which maps to the set of radio capabilities currently enabled at the UE; or

2) a manufacturer-assigned UE radio capability ID which maps to the set of radio capabilities currently enabled at the UE.

**CAG cell:** A cell in which only members of the CAG can get normal service. Depending on local regulation, the CAG cell can provide emergency services also to subscribers who are not members of the CAG.

**CAG-ID:** A CAG-ID is a unique identifier within the scope of one PLMN defined in 3GPP TS 23.003 [4] which identifies a Closed Access Group (CAG) in the PLMN associated with a cell or group of cells to which access is restricted to members of the CAG.

**CAG restrictions:** Restrictions applied to a UE in accessing a PLMN's 5GCN via:

a) a non-CAG cell if the entry for the PLMN in the UE's "CAG information list" includes an "indication that the UE is only allowed to access 5GS via CAG cells"; or

b) a CAG cell if none of the CAG-ID(s) supported by the CAG cell is included in the "allowed CAG list" for the PLMN in the UE's "CAG information list".

The CAG restrictions are not applied in a PLMN when a UE accesses the PLMN due to emergency services.

**Cleartext IEs:** Information elements that can be sent without confidentiality protection in initial NAS messages as specified in subclause 4.4.6.

**Control plane CIoT 5GS optimization:** Signalling optimizations to enable efficient transport of user data (IP, Ethernet, Unstructured or SMS) over control plane via the AMF including optional header compression of IP data and Ethernet data.

**DNN determined by the AMF:** If no DNN requested by the UE is provided, a DNN determined by the AMF based subscription information or local policy. Otherwise DNN determined by the AMF is the DNN requested by the UE.

**DNN requested by the UE:** A DNN explicitly requested by the UE and included in a NAS request message.

**DNN selected by the network:** If DNN replacement applies, a DNN selected and indicated to the AMF by PCF. Otherwise DNN selected by the network is the DNN determined by the AMF.

**Default S-NSSAI**: An S-NSSAI in the subscribed S-NSSAIs marked as default.

**Globally-unique SNPN identity:** An SNPN identity with an NID whose assignment mode is not set to 1 (see 3GPP TS 23.003 [4]).

**User plane CIoT 5GS optimization:** Signalling optimizations to enable efficient transport of user data (IP, Ethernet or Unstructured) over the user plane.

**UE supporting CIoT 5GS optimizations:** A UE that supports control plane CIoT 5GS optimization or user plane CIoT 5GS optimization and one or more other CIoT 5GS optimizations when the UE is in N1 mode.

**Registered for 5GS services with control plane CIoT 5GS optimization:** A UE supporting CIoT 5GS optimizations is registered for 5GS services, and control plane CIoT 5GS optimization along with one or more other CIoT 5GS optimizations have been accepted by the network.

**Registered** **for 5GS services with user plane CIoT 5GS optimization:** A UE supporting CIoT 5GS optimizations is registered for 5GS services, and user plane CIoT 5GS optimization along with one or more other CIoT 5GS optimizations have been accepted by the network.

**Registered** **for 5GS services with CIoT 5GS optimization:** A UE is registered for 5GS services with control plane CIoT 5GS optimization or registered for 5GS services with user plane CIoT 5GS optimization.

**DNN based congestion control:** Type of congestion control at session management level that is applied to reject session management requests from UEs or release PDU sessions when the associated DNN is congested. DNN based congestion control can be activated at the SMF over session management level and also activated at the AMF over mobility management level.

**Emergency PDU session:** A PDU session established with the request type "initial emergency request" or "existing emergency PDU session".

**General NAS level congestion control:** Type of congestion control at mobility management level that is applied at a general overload or congestion situation in the network, e.g. lack of processing resources.

**Initial NAS message:** A NAS message is considered as an initial NAS message, if this NAS message can trigger the establishment of an N1 NAS signalling connection. For instance, the REGISTRATION REQUEST message is an initial NAS message.

**Initial registration for emergency services:** A registration performed with 5GS registration type "emergency registration" in the REGISTRATION REQUEST message.

**Last visited registered TAI:** A TAI which is contained in the registration area that the UE registered to the network and which identifies the tracking area last visited by the UE.

**Mapped S-NSSAI:** An S-NSSAI in the subscribed S-NSSAIs for the HPLMN, which is mapped to an S-NSSAI of the registered PLMN in case of a roaming scenario.

**N1 mode:** A mode of a UE allowing access to the 5G core network via the 5G access network.

**Native 5G-GUTI:** A 5G-GUTI previously allocated by an AMF.

**Non 5G capable over WLAN (N5CW) device:** A device that is not capable to operate as a UE supporting NAS signalling with the 5GCN over a WLAN access network. However, this device may be capable to operate as a UE supporting NAS signalling with 5GCN using the N1 reference point as specified in this specification over 3GPP access. An N5CW device may be allowed to access the 5GCN via trusted WLAN access network (TWAN) that supports a trusted WLAN interworking function (TWIF) as specified in 3GPP TS 24.502 [18].

**Non-CAG Cell:** An NR cell which does not broadcast any Closed Access Group identity or an E-UTRA cell connected to 5GCN.

**Non-globally-unique SNPN identity:** An SNPN identity with an NID whose assignment mode is set to 1 (see 3GPP TS 23.003 [4]).

**In NB-N1 mode:** Indicates this paragraph applies only to a system which operates in NB-N1 mode. For a multi-access system this case applies if the current serving radio access network provides access to network services via E-UTRA connected to 5GCN by NB-IoT (see 3GPP TS 36.300 [25B], 3GPP TS 36.331 [25A], 3GPP TS 36.306 [25D]).

**In WB-N1 mode:** Indicates this paragraph applies only to a system which operates in WB-N1 mode. For a multi-access system this case applies if the system operates in N1 mode with E-UTRA connected to 5GCN, but not in NB-N1 mode.

**In WB-N1/CE mode:** Indicates this paragraph applies only when a UE, which is a CE mode B capable UE (see 3GPP TS 36.306 [25D]), is operating in CE mode A or B in WB-N1 mode.

**Initial small data rate control parameters:** Parameters that, if received by the UE during the establishment of a PDU session, are used as initial parameters to limit the allowed data for the PDU session according to small data rate control after establishment of a PDU session as described in subclause 6.2.13. At expiry of the associated validity period, the initial small data rate control parameters are no longer valid and the small data rate control parameters apply.

**Initial small data rate control parameters for exception data:** Parameters corresponding to initial small data rate control parameters for small data rate control of exception data.

**N1 NAS signalling connection:** A peer to peer N1 mode connection between UE and AMF. An N1 NAS signalling connection is either the concatenation of an RRC connection via the Uu reference point and an NG connection via the N2 reference point for 3GPP access, or the concatenation of an IPsec tunnel via the NWu reference point and an NG connection via the N2 reference point for non-3GPP access.

**N6 PDU session:** A PDU session established between the UE and the User Plane Function (UPF) for transmitting the UE's IP data, Ethernet data or Unstructured data related to a specific application.

**NEF PDU session:** A PDU session established between the UE and the Network Exposure Function (NEF) for transmitting the UE's Unstructured data related to a specific application.

**Network slicing information:** information stored at the UE consisting of one or more of the following:

a) default configured NSSAI for PLMN;

b) configured NSSAI for a PLMN or an SNPN;

c) mapped S-NSSAI(s) for the configured NSSAI for a PLMN;

d) pending NSSAI for a PLMN or an SNPN;

e) mapped S-NSSAI(s) for the pending NSSAI for a PLMN;

f) rejected NSSAI for the current PLMN or SNPN;

g) mapped S-NSSAI(s) for the rejected NSSAI for the current PLMN;

h) rejected NSSAI for the failed or revoked NSSAA; and

i) for each access type:

1) allowed NSSAI for a PLMN or an SNPN;

2) mapped S-NSSAI(s) for the allowed NSSAI for a PLMN;

3) rejected NSSAI for the current registration area; and

4) mapped S-NSSAI(s) for the rejected NSSAI for the current registration area.

**Non-cleartext IEs:** Information elements that are not cleartext IEs.

**Non-emergency PDU session:** Any PDU session which is not an emergency PDU session.

**PDU address:** An IP address assigned to the UE by the packet data network.

**PDU session for LADN:** A PDU session with a DNN associated with a LADN.

**PDU session with suspended user-plane resources:** A PDU session for which user-plane resources were established or re-established, and for which data radio bearers were suspended when transition to 5GMM-CONNECTED mode with RRC inactive indication.

**Persistent PDU session:** either a non-emergency PDU session contains a GBR QoS flow with QoS equivalent to QoS of teleservice 11 and where there is a radio bearer associated with that PDU session over 3GPP access, or an emergency PDU session where there is a radio bearer associated with that PDU session over 3GPP access.

NOTE 2: An example of a persistent PDU session is a non-emergency PDU session with 5QI = 1 where there is a radio bearer associated with that context.

**Procedure transaction identity:** An identity which is dynamically allocated by the UE for the UE-requested 5GSM procedures or allocated by the UE or the PCF for the UE policy delivery procedures. The procedure transaction identity is released when the procedure is completed but it should not be released immediately.

**RAT frequency selection priority index:** A parameter provided by the AMF to the NG-RAN via the N2 reference point. The AMF selects an RFSP index for a particular UE based on the subscribed RFSP index, the locally configured operator's policies, the allowed NSSAI and the UE context information, including the UE's usage setting, if received during the registration procedure. Definition derived from 3GPP TS 23.501 [8].

**Registered for emergency services:** A UE is considered as "registered for emergency services" when it has successfully completed initial registration for emergency services.

**Registered PLMN**: The PLMN on which the UE is registered. The identity of the registered PLMN (MCC and MNC) is provided to the UE within the GUAMI field of the 5G-GUTI.

**Rejected NSSAI:** Rejected NSSAI for the current PLMN, SNPN or rejected NSSAI for the current registration area or rejected NSSAI for the failed or revoked NSSAA.

NOTE 3: Rejected NSSAI for the current PLMN, SNPN or rejected NSSAI for the current registration area contains a set of S-NSSAI(s) associated with a PLMN identity or SNPN identity for the current PLMN or SNPN and in roaming scenarios also contains a set of mapped HPLMN S-NSSAI(s) if available. Rejected NSSAI for the failed or revoked NSSAA only contains a set of S-NSSAI(s) associated with a PLMN identity or SNPN identity for the HPLMN or RSNPN.

**Rejected NSSAI for the current PLMN or SNPN:** A set of S-NSSAI(s) which was included in the requested NSSAI by the UE and is sent by the AMF with the rejection cause "S-NSSAI not available in the current PLMN or SNPN".

**Rejected NSSAI for the current registration area:** A set of S-NSSAI(s) which was included in the requested NSSAI by the UE and is sent by the AMF with the rejection cause "S-NSSAI not available in the current registration area".

**Rejected NSSAI for the failed or revoked NSSAA**: A set of S-NSSAI(s) which is sent by the AMF with the rejection cause "S-NSSAI not available due to the failed or revoked network slice-specific authentication and authorization".

**Local release:** Release of a PDU session without peer-to-peer signalling between the network and the UE.

NOTE 4: Local release can include communication among network entities.

**Removal of eCall only mode restriction:** All the limitations as described in 3GPP TS 22.101 [2] for the eCall only mode do not apply any more.

**SNPN access operation mode**: SNPN access mode or access to SNPN over non-3GPP access.

NOTE 5: The term "non-3GPP access" in an SNPN refers to the case where the UE is accessing SNPN services via a PLMN.

**S-NSSAI** **based congestion control:** Type of congestion control at session management level that is applied to reject session management requests from UEs or release PDU sessions when the associated S-NSSAI and optionally the associated DNN are congested. S-NSSAI based congestion control can be activated at the SMF over session management level and also activated at the AMF over mobility management level.

**Selected core network type information:** A type of core network (EPC or 5GCN) selected by the UE NAS layer in case of an E-UTRA cell connected to both EPC and 5GCN.

**UE configured for high priority access in selected PLMN:** A UE configured with one or more access identities equal to 1, 2, or 11-15 applicable in the selected PLMN as specified in subclause 4.5.2. Definition derived from 3GPP TS 22.261 [3].

**N5CW device supporting 3GPP access:** An N5CW device which supports acting as a UE in 3GPP access (i.e. which supports NAS over 3GPP access).

**UE operating in single-registration mode in a network supporting N26 interface:** A UE, supporting both N1 mode and S1 mode. During the last attach, tracking area update (see 3GPP TS 24.301 [15]) or registration procedures, the UE has received either a 5GS network feature support IE with IWK N26 bit set to "interworking without N26 interface not supported" or an EPS network feature support IE with IWK N26 bit set to "interworking without N26 interface not supported".

**UE using 5GS services with control plane CIoT 5GS optimization:** AUE that is registered for 5GS services with the control plane CIOT 5GS optimization accepted by the network.

**UE-DS-TT residence time:** The time taken within the UE and DS-TT to forward a packet between the UE and the DS-TT port.

**User-plane resources:** Resources established between the UE and the UPF. The user-plane resources consist of one of the following:

- user plane radio bearers via the Uu reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for 3GPP access;

- IPsec tunnels via the NWu reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for untrusted non-3GPP access;

- IPsec tunnels via the NWt reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for trusted non-3GPP access used by the UE;

- a layer-2 connection via the Yt reference point, a layer-2 or layer-3 connection via the Yw reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for trusted non-3GPP access used by the N5CW device;

- W-UP resources via Y4 reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for wireline access used by the 5G-RG; and

- L-W-UP resources via Y5 reference point, a tunnel via the N3 reference point and a tunnel via the N9 reference point (if any) for wireline access used by the FN-RG.

**W-AGF acting on behalf of the N5GC device:** A W-AGF that enables an N5GC device behind a 5G-CRG or an FN-CRG to connect to the 5G Core.

For the purposes of the present document, the following terms and definitions given in 3GPP TS 22.261 [2] apply:

**Non-public network**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.003 [4] apply:

**5G-GUTI**

**5G-S-TMSI**

**5G-TMSI**

**Global Line Identifier (GLI)**

**Global Cable Identifier (GCI)**

**GUAMI**

**IMEI**

**IMEISV**

**IMSI**

**PEI**

**SUPI**

**SUCI**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.122 [5] apply:

**CAG selection**

**Country**

**EHPLMN**

**HPLMN**

**Registered SNPN**

**Selected PLMN**

**Selected SNPN**

**Shared network**

**SNPN identity**

**Steering of Roaming (SOR)**

**Steering of Roaming information**

Subscribed SNPN

**Suitable cell**

**VPLMN**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.167 [6] apply:

**eCall over IMS**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.216 [6A] apply:

**SRVCC**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.401 [7] apply:

**eCall only mode**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.501 [8] apply:

**5G access network**

**5G core network**

**5G QoS flow**

**5G QoS identifier**

**5G-RG**

**5G-BRG**

**5G-CRG**

**5G System**

**Allowed area**

**Allowed NSSAI**

**AMF region**

**AMF set**

**Closed access group**

**Configured NSSAI**

**IAB-node**

**Local area data network**

**Network identifier (NID)**

**Network slice**

**NG-RAN**

**Non-allowed area**

**PDU session**

**PDU session type**

**Pending NSSAI**

**Requested NSSAI**

**Routing Indicator**

**Service data flow**

**Service Gap Control**

**Serving PLMN rate control**

**Small data rate control status**

**SNPN access mode**

**SNPN enabled UE**

**Stand-alone Non-Public Network**

**Time Sensitive Communication**

**UE presence in LADN service area**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 23.503 [10] apply:

**UE local configuration**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 24.008 [12] apply:

**GMM**

**MM**

**A/Gb mode**

**Iu mode**

**GPRS**

**Non-GPRS**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 24.301 [15] apply:

**CIoT EPS optimization**

**Control plane CIoT EPS optimization**

**EENLV**

**EMM**

**EMM-DEREGISTERED**

**EMM-DEREGISTERED-INITIATED**

**EMM-IDLE mode**

**EMM-NULL**

**EMM-****REGISTERED**

**EMM-REGISTERED-INITIATED**

**EMM-SERVICE-REQUEST-INITIATED**

**EMM-TRACKING-AREA-UPDATING-INITIATED**

**EPS**

**EPS security context**

**EPS services**

**Lower layer failure**

**Megabit**

**Message header**

**NAS signalling connection recovery**

**NB-S1 mode**

**Non-EPS services**

**S1 mode**

**User plane CIoT EPS optimization**

**WB-S1 mode**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 33.501 [24] apply:

**5G security context**

**5G NAS security context**

**ABBA**

**Current 5G NAS security context**

**Full native 5G NAS security context**

**K'**AME

**K**AMF

**K**ASME

**Mapped 5G NAS security context**

**Mapped security context**

**Native 5G NAS security context**

**NCC**

**Non-current 5G NAS security context**

**Partial native 5G NAS security context**

**RES\***

For the purposes of the present document, the following terms and definitions given in 3GPP TS 38.413 [31] apply:

**NG connection**

For the purposes of the present document, the following terms and definitions given in 3GPP TS 24.587 [19B] apply:

**E-UTRA-PC5**

**NR-PC5**

**V2X**

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Next change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## C.2 Storage of 5GMM information for UEs operating in SNPN access operation mode

The 5GMM information for UEs operating in SNPN access operation mode are stored according to the following conditions:

- if the UE does not support access to an SNPN using credentials from a credentials holder, the following 5GMM parameters shall be stored per subscribed SNPN in a non-volatile memory in the ME together with the subscriber identifier associated with the SNPN identity of the SNPN in the "list of subscriber data" configured in the ME (see 3GPP TS 23.122 [5]);and

- if the UE supports access to an SNPN using credentials from a credentials holder, the following 5GMM parameters shall be stored in a non-volatile memory in the ME per:

i) the subscribed SNPN together with the subscriber identifier associated with the selected entry in the "list of subscriber data" configured in the ME (see 3GPP TS 23.122 [5]); or

ii) the PLMN subscription together with the SUPI from the USIM which is associated with the PLMN subscription:

a) 5G-GUTI;

b) last visited registered TAI;

c) 5GS update status;

d) 5G NAS security context parameters from a full native 5G NAS security context (see 3GPP TS 33.501 [24]);

e) KAUSF and KSEAF (see 3GPP TS 33.501 [24]);

f) UE parameter update counter (see subclause 9.11.3.53A);

g) configured NSSAI(s);

h) NSSAI inclusion mode(s);

i) MPS indicator;

j) MCS indicator;

k) operator-defined access category definitions;

l) network-assigned UE radio capability IDs; and

m) signalled URSP (see 3GPP TS 24.526 [24]).

NOTE: Steering of roaming does not apply to an SNPN. Therefore, for a KAUSF which is generated for an SNPN, the UE does not store an associated SOR counter in the non-volatile memory.

If the 5GMM parameters are associated with the PLMN subscription, then the 5GMM parameters can only be used if the SUPI from the USIM which is associated with the selected PLMN subscription matches the SUPI stored in the non-volatile memory; else the UE shall delete the 5GMM parameters.

If the 5GMM parameters are associated with the subscribed SNPN of the entry in the "list of subscriber data", then the 5GMM parameters can only be used if the subscriber identifier of the selected entry of the "list of subscriber data" matches the subscriber identifier stored in the non-volatile memory.

Each configured NSSAI consists of S-NSSAI(s) stored together with an SNPN identity, if it is associated with an SNPN.

Each NSSAI inclusion mode is associated with an SNPN identity and access type.

The MPS indicator is stored together with an SNPN identity of the SNPN that provided it, and is valid in that registered SNPN.

The MCS indicator is stored together with an SNPN identity of the SNPN that provided it, and is valid in that registered SNPN.

Operator-defined access category definitions are stored together with an SNPN identity of the SNPN that provided them, and are valid in that SNPN. The maximum number of stored operator-defined access category definitions is UE implementation dependent.

Each network-assigned UE radio capability ID is stored together with an SNPN identity of the SNPN that provided it as well as a mapping to the corresponding UE radio configuration, and is valid in that SNPN. The UE shall be able to store at least the last 16 received network-assigned UE radio capability IDs. There shall be only one network-assigned UE radio capability ID stored for a given combination of SNPN identity and UE radio configuration and any existing UE radio capability ID shall be deleted when a new UE radio capability ID is added for the same combination of SNPN identity and UE radio configuration. If the UE receives a network-assigned UE radio capability ID with a Version ID value different from the value included in the network-assigned UE radio capability ID(s) stored at the UE for the serving SNPN, the UE may delete these stored network-assigned UE radio capability ID(s).

The allowed NSSAI(s) can be stored in a non-volatile memory in the ME. Allowed NSSAI consists of S-NSSAI(s) stored together with an SNPN identity, if it is associated with an SNPN.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*End of change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*