**3GPP TSG-CT WG1 Meeting #131-eC1-21xxxx**

**E-meeting, 19-27 August 2021 (was C1-214533)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **23.122** | **CR** | **0762** | **rev** | **1** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | The match all type criterion in SOR-CMCI |
|  |  |
| ***Source to WG:*** | vivo, Huawei, HiSilicon, Orange |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | eCPSOR\_CON |  | ***Date:*** | 2021-08-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | 1) It is not clear how to use the "match all type criterion" of SOR-CMCI.2) It is not clear how many match all type criterion can be in the SOR-CMCI.3) The description about SOR-CMCI in TS 23.122 v17.3.0 seems that, a SOR-CMCI rule can contain multiple criterions, which contradicts to the definition in TS24.501. |
|  |  |
| ***Summary of change:*** | It is proposed to: 1) consider the "match all type criterion" as the lowest priority in SOR-CMCI;2) clarify that there can be zero or one match all type critrion in the SOR-CMCI;3) clarify that each SOR-CMCI rule contains only one criterion. |
|  |  |
| ***Consequences if not approved:*** | 1) It is not clear how to use the "match all type criterion" of SOR-CMCI.2) It is not clear how many match all type criterion can be in the SOR-CMCI 3) The description about SOR-CMCI in TS 23.122 v17.3.0 can lead to misunderstanding that contradicts to the definition in TS24.501. |
|  |  |
| ***Clauses affected:*** | C.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The first Change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### C.4.1 General

The HPLMN, based on operator policy, may provide the UE with SOR-CMCI to control the timing when the UE enters idle mode and perform higher priority PLMN /access technology selection. This is achieved by the HPLMN indicating to the UE the criteria for releasing specific PDU session(s) or services to enter idle mode.

NOTE 1: The released PDU sessions may be re-established by the application once the UE successfully registers on a higher priority PLMN. User interaction is required for some applications.

The HPLMN may configure the SOR-CMCI in the UE, and may also provide the SOR-CMCI to the UE over N1 NAS signalling. The SOR-CMCI received over N1 NAS signalling takes precedence over the SOR-CMCI configured in the UE.

NOTE 2: The SOR-CMCI received over N1 NAS signalling in the SOR information is either the SOR-CMCI in the USAT REFRESH with command qualifier of type "Steering of Roaming" (see 3GPP TS 31.111 [41]) which is received in a secured packet, or the SOR-CMCI received in plain text.

If the UE receives SOR information containing the list of preferred PLMN/access technology combinations without SOR-CMCI, or the ME receives USAT REFRESH with command qualifier (see 3GPP TS 31.111 [41]) of type "Steering of Roaming" without SOR-CMCI, then:

1) if the UE has SOR-CMCI stored in the non-volatile memory of the ME, the UE shall use the SOR-CMCI stored in the non-volatile memory of the ME; and

2) if the UE has no SOR-CMCI stored in the non-volatile memory of the ME, the UE shall use the SOR-CMCI stored in the USIM, if any.

The UE shall delete the stored SOR-CMCI, if any, in the non-volatile memory of the ME and store the received SOR-CMCI in the non-volatile memory of the ME when:

1) the ME receives SOR-CMCI in the USAT REFRESH with command qualifier (see 3GPP TS 31.111 [41]) of type "Steering of Roaming"; or

2) the UE receives the steering of roaming information containing the SOR-CMCI over N1 NAS signalling and the UE receives the "Store the SOR-CMCI in the ME" indicator;

The ME shall not delete the SOR-CMCI when the UE is switched off. The ME shall delete the SOR-CMCI when a new USIM is inserted.

SOR-CMCI consists of SOR-CMCI rules. Each SOR-CMCI rule consists of the following parameters:

i) a criterion of one of the following types:

- PDU session attribute type criterion;

- service type criterion; or:

- match all type criterion; and

ii) a value for Tsor-cm timer associated with each criterion presented in i) indicating the time the UE shall wait before releasing the PDU sessions and entering idle mode.

SOR-CMCI contains zero, one or more SOR-CMCI rules with PDU session attribute type criterion, zero, one or more SOR-CMCI rules with service type criterion, and zero or one SOR-CMCI rule with match all type criterion.

If the SOR-CMCI received by the UE contains no SOR-CMCI rules, the UE shall act as if no SOR-CMCI is configured. Additionally, if the SOR-CMCI received by the UE also contains an indication to store the SOR-CMCI in the ME, the UE shall delete any configured SOR-CMCI in the ME.

PDU session attribute type criterion consists of one of the following:

a) DNN of the PDU session; or

b) S-NSSAI of the PDU session.

Service type criterion consists of one of the following:

a) IMS registration related signalling;

b) MMTEL voice call;

c) MMTEL video call; or

d) MO SMS over NAS or MO SMSoIP.

Match all type criterion consists of:

1. match all.

Editor's note: How to specify handling of the match all criterion to make the lowest priority in the SOR-CMCI criteria is FFS.

If there are more than one criterion applicable for a PDU session (ex. a criterion for the PDU session and another one for the service) then the timer Tsor-cm with the highest value shall apply.

If there are more than one criterion applicable to different ongoing PDU sessions or services leading to multiple applicable Tsor-cm timers, then all the applicable Tsor-cm timers shall be started. Further handling of such cases is described in clause C.4.2.

If the value for Tsor-cm timer equals "infinity" then the UE shall wait until the PDU session is released or the service is stopped.

The timer Tsor-cm is applicable only if the UE is in automatic network selection mode.

Upon switching to the manual network selection mode, the UE shall stop any timer Tsor-cm, if running. In this case, the UE is not required to enter idle mode and perform the de-registration procedure.

The UE shall consider the following services as exempted from being forced to release the related established PDU session, if any, enter idle mode and perform high priority PLMN/Access technology selection. These services are known to the UE by default and the UE shall not follow the SOR-CMCI criteria even if configured to interrupt such services:

i) emergency services.

The UE configured with high priority access in the selected PLMN shall consider all services to be exempted from being forced to release the related established PDU session, if any, enter idle mode and perform high priority PLMN/Access technology selection.

The user may configure the UE with a "user controlled list of services exempted from release due to SOR", consisting of one or more of the following:

i) MMTEL voice call;

ii) MMTEL video call; and

ii) SMS over NAS or SMSoIP.

If the UE has a configured "user controlled list of services exempted from release due to SOR" which is stored in the non-volatile memory of the ME, the "user controlled list of services exempted from release due to SOR" shall be deleted when a new USIM is inserted.

The UE shall set the value for Tsor-cm timer for all services included in the "user controlled list of services exempted from release due to SOR" to infinity.

Editor's Note: It is FFS how to ensure that the HPLMN can control if the UE can have a configured "user controlled list of services exempted from release due to SOR" and/or is aware that the UE has a configured "user controlled list of services exempted from release due to SOR", and/or the user is having a service that matches one of the services included in the "user controlled list of services exempted from release due to SOR" during SOR.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*End of Change\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*