**3GPP TSG-CT WG1 Meeting #137-eC1-224585**

**E-Meeting, 18th – 26th August 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.483** | **CR** | **0157** | **rev** | **1** | **Current version:** | **17.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Correcting MCData user profile MO below IPInformation |
|  |  |
| ***Source to WG:*** | , Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | MCProtoc18 |  | ***Date:*** | 2022-08-03 |
|  |  |  |  |  |
| ***Category:*** | **D** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In the headings of the management objects of /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry the "/" in front of the last "Entry" is missing. This CR adds the missing "/" to all the affeced headings. |
|  |  |
| ***Summary of change:*** | Adding the missing "/" to the headings of clauses 10.2.16L, 10.2.16M, 10.2.16N, 10.2.16O |
| ***To***  |  |
| ***Consequences if not approved:*** | Errors in the heading of the MO of these entries remain wrong. |
|  |  |
| ***Clauses affected:*** | 10.2.16L, 10.2.16M, 10.2.16N, 10.2.16O |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

### 10.2.16L /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry

Table 10.2.16L.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry

|  |
| --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of IPInformation data that can be used in the setup of an IP Connectivity session for a specific MCData user in a one-to-one communication. |

### 10.2.16M /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv4Information

Table 10.2.16M.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/
IPv4Information

|  |
| --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv4Information |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv4 host address or an IPv4 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. |

### 10.2.16N /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv6Information

Table 10.2.16N.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/
IPv6Information

|  |
| --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv6Information |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv6 host address or an IPv6 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. |

### 10.2.16O /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN

Table 10.2.16O.1: /<x>/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN

|  |
| --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a fully qualified domain name for a specific host or domain that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. |

\* \* \* End of Changes \* \* \* \*