**3GPP TSG-CT WG1 Meeting #137-eC1-22xxxx**

**E-Meeting, 18th – 26th August 2022 (was C1-224642)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.539** | **CR** | **0016** | **rev** | **1** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Removal of TSN AF feature support IE and TT feature support IE |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | Vertical\_LAN |  | ***Date:*** | 2022-08-18 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | At CT1#127, CR 0022 to TS 24.519 (C1-207687) was agreed. The CR added support for per-instance parameter handling for stream filter instance table, with a TSN AF and TT capability indications. The CR was revised at CT#90-e based on further feedback to remove the capability indications (see CP-203267) and instead add the following note in Table 9.8.1:NOTE 1: A sender compliant with this release of the specification shall include the StreamFilterInstanceIndex value in the Stream filter instance of the Stream filter instance table information element. A sender compliant with earlier versions of this specification does not include the StreamFilterInstanceIndex value in the Stream filter instance of the Stream filter instance table information element.However somehow the new IEs related to capability indications were implemented into the specification.Since they are not used in any message and serve no purpose, they must be removed from the specification. |
|  |  |
| ***Summary of change:*** | The TSN AF feature support IE and TT feature support IE were removed.Backward compatibility analysis:The CR is backward compatible since it removes IEs which are not used by either the TSN AF or the TT. |
|  |  |
| ***Consequences if not approved:*** | IEs which are not used in any message and serve no purpose will remain the specification, leading to erroneous implementations and interoperability issues. |
|  |  |
| ***Clauses affected:*** | 9.12, 9.13 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

## 9.12 Void

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
|  |  |
|  |  |
|  |  |  |  |  |  |  |  |  |

|  |
| --- |
|  |
|  |
|  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |

## 9.13 Void

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
|  |  |
|  |  |
|  |  |  |  |  |  |  |  |  |

|  |
| --- |
|  |
|  |
|  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |

\* \* \* End of Changes \* \* \* \*