**3GPP TSG-CT WG1 Meeting #137-eC1-22xxxx**

**E-Meeting, 18th – 26th August 2022 *was* C1-224832**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.554** | **CR** | **0130** | **rev** | **1** | **Current version:** | **17.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Non-IP PDU transport procedure |
|  |  |
| ***Source to WG:*** | ZTE, OPPO |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | 5G\_ProSe |  | ***Date:*** | 2022-08-18 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The discussion paper C1-224831 analyses the non-IP PDU (as defined in clause 11.5 of TS 24.554) for non-IP data transport between over PC5 and gives justifications that the non-IP type field is not needed. In another word, it is unnecessary to specifically design the non-IP PDU format. The non-IP PDU transport handling should be nothing different from the IP PDU transport handling. |
|  |  |
| ***Summary of change:*** | Remove clause 7.5 and 11.5. |
|  |  |
| ***Consequences if not approved:*** | Redundant non-IP PDU type field in the PDU is a waste of the radio signaling resource over PC5. |
|  |  |
| ***Clauses affected:*** | 7.5, 7.5.1, 7.5.2, 7.5.3, 11.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

## 7.5 Void

### 7.5.1 Void

### 7.5.2 Void

### 7.5.3 Void

\* \* \* Next Change \* \* \* \*

## 11.5 Void

|  |  |
| --- | --- |
|  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |
|  |  |
|  |
|  |
|  |

|  |
| --- |
|  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |
|  |
|  |
|  |

\* \* \* End of Changes \* \* \* \*