|  |  |
| --- | --- |
| 3GPP TS 23.038 V18.0.0 (2022-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  Alphabets and language-specific information  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 6

2 References 6

3 Abbreviations and definitions 7

4 SMS Data Coding Scheme 8

5 CBS Data Coding Scheme 11

6 Individual parameters 14

6.1 General principles 14

6.1.1 General notes 14

6.1.2 Character packing 14

6.1.2.1 SMS Packing 14

6.1.2.1.1 Packing of 7-bit characters 14

6.1.2.2 CBS Packing 15

6.1.2.2.1 Packing of 7-bit characters 15

6.1.2.3 USSD packing 16

6.1.2.3.1 Packing of 7 bit characters 16

6.2 Character sets and coding 19

6.2.1 GSM 7 bit Default Alphabet 19

6.2.1.1 GSM 7 bit default alphabet extension table 20

6.2.1.2 National Language Identifier 22

6.2.1.2.1 Introduction 22

6.2.1.2.2 Single shift mechanism 22

6.2.1.2.3 Locking shift mechanism 22

6.2.1.2.4 National Language Identifier 22

6.2.1.2.5 Processing of national language characters 23

6.2.2 8 bit data 24

6.2.3 UCS2 24

Annex A (normative): National Language Tables 25

A.1 Introduction 25

A.2 National Language Single Shift Tables 26

A.2.1 Turkish National Language Single Shift Table 26

A.2.2 Spanish National Language Single Shift Table 27

A.2.3 Portuguese National Language Single Shift Table 28

A.2.4 Bengali National Language Single Shift Table 28

A.2.5 Gujarati National Language Single Shift Table 30

A.2.6 Hindi National Language Single Shift Table 31

A.2.7 Kannada National Language Single Shift Table 32

A.2.8 Malayalam National Language Single Shift Table 33

A.2.9 Oriya National Language Single Shift Table 34

A.2.10 Punjabi National Language Single Shift Table 35

A.2.11 Tamil National Language Single Shift Table 36

A.2.12 Telugu National Language Single Shift Table 37

A.2.13 Urdu National Language Single Shift Table 38

A.3 National Language Locking Shift Tables 39

A.3.1 Turkish National Language Locking Shift Table 39

A.3.2 Void 40

A.3.3 Portuguese National Language Locking Shift Table 40

A.3.4 Bengali National Language Locking Shift Table 40

A.3.5 Gujarati National Language Locking Shift Table 42

A.3.6 Hindi National Language Locking Shift Table 43

A.3.7 Kannada National Language Locking Shift Table 44

A.3.8 Malayalam National Language Locking Shift Table 45

A.3.9 Oriya National Language Locking Shift Table 46

A.3.10 Punjabi National Language Locking Shift Table 47

A.3.11 Tamil National Language Locking Shift Table 48

A.3.12 Telugu National Language Locking Shift Table 49

A.3.13 Urdu National Language Locking Shift Table 50

Annex B (informative): Guidelines for creating language tables 51

B.1 Introduction 51

B.2 Template for Single Shift Language Tables 51

B.3 Template for Locking Shift Language Tables 53

Annex C (Informative): Example for locking shift and single shift mechanisms 54

C.1 Introduction 54

C.2 Example of single shift 54

C.3 Example of locking shift 54

Annex D (informative): Document change history 56

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 Indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the specification;

# 1 Scope

The present document defines the character sets, languages and message handling requirements for SMS, CBS and USSD and may additionally be used for Man Machine Interface (MMI) (3GPP TS 22.030 [2]).

The specification for the Data Circuit terminating Equipment/Data Terminal Equipment (DCE/DTE) interface (3GPP TS  27.005 [8]) will also use the codes specified herein for the transfer of SMS data to an external terminal.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] void

[2] 3GPP TS 22.030: "Man-Machine Interface (MMI) of the User Equipment (UE)".

[3] 3GPP TS 23.090: "Unstructured Supplementary Service Data (USSD) - Stage 2".

[4] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS) ".

[5] 3GPP TS 23.041: "Technical realization of Cell Broadcast Service (CBS)".

[6] 3GPP TS 24.011: "Point-to-Point (PP) Short Message Service (SMS) support on mobile radio interface".

[7] Void.

[8] 3GPP TS 27.005: "Use of Data Terminal Equipment - Data Circuit terminating Equipment (DTE - DCE) interface for Short Message Service (SMS) and Cell Broadcast Service (CBS)".

[10] ISO/IEC 10646: "Information technology; Universal Multiple-Octet Coded Character Set (UCS)".

[11] 3GPP TS 24.090: "Unstructured Supplementary Service Data (USSD); Stage 3".

[12] ISO 639: "Code for the representation of names of languages".

[13] 3GPP TS 23.042: "Compression algorithm for text messaging services".

[14] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[15] "Wireless Datagram Protocol Specification", Wireless Application Protocol Forum Ltd.

[16] ISO 1073-1 and ISO 1073-2 Alphanumeric character sets for optical recognition – Parts 1 and 2: Character sets OCR-A and OCR-B, respectively - Shapes and dimensions of the printed image.

[17] 3GPP TS 31.102: "Characteristics of the USIM application"

[18] 3GPP TS 51.011 Release 4 (version 4.x.x): “Specification of the Subscriber Identity Module - Mobile Equipment (SIM - ME) interface”

[19] 3GPP TS 24.294: "IMS Centralized Services (ICS) Protocol via I1 Interface".

[20] 3GPP TS 24.008: "Mobile radio interface Layer 3 specification; Core network protocols; Stage 3".

[21] 3GPP TS 24.301: " Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3".

# 3 Abbreviations and definitions

For the purposes of the present document, the following terms and definitions apply:

**National Language Identifier:** A code representing a specific language and thereby selecting a specific National Language Table.

**National Language Locking Shift Table:** A national language table which replaces the GSM 7 bit default alphabet table in the case where the locking shift mechanism as defined in subclause 6.2.1.2.3 is used.

**National Language Single Shift Table:** A national language table which replaces the GSM 7 bit default alphabet extension table in the case where the single shift mechanism as defined in subclause 6.2.1.2.2 is used.

**National Language Table:** A table containing the characters of a specific national language.

For the purposes of the present document, the abbreviations used in the present document are listed in 3GPP TR 21.905 [14].

# 4 SMS Data Coding Scheme

The TP-Data-Coding-Scheme field, defined in 3GPP TS 23.040 [4], indicates the data coding scheme of the TP‑UD field, and may indicate a message class. Any reserved codings shall be assumed to be the GSM 7 bit default alphabet (the same as codepoint 00000000) by a receiving entity. The octet is used according to a coding group which is indicated in bits 7..4. The octet is then coded as follows:

| Coding Group Bits  7..4 | Use of bits 3..0 |
| --- | --- |
| 00xx | General Data Coding indication Bits 5..0 indicate the following:  Bit 5, if set to 0, indicates the text is uncompressed Bit 5, if set to 1, indicates the text is compressed using the compression algorithm defined in 3GPP TS 23.042 [13]   Bit 4, if set to 0, indicates that bits 1 to 0 are reserved and have no message class meaning  Bit 4, if set to 1, indicates that bits 1 to 0 have a message class meaning::   Bit 1 Bit 0 Message Class 0 0 Class 0 0 1 Class 1 Default meaning: ME-specific. 1 0 Class 2 (U)SIM specific message 1 1 Class 3 Default meaning: TE specific (see 3GPP TS 27.005 [8])   Bits 3 and 2 indicate the character set being used, as follows : Bit 3 Bit2 Character set: 0 0 GSM 7 bit default alphabet 0 1 8 bit data 1 0 UCS2 (16bit) [10] 1 1 Reserved  NOTE: The special case of bits 7..0 being 0000 0000 indicates the GSM 7 bit default alphabet with no message class |
| 01xx | Message Marked for Automatic Deletion Group  This group can be used by the SM originator to mark the message ( stored in the ME or (U)SIM ) for deletion after reading irrespective of the message class.  The way the ME will process this deletion should be manufacturer specific but shall be done without the intervention of the End User or the targeted application. The mobile manufacturer may optionally provide a means for the user to prevent this automatic deletion.  Bit 5..0 are coded exactly the same as Group 00xx |
| 1000..1011 | Reserved coding groups |
| 1100 | Message Waiting Indication Group: Discard Message  The specification for this group is exactly the same as for Group 1101, except that:  - after presenting an indication and storing the status, the ME may discard the contents of the message.  The ME shall be able to receive, process and acknowledge messages in this group, irrespective of memory availability for other types of short message. |
| 1101 | Message Waiting Indication Group: Store Message  This Group defines an indication to be provided to the user about the status of types of message waiting on systems connected to the GSM/UMTS PLMN. The ME should present this indication as an icon on the screen, or other MMI indication. The ME shall update the contents of the Message Waiting Indication Status on the SIM (see 3GPP TS 51.011 [18]) or USIM (see 3GPP TS 31.102 [17]) when present or otherwise should store the status in the ME. In case there are multiple records of EFMWIS this information shall be stored within the first record. The contents of the Message Waiting Indication Status should control the ME indicator. For each indication supported, the mobile may provide storage for the Origination Address. The ME may take note of the Origination Address for messages in this group and group 1100.  Text included in the user data is coded in the GSM 7 bit default alphabet. Where a message is received with bits 7..4 set to 1101, the mobile shall store the text of the SMS message in addition to setting the indication. The indication setting should take place irrespective of memory availability to store the short message.  Bits 3 indicates Indication Sense:   Bit 3  0 Set Indication Inactive  1 Set Indication Active   Bit 2 is reserved, and set to 0   Bit 1 Bit 0 Indication Type:  0 0 Voicemail Message Waiting  0 1 Fax Message Waiting  1 0 Electronic Mail Message Waiting  1 1 Other Message Waiting\*  \* Mobile manufacturers may implement the "Other Message Waiting" indication as an additional indication without specifying the meaning. |
| 1110 | Message Waiting Indication Group: Store Message  The coding of bits 3..0 and functionality of this feature are the same as for the Message Waiting Indication Group above, (bits 7..4 set to 1101) with the exception that the text included in the user data is coded in the uncompressed UCS2 character set. |
| 1111 | Data coding/message class    Bit 3 is reserved, set to 0.    Bit 2 Message coding:  0 GSM 7 bit default alphabet  1 8-bit data    Bit 1 Bit 0 Message Class:  0 0 Class 0  0 1 Class 1 default meaning: ME-specific.  1 0 Class 2 (U)SIM-specific message.  1 1 Class 3 default meaning: TE specific (see 3GPP TS 27.005 [8]) |

GSM 7 bit default alphabet indicates that the TP-UD is coded from the GSM 7 bit default alphabet given in clause 6.2.1. When this character set is used, the characters of the message are packed in octets as shown in clause 6.1.2.1.1, and the message can consist of up to 160 characters. The GSM 7 bit default alphabet shall be supported by all MSs and SCs offering the service. If the GSM 7 bit default alphabet extension mechanism is used then the number of displayable characters will reduce by one for every instance where the GSM 7 bit default alphabet extension table is used. 8-bit data indicates that the TP-UD has user-defined coding, and the message can consist of up to 140 octets.

UCS2 character set indicates that the TP-UD has a UCS2 [10] coded message, and the message can consist of up to 140 octets, i.e. up to 70 UCS2 characters. The General notes specified in clause 6.1.1 override any contrary specification in UCS2, so for example even in UCS2 a <CR> character will cause the MS to return to the beginning of the current line and overwrite any existing text with the characters which follow the <CR>.

When a message is compressed, the TP-UD consists of the GSM 7 bit default alphabet or UCS2 character set compressed message, and the compressed message itself can consist of up to 140 octets in total.

When a mobile terminated message is class 0 and the MS has the capability of displaying short messages, the MS shall display the message immediately and send an acknowledgement to the SC when the message has successfully reached the MS irrespective of whether there is memory available in the (U)SIM or ME. The message shall not be automatically stored in the (U)SIM or ME.

The ME may make provision through MMI for the user to selectively prevent the message from being displayed immediately.

If the ME is incapable of displaying short messages or if the immediate display of the message has been disabled through MMI then the ME shall treat the short message as though there was no message class, i.e. it will ignore bits 0 and 1 in the TP-DCS and normal rules for memory capacity exceeded shall apply.

When a mobile terminated message is Class 1, the MS shall send an acknowledgement to the SC when the message has successfully reached the MS and can be stored. The MS shall normally store the message in the ME by default, if that is possible, but otherwise the message may be stored elsewhere, e.g. in the (U)SIM. The user may be able to override the default meaning and select their own routing.

When a mobile terminated message is Class 2 ((U)SIM-specific), an MS shall ensure that the message has been transferred to the SMS data field in the (U)SIM before sending an acknowledgement to the SC. The MS shall return a "protocol error, unspecified" error message (see 3GPP TS 24.011 [6]) if the short message cannot be stored in the (U)SIM and there is other short message storage available at the MS. If all the short message storage at the MS is already in use, the MS shall return "memory capacity exceeded". This behaviour applies in all cases except for an MS supporting (U)SIM Application Toolkit when the Protocol Identifier (TP-PID) of the mobile terminated message is set to "(U)SIM Data download" (see 3GPP TS 23.040 [4]).

When a mobile terminated message is Class 3, the MS shall send an acknowledgement to the SC when the message has successfully reached the MS and can be stored, irrespectively of whether the MS supports an SMS interface to a TE, and without waiting for the message to be transferred to the TE. Thus the acknowledgement to the SC of a TE-specific message does not imply that the message has reached the TE. Class 3 messages shall normally be transferred to the TE when the TE requests "TE‑specific" messages (see 3GPP TS 27.005 [8]). The user may be able to override the default meaning and select their own routing.

The message class codes may also be used for mobile originated messages, to provide an indication to the destination SME of how the message was handled at the MS.

The MS will not interpret reserved or unsupported values but shall store them as received. The SC may reject messages with a Data Coding Scheme containing a reserved value or one which is not supported.

# 5 CBS Data Coding Scheme

The CBS Data Coding Scheme indicates the intended handling of the message at the MS, the character set/coding, and the language (when applicable). Any reserved codings shall be assumed to be the GSM 7 bit default alphabet (the same as codepoint 00001111) by a receiving entity. The octet is used according to a coding group which is indicated in bits 7..4. The octet is then coded as follows:

| Coding Group  Bits  7..4 | Use of bits 3..0 |
| --- | --- |
| 0000 | Language using the GSM 7 bit default alphabet |
|  |  |
|  | Bits 3..0 indicate the language: |
|  | 0000 German |
|  | 0001 English |
|  | 0010 Italian |
|  | 0011 French |
|  | 0100 Spanish |
|  | 0101 Dutch |
|  | 0110 Swedish |
|  | 0111 Danish |
|  | 1000 Portuguese |
|  | 1001 Finnish |
|  | 1010 Norwegian |
|  | 1011 Greek |
|  | 1100 Turkish |
|  | 1101 Hungarian  1110 Polish |
|  | 1111 Language unspecified |
| 0001 | 0000 GSM 7 bit default alphabet; message preceded by language indication.  The first 3 characters of the message are a two-character representation of the language encoded according to ISO 639 [12], followed by a CR character. The CR character is then followed by 90 characters of text (NOTE 1).  0001 UCS2; message preceded by language indication  The message starts with a two GSM 7-bit default alphabet character representation of the language encoded according to ISO 639 [12]. This is padded to the octet boundary with two bits set to 0 and then followed by 40 characters of UCS2-encoded message (NOTE 1).  An MS not supporting UCS2 coding will present the two character language identifier followed by improperly interpreted user data.  0010..1111 Reserved |
| 0010.. | 0000 Czech  0001 Hebrew (NOTE 2)  0010 Arabic (NOTE 2)  0011 Russian (NOTE 2)  0100 Icelandic  0101..1111 Reserved for other languages using the GSM 7 bit default alphabet, with unspecified handling at the MS |
| 0011 | 0000..1111 Reserved for other languages using the GSM 7 bit default alphabet, with unspecified handling at the MS |
| 01xx | General Data Coding indication  Bits 5..0 indicate the following: |
|  |  |
|  | Bit 5, if set to 0, indicates the text is uncompressed  Bit 5, if set to 1, indicates the text is compressed using the compression algorithm defined in 3GPP TS 23.042 [13] |
|  |  |
|  | Bit 4, if set to 0, indicates that bits 1 to 0 are reserved and have no message class meaning  Bit 4, if set to 1, indicates that bits 1 to 0 have a message class meaning: |
|  |  |
|  | Bit 1 Bit 0 Message Class: |
|  | 0 0 Class 0 |
|  | 0 1 Class 1 Default meaning: ME-specific. |
|  | 1 0 Class 2 (U)SIM specific message. |
|  | 1 1 Class 3 Default meaning: TE-specific (see 3GPP TS 27.005 [8]) |
|  |  |
|  | Bits 3 and 2 indicate the character set being used, as follows: |
|  | Bit 3 Bit 2 Character set: |
|  | 0 0 GSM 7 bit default alphabet |
|  | 0 1 8 bit data |
|  | 1 0 UCS2 (16 bit) [10] |
|  | 1 1 Reserved |
| 1000 | Reserved coding groups |
| 1001 | Message with User Data Header (UDH) structure: |
|  |  |
|  | Bit 1 Bit 0 Message Class: |
|  | 0 0 Class 0 |
|  | 0 1 Class 1 Default meaning: ME-specific. |
|  | 1 0 Class 2 (U)SIM specific message. |
|  | 1 1 Class 3 Default meaning: TE-specific (see 3GPP TS 27.005 [8]) |
|  |  |
|  | Bits 3 and 2 indicate the alphabet being used, as follows: |
|  | Bit 3 Bit 2 Alphabet: |
|  | 0 0 GSM 7 bit default alphabet |
|  | 0 1 8 bit data |
|  | 1 0 USC2 (16 bit) [10] |
|  | 1 1 Reserved |
| 1010..1100 | Reserved coding groups |
| 1101 | I1 protocol message defined in 3GPP TS 24.294 [19] |
| 1110 | Defined by the WAP Forum [15] |
| 1111 | Data coding / message handling |
|  |  |
|  | Bit 3 is reserved, set to 0. |
|  |  |
|  | Bit 2 Message coding: |
|  | 0 GSM 7 bit default alphabet |
|  | 1 8 bit data |
|  |  |
|  | Bit 1 Bit 0 Message Class: |
|  | 0 0 No message class. |
|  | 0 1 Class 1 user defined. |
|  | 1 0 Class 2 user defined. |
|  | 1 1 Class 3 |
|  | default meaning: TE specific  (see 3GPP TS 27.005 [8]) |
| NOTE 1: The language indication shall appear at the start of each Message Information Page (see 3GPP TS 23.041 [5]) and the language indication on each Message Information Page shall be for the same language.  NOTE 2: Message text in Hebrew, Arabic and Russian cannot be encoded in the GSM 7-bit default alphabet. For these languages UCS2 encoding shall be used. | |

These codings may also be used for USSD and MMI/display purposes.

The message length specified in this subclause is not applicable for UTRAN, E-UTRAN, and NG-RAN, but only applicable for GSM.

See 3GPP TS 24.090 [11] for specific coding values applicable to USSD for MS originated USSD messages and MS terminated USSD messages. USSD messages using the default alphabet are coded with the GSM 7-bit default alphabet given in clause 6.2.1. The message can then consist of up to 182 user characters.

Cell Broadcast messages using the default alphabet are coded with the GSM 7-bit default alphabet given in clause 6.2.1. The Message Information Page then consists of 93 user characters.

If the GSM 7 bit default alphabet extension mechanism is used then the number of displayable characters will reduce by one for every instance where the GSM 7 bit default alphabet extension table is usedCell Broadcast Messages Information Page using 8-bit data have user-defined coding, and will each be 82 octets in length.

UCS2 character set indicates that the message is coded in UCS2 [10]. The General notes specified in clause 6.1.1 override any contrary specification in UCS2, so for example even in UCS2 a <CR> character will cause the MS to return to the beginning of the current line and overwrite any existing text with the characters which follow the <CR>. Cell Broadcast Messages Information Page encoded in UCS2 consist of 41 characters each.

When a CBS message received by the MS is message class 0 and the MS has the capability of displaying CBS messages, the MS shall display the message immediately. The message shall not be automatically stored in the (U)SIM or ME.

The ME may make provision through MMI for the user to selectively prevent the message from being displayed immediately.

If the ME is incapable of displaying CBS messages or if the immediate display of the message has been disabled through MMI then the ME shall treat the CBS message as though there was no message class, i.e. it will ignore bits 0 and 1 in the TP-DCS but may store the message either on the ME or on the (U)SIM.

Class 1 and Class 2 messages may be routed by the ME to user-defined destinations, but the user may override any default meaning and select their own routing.

Class 3 messages will normally be selected for transfer to a TE, in cases where a ME supports an SMS/CBS interface to a TE, and the TE requests "TE-specific" cell broadcast messages (see 3GPP TS 27.005 [8]). The user may be able to override the default meaning and select their own routing.

Messages with a User Data Header Structure are encoded as described in 3GPP TS 23.040 [4] for SMS, in subclauses 3.10 and 9.2.3.24.

The use of Cell Broadcast DCS values for messages with a User Data Header structure implies that the 82-bytes CB payload has a User Data Header structure.

The CBS message information field will contain the IEs as described in 3GPP TS 23.040. The concatenation IEs will not be used, as CB concatenation will rely in that case on the existing CB mechanism. Note that IEs that cannot be split and that IEs that are too large to fit in one CB segment cannot be transmitted using this mechanism. Also, some IEs as defined for SMS are not applicable for CB:

|  |  |
| --- | --- |
| VALUE (hex) | MEANING |
| 00 | Concatenated short messages, 8-bit reference number |
| 01 | Special SMS Message Indication |
| 06 | SMSC Control Parameters |
| 08 | Concatenated short message, 16-bit reference number |
| 20 | RFC 822 E-Mail Header |
| 23 | Enhanced Voice Mail Information |
| 70-7F | (U)SIM Toolkit Security Headers |
| 80-89 | SME to SME specific use |

# 6 Individual parameters

## 6.1 General principles

### 6.1.1 General notes

Except where otherwise indicated, the following shall apply to all character sets:

1: The characters marked "1)" are not used but are displayed as a space.

2: The characters of this set, when displayed, should approximate to the appearance of the relevant characters specified in ISO 1073 [16]and the relevant national standards.

3: Control characters:

|  |  |
| --- | --- |
| Code | Meaning |
| LF | Line feed: Any characters following LF which are to be displayed shall be presented as the next line of the message, commencing with the first character position. |
| CR | Carriage return: Any characters following CR which are to be displayed shall be presented as the current line of the message, commencing with the first character position. |
| SP | Space character. |

4: The display of characters within a message is achieved by taking each character in turn and placing it in the next available space from left to right and top to bottom.

### 6.1.2 Character packing

#### 6.1.2.1 SMS Packing

##### 6.1.2.1.1 Packing of 7-bit characters

If a character number α is noted in the following way:

b7 b6 b5 b4 b3 b2 b1

αa αb αc αd αe αf αg

The packing of the 7-bitscharacters in octets is done by completing the octets with zeros on the left.

For examples, packing: α

- one character in one octet:

- bits number:

7 6 5 4 3 2 1 0

0 1a 1b 1c 1d 1e 1f 1g

- two characters in two octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

0 0 2a 2b 2c 2d 2e 2f

- three characters in three octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

0 0 0 3a 3b 3c 3d 3e

- seven characters in seven octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

0 0 0 0 0 0 0 7a

- eight characters in seven octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

8a 8b 8c 8d 8e 8f 8g 7a

The bit number zero is always transmitted first.

Therefore, in 140 octets, it is possible to pack (140x8)/7=160 characters.

#### 6.1.2.2 CBS Packing

##### 6.1.2.2.1 Packing of 7-bit characters

If a character number α is noted in the following way:

b7 b6 b5 b4 b3 b2 b1

αa αb αc αd αe αf αg

the packing of the 7-bits characters in octets is done as follows:

bit number

7 6 5 4 3 2 1 0

octet number

1 2g 1a 1b 1c 1d 1e 1f 1g

2 3f 3g 2a 2b 2c 2d 2e 2f

3 4e 4f 4g 3a 3b 3c 3d 3e

4 5d 5e 5f 5g 4a 4b 4c 4d

5 6c 6d 6e 6f 6g 5a 5b 5c

6 7b 7c 7d 7e 7f 7g 6a 6b

7 8a 8b 8c 8d 8e 8f 8g 7a

8 10g 9a 9b 9c 9d 9e 9f 9g

.

.

81 93d 93e 93f 93g 92a 92b 92c 92d

82 0 0 0 0 0 93a 93b 93c

The bit number zero is always transmitted first.

Therefore, in 82 octets, it is possible to pack (82x8)/7 = 93.7, that is 93 characters. The 5 remaining bits are set to zero as stated above.

#### 6.1.2.3 USSD packing

#### 6.1.2.3.1 Packing of 7 bit characters

If a character number α is noted in the following way:

b7 b6 b5 b4 b3 b2 b1

αa αb αc αd αe αf αg

The packing of the 7-bit characters in octets is done by completing the octets with zeros on the left.

For example, packing: α

- one character in one octet:

- bits number:

7 6 5 4 3 2 1 0

0 1a 1b 1c 1d 1e 1f 1g

- two characters in two octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

0 0 2a 2b 2c 2d 2e 2f

- three characters in three octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

0 0 0 3a 3b 3c 3d 3e

- six characters in six octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

0 0 0 0 0 0 6a 6b

- seven characters in seven octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

0 0 0 1 1 0 1 7a

The bit number zero is always transmitted first.

- eight characters in seven octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

8a 8b 8c 8d 8e 8f 8g 7a

- nine characters in eight octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

8a 8b 8c 8d 8e 8f 8g 7a

0 9a 9b 9c 9d 9e 9f 9g

- fifteen characters in fourteen octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

8a 8b 8c 8d 8e 8f 8g 7a

10g 9a 9b 9c 9d 9e 9f 9g

11f 11g 10a 10b 10c 10d 10e 10f

12e 12f 12g 11a 11b 11c 11d 11e

13d 13e 13f 13g 12a 12b 12c 12d

14c 14d 14e 14f 14g 13a 13b 13c

15b 15c 15d 15e 15f 15g 14a 14b

0 0 0 1 1 0 1 15a

- sixteen characters in fourteen octets:

- bits number:

7 6 5 4 3 2 1 0

2g 1a 1b 1c 1d 1e 1f 1g

3f 3g 2a 2b 2c 2d 2e 2f

4e 4f 4g 3a 3b 3c 3d 3e

5d 5e 5f 5g 4a 4b 4c 4d

6c 6d 6e 6f 6g 5a 5b 5c

7b 7c 7d 7e 7f 7g 6a 6b

8a 8b 8c 8d 8e 8f 8g 7a

10g 9a 9b 9c 9d 9e 9f 9g

11f 11g 10a 10b 10c 10d 10e 10f

12e 12f 12g 11a 11b 11c 11d 11e

13d 13e 13f 13g 12a 12b 12c 12d

14c 14d 14e 14f 14g 13a 13b 13c

15b 15c 15d 15e 15f 15g 14a 14b

16a 16b 16c 16d 16e 16f 16g 15a

The bit number zero is always transmitted first.

Therefore, in 160 octets, is it possible to pack (160\*8)/7 = 182.8, that is 182 characters. The remaining 6 bits are set to zero as stated above.

Packing of 7 bit characters in USSD strings is done in the same way as for SMS (clause 6.1.2.1). The character stream is bit padded to octet boundary with binary zeroes as shown above.

If the total number of characters to be sent equals (8n‑1) where n=1,2,3 etc. then there are 7 spare bits at the end of the message. To avoid the situation where the receiving entity confuses 7 binary zero pad bits as the @ character, the carriage return or <CR> character (defined in clause 6.1.1) shall be used for padding in this situation, just as for Cell Broadcast.

If <CR> is intended to be the last character and the message (including the wanted <CR>) ends on an octet boundary, then another <CR> must be added together with a padding bit 0. The receiving entity will perform the carriage return function twice, but this will not result in misoperation as the definition of <CR> in clause 6.1.1 is identical to the definition of <CR><CR>.

The receiving entity shall remove the final <CR> character where the message ends on an octet boundary with <CR> as the last character.

## 6.2 Character sets and coding

This section provides list of character sets and codings to be supported by SMS, CBS, USSD and IEs included in NAS messages as specified in 3GPP TS 24.008 [20] and 3GPP TS 24.301 [21]. Implementation of the GSM 7 bit default alphabet is mandatory. Support of other character sets is optional.

It should be noted that support of Latin and non-Latin languages by GSM 7 bit default alphabet is limited. It is therefore essential to introduce UCS 2 character set in mobile stations, SCs and systems handling SMSs, CBSs, USSDs, and IEs included in NAS messages.

### 6.2.1 GSM 7 bit Default Alphabet

Bits per character: 7

CBS/USSD/IE of NAS message pad character: CR

Character table:

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ |  | SP | 0 | ¡ | P | ¿ | p |
| 0 | 0 | 0 | 1 | 1 | £ | \_ | ! | 1 | A | Q | a | q |
| 0 | 0 | 1 | 0 | 2 | $ |  | " | 2 | B | R | b | r |
| 0 | 0 | 1 | 1 | 3 | ¥ |  | # | 3 | C | S | c | s |
| 0 | 1 | 0 | 0 | 4 | è |  | ¤ | 4 | D | T | d | t |
| 0 | 1 | 0 | 1 | 5 | é |  | % | 5 | E | U | e | u |
| 0 | 1 | 1 | 0 | 6 | ù |  | & | 6 | F | V | f | v |
| 0 | 1 | 1 | 1 | 7 | ì |  | ' | 7 | G | W | g | w |
| 1 | 0 | 0 | 0 | 8 | ò |  | ( | 8 | H | X | h | x |
| 1 | 0 | 0 | 1 | 9 | Ç |  | ) | 9 | I | Y | i | y |
| 1 | 0 | 1 | 0 | 10 | LF |  | \* | : | J | Z | j | z |
| 1 | 0 | 1 | 1 | 11 | Ø | 1) | + | ; | K | Ä | k | ä |
| 1 | 1 | 0 | 0 | 12 | ø | Æ | , | < | L | Ö | l | ö |
| 1 | 1 | 0 | 1 | 13 | CR | æ | - | = | M | Ñ | m | ñ |
| 1 | 1 | 1 | 0 | 14 | Å | ß | . | > | N | Ü | n | ü |
| 1 | 1 | 1 | 1 | 15 | å | É | / | ? | O | § | o | à |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

#### 6.2.1.1 GSM 7 bit default alphabet extension table

The table below is reserved for symbols of international significance (e.g currency symbols). It also contains a mechanism to permit escape (Note 1) to additional tables for symbols of international significance in the event that the table below becomes fully populated.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  |  |  | | |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 0 | 4 |  | ^ |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 |  |  |  |  |  |  | € |  |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 0 | 8 |  |  | { |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 |  |  | } |  |  |  |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  |  |  |  |  |  |
| 1 | 1 | 0 | 0 | 12 |  |  |  | [ |  |  |  |  |
| 1 | 1 | 0 | 1 | 13 |  |  |  | ~ |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 |  |  |  | ] |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 |  |  | \ |  |  |  |  |  |
| In the event that an MS receives a code where a symbol is not represented in the above table then the MS shall display either the character shown in the main GSM 7 bit default alphabet table in subclause 6.2.1., or the character from the National Language Locking Shift Table in the case where the locking shift mechanism as defined in subclause 6.2.1.2.3 is used.  NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined. It is not intended that this extension mechanism should be used as an alternative to UCS2 to enhance the 7bit default alphabet character repertoire for national specific character sets.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed. | | | | | | | | | | | | |

#### 6.2.1.2 National Language Identifier

##### 6.2.1.2.1 Introduction

The national language tables are used for adding the special characters of certain languages that cannot be expressed using the GSM default 7 bit alphabet.

The principle is to use the National Language Identifier to indicate to a receiving entity that the message has been encoded using a national language table. Both single shift and locking shift mechanisms are defined.

The single shift mechanism, as defined in subclause 6.2.1.2.2, applies to a single character and it replaces the GSM 7 bit default alphabet extension table defined in subclause 6.2.1.1 with a National Language Single Shift Table (see subclause A.2).

The locking shift mechanism, as defined in subclause 6.2.1.2.3, applies throughout the message, or the current segment in case of a concatenated message, and it replaces the GSM 7 bit default alphabet defined in subclause 6.2.1 with a National Language Locking Shift Table (see subclause A.3) that defines the whole character set needed for the language.

In case that several languages are used, which require different national language tables, it is recommended to encode the message in UCS-2, however it is possible to use both single shift and locking shift with the corresponding tables in a single message.

Implementations based on older reference versions (so-called "legacy implementations") will use the fallback mechanisms that are defined in the earlier versions of the specification for handling of unknown characters.

##### 6.2.1.2.2 Single shift mechanism

In the case where single shift is not combined with locking shift, single shift means that the receiving entity shall decode all characters in the message (or the current segment in case of a concatenated message) using the GSM 7 bit default alphabet unless the escape mechanism is used, i.e <escape><character>, as defined in subclause 6.2.1.

The case where single shift and locking shift (which may be for the same or different languages) are combined is described in subclause 6.2.1.2.3.

If the escape mechanism is used then instead of the GSM 7 bit default alphabet extension table in subclause 6.2.1.1 the receiving entity shall decode the subsequent character using the National Language Single Shift Table for the indicated language in table 6.2.1.2.4.1. Each time a sending entity requires to send a character from the National Language Single Shift Table the sending entity shall encode this as <escape><character>, where the <character> is encoded using the indicated National Language Single Shift Table.

##### 6.2.1.2.3 Locking shift mechanism

Locking Shift means that the receiving entity shall decode all characters in the message (or the current segment in case of a concatenated message) using the National Language Locking Shift Table unless the escape mechanism is used. i.e. <escape><character>, as defined in subclause 6.2.1.

If the escape mechanism is used and no National Language Single Shift Table is indicated (see subclause 6.2.1.2.4), the receiving entity shall decode the message (or the current segment in case of a concatenated message) using the GSM 7 bit default alphabet extension table as defined in subclause 6.2.1.1.

If the escape mechanism is used and a National Language Single Shift Table is indicated (see subclause 6.2.1.2.4), the receiving entity shall decode the message (or the current segment in case of a concatenated message) using the National Language Single Shift Table as defined in subclause 6.2.1.2.2.

##### 6.2.1.2.4 National Language Identifier

A National Language Single Shift IE and a National Language Locking Shift IE can be included in the TP User Data Header, as defined in 3GPP TS 23.040 [4]. The receiving entity shall decode using single shift or locking shift as applicable for the language indicated in the National Language Identifier within these IEs.

The National Language Identifier octet is encoded as shown in table 6.2.1.2.4.1.

Table 6.2.1.2.4.1

|  |  |  |  |
| --- | --- | --- | --- |
| Language code b7……b0 | Language | National Language Single Shift Table | National Language Locking Shift Table |
| 00000000 | Reserved | n/a | n/a |
| 00000001 | Turkish | Subclause A.2.1 | Subclause A.3.1 |
| 00000010 | Spanish | Subclause A.2.2 | Not defined – fallback to GSM 7 bit default alphabet (see subclause 6.2.1) |
| 00000011 | Portuguese | Subclause A.2.3 | Subclause A.3.3 |
| 00000100 | Bengali | Subclause A.2.4 | Subclause A.3.4 |
| 00000101 | Gujarati | Subclause A.2.5 | Subclause A.3.5 |
| 00000110 | Hindi | Subclause A.2.6 | Subclause A.3.6 |
| 00000111 | Kannada | Subclause A.2.7 | Subclause A.3.7 |
| 00001000 | Malayalam | Subclause A.2.8 | Subclause A.3.8 |
| 00001001 | Oriya | Subclause A.2.9 | Subclause A.3.9 |
| 00001010 | Punjabi | Subclause A.2.10 | Subclause A.3.10 |
| 00001011 | Tamil | Subclause A.2.11 | Subclause A.3.11 |
| 00001100 | Telugu | Subclause A.2.12 | Subclause A.3.12 |
| 00001101 | Urdu | Subclause A.2.13 | Subclause A.3.13 |
| 00001110 to 11111111 | Reserved | n/a | n/a |

##### 6.2.1.2.5 Processing of national language characters

When supporting a specific national language, the sending entity shall support the encoding of messages using the corresponding National Language Identifier defined in subclause 6.2.1.2.4.

The receiving entity should be able to decode messages usingthe National Language Identifiers defined in subclause 6.2.1.2.4 for the languages that are supported by that entity.

If a message is received, containing a National Language Identifier indicating a reserved value or a value that is not supported by the receiving entity, the receiving entity shall ignore the IE (see 3GPP TS 23.040 [4]) in which the National Language Identifier was indicated.

The receiving entity shall be capable of processing both single shift and locking shift within the same message.

It is an implementation option for the sending entity whether to use the single shift mechanism, the locking shift mechanism or both.

NOTE 1: A message using the locking shift mechanism cannot make use of characters from the GSM 7 bit Default Alphabet table unless such characters are replicated in the National Language Locking Shift Table or (in the case of locking shift and single shift), the National Language Single Shift table.

NOTE 2: Encoding of a message using the national locking shift mechanism is not intended to be implemented until a formal request is issued by the relevant national regulatory body. This is because a receiving entity not supporting the relevant locking-shift decoding will present different characters from the ones intended by the sending entity.

NOTE 3: An SMS message using a locking shift table for a language may not be properly displayed when the terminal does not support the locking shift table for that language. When the network is aware of the list of the locking shift tables supported by the UE, the network can deliver the SMS messages using an appropriate encoding.

### 6.2.2 8 bit data

8 bit data is user defined

Padding: CR in the case of an 8 bit character set

Otherwise - user defined

Character table: User Specific

### 6.2.3 UCS2

Bits per character: 16

CBS/USSD pad character: CR

Character table: ISO/IEC 10646 [10]

Annex A (normative):   
National Language Tables

# A.1 Introduction

This annex contains character tables for specific languages whose characters are not wholly or partially present within the GSM 7 bit default alphabet.

# A.2 National Language Single Shift Tables

## A.2.1 Turkish National Language Single Shift Table

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | B1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  |  |  | | |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  | Ş | ç | ş |
| 0 | 1 | 0 | 0 | 4 |  | ^ |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 |  |  |  |  |  |  | € |  |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  | Ğ |  | ğ |  |
| 1 | 0 | 0 | 0 | 8 |  |  | { |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 |  |  | } |  | İ |  | ı |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  |  |  |  |  |  |
| 1 | 1 | 0 | 0 | 12 |  |  |  | [ |  |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) |  |  | ~ |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 |  |  |  | ] |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 |  |  | \ |  |  |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined. NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.2 Spanish National Language Single Shift Table

NOTE: This table also includes the character "ç" used in Catalan.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  |  |  | | |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  | Á |  | á |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 0 | 4 |  | ^ |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 |  |  |  |  |  | Ú | € | ú |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 0 | 8 |  |  | { |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 | ç |  | } |  | Í |  | í |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  |  |  |  |  |  |
| 1 | 1 | 0 | 0 | 12 |  |  |  | [ |  |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) |  |  | ~ |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 |  |  |  | ] |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 |  |  | \ |  | Ó |  | ó |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.3 Portuguese National Language Single Shift Table

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  |  |  | | |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  | À |  | Â |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 0 | 4 |  | ^ |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 | ê |  |  |  |  | Ú | € | ú |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 0 | 8 |  |  | { |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 | ç |  | } |  | Í |  | í |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 | Ô | 1) |  |  |  | Ã |  | ã |
| 1 | 1 | 0 | 0 | 12 | ô |  |  | [ |  | Õ |  | õ |
| 1 | 1 | 0 | 1 | 13 | 4) |  |  | ~ |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 | Á |  |  | ] |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 | á | Ê | \ |  | Ó |  | ó | â |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void.  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.4 Bengali National Language Single Shift Table

NOTE: In the table below, the Bengali characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 09EC | 09F6 | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 09ED | 09F7 | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 09EE | 09F8 | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 09EF | 09F9 | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 09DF | 09FA | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 09E0 |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 09E1 |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 09E2 |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 09E6 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 09E7 | 09E3 |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 09F2 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 09E8 | 09F3 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 09E9 | 09F4 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 09EA | 09F5 | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 09EB | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.5 Gujarati National Language Single Shift Table

NOTE: In the table below, the Gujarati characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0AEA |  | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0AEB |  | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0AEC |  | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 0AED |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0AEE |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0AEF |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ |  |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # |  |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 |  |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) |  |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0AE6 |  | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0AE7 |  | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0AE8 |  | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0AE9 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.6 Hindi National Language Single Shift Table

NOTE: In the table below, the Hindi characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 096A | 095B | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 096B | 095C | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 096C | 095D | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 096D | 095E | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 096E | 095F | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 096F | 0960 | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0951 | 0961 | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0952 | 0962 | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { | 0963 | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } | 0970 | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0953 | 0971 | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0954 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0966 | 0958 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0967 | 0959 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0968 | 095A | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0969 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.7 Kannada National Language Single Shift Table

NOTE: In the table below, the Kannada characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0CEA |  | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0CEB |  | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0CEC |  | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 0CED |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0CEE |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0CEF |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0CDE |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0CF1 |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0CF2 |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) |  |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0CE6 |  | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0CE7 |  | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0CE8 |  | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0CE9 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.8 Malayalam National Language Single Shift Table

NOTE: In the table below, the Malayalam characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0D6A | 0D7B | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0D6B | 0D7C | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0D6C | 0D7D | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 0D6D | 0D7E | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0D6E | 0D7F | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0D6F |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0D70 |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0D71 |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0D72 |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0D73 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0D66 | 0D74 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0D67 | 0D75 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0D68 | 0D7A | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0D69 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.9 Oriya National Language Single Shift Table

NOTE: In the table below, the Oriya characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0B6A |  | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0B6B |  | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0B6C |  | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 0B6D |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0B6E |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0B6F |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0B5C |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0B5D |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0B5F |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0B70 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0B66 | 0B71 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0B67 |  | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0B68 |  | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0B69 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.10 Punjabi National Language Single Shift Table

NOTE: In the table below, the Punjabi characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0A6A |  | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0A6B |  | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0A6C |  | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | OA6D |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0A6E |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0A6F |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0A59 |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0A5A |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0A5B |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0A5C |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0A66 | 0A5E | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0A67 | 0A75 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0A68 |  | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0A69 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.11 Tamil National Language Single Shift Table

NOTE: In the table below, the Tamil characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0BEA |  | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0BEB |  | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 0BEC |  | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 0BED |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0BEF |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0BEF |  | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0BF3 |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0BF4 |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0964 | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0965 | 0BF5 |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0BF6 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0BE6 | 0BF7 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0BE7 | 0BF8 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0BE8 | 0BFA | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0BE9 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.12 Telugu National Language Single Shift Table

NOTE: In the table below, the Telugu characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 0C6A | 0C7D | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 0C6B | 0C7E | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 06CC | 0C7F | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 06CD |  | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 0C6E |  | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 0C6F |  | E | U |  |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 0C58 |  | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 0C59 |  | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { |  | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' |  | } |  | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  | 0C78 |  | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 0C79 |  | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 0C66 | 0C7A | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 0C67 | 0C7B | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 0C68 | 0C7C | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 0C69 | \ |  | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

## A.2.13 Urdu National Language Single Shift Table

NOTE: In the table below, the Urdu characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ | < | 06F4 | 0613 | | | P |  |  |
| 0 | 0 | 0 | 1 | 1 | £ | = | 06F5 | 0614 | A | Q |  |  |
| 0 | 0 | 1 | 0 | 2 | $ | > | 06F6 | 061B | B | R |  |  |
| 0 | 0 | 1 | 1 | 3 | ¥ | ¡ | 06F7 | 061F | C | S |  |  |
| 0 | 1 | 0 | 0 | 4 | ¿ | ^ | 06F8 | 0640 | D | T |  |  |
| 0 | 1 | 0 | 1 | 5 | " | ¡ | 06F9 | 0652 | E | U | € |  |
| 0 | 1 | 1 | 0 | 6 | ¤ | \_ | 060C | 0658 | F | V |  |  |
| 0 | 1 | 1 | 1 | 7 | % | # | 060D | 066B | G | W |  |  |
| 1 | 0 | 0 | 0 | 8 | & | \* | { | 066C | H | X |  |  |
| 1 | 0 | 0 | 1 | 9 | ' | 0600 | } | 0672 | I | Y |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) | 0601 | 060E | 0673 | J | Z |  |  |
| 1 | 0 | 1 | 1 | 11 | \* | 1) | 060F | 06CD | K |  |  |  |
| 1 | 1 | 0 | 0 | 12 | + | 06F0 | 0610 | [ | L |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) | 06F1 | 0611 | ~ | M |  |  |  |
| 1 | 1 | 1 | 0 | 14 | - | 06F2 | 0612 | ] | N |  |  |  |
| 1 | 1 | 1 | 1 | 15 | / | 06F3 | \ | 06D4 | O |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

# A.3 National Language Locking Shift Tables

## A.3.1 Turkish National Language Locking Shift Table

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ |  | SP | 0 | İ | P | ç | p |
| 0 | 0 | 0 | 1 | 1 | £ | \_ | ! | 1 | A | Q | a | q |
| 0 | 0 | 1 | 0 | 2 | $ |  | " | 2 | B | R | b | r |
| 0 | 0 | 1 | 1 | 3 | ¥ |  | # | 3 | C | S | c | s |
| 0 | 1 | 0 | 0 | 4 | € |  | ¤ | 4 | D | T | d | t |
| 0 | 1 | 0 | 1 | 5 | é |  | % | 5 | E | U | e | u |
| 0 | 1 | 1 | 0 | 6 | ù |  | & | 6 | F | V | f | v |
| 0 | 1 | 1 | 1 | 7 | ı |  | ' | 7 | G | W | g | w |
| 1 | 0 | 0 | 0 | 8 | ò |  | ( | 8 | H | X | h | x |
| 1 | 0 | 0 | 1 | 9 | Ç |  | ) | 9 | I | Y | i | y |
| 1 | 0 | 1 | 0 | 10 | LF |  | \* | : | J | Z | j | z |
| 1 | 0 | 1 | 1 | 11 | Ğ | 1) | + | ; | K | Ä | k | ä |
| 1 | 1 | 0 | 0 | 12 | ğ | Ş | , | < | L | Ö | l | ö |
| 1 | 1 | 0 | 1 | 13 | CR | ş | - | = | M | Ñ | m | ñ |
| 1 | 1 | 1 | 0 | 14 | Å | ß | . | > | N | Ü | n | ü |
| 1 | 1 | 1 | 1 | 15 | å | É | / | ? | O | § | o | à |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.2 Void

## A.3.3 Portuguese National Language Locking Shift Table

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | @ |  | SP | 0 | Í | P | ~ | p |
| 0 | 0 | 0 | 1 | 1 | £ | \_ | ! | 1 | A | Q | a | q |
| 0 | 0 | 1 | 0 | 2 | $ | ª | " | 2 | B | R | b | r |
| 0 | 0 | 1 | 1 | 3 | ¥ | Ç | # | 3 | C | S | c | s |
| 0 | 1 | 0 | 0 | 4 | ê | À | º | 4 | D | T | d | t |
| 0 | 1 | 0 | 1 | 5 | é | ∞ | % | 5 | E | U | e | u |
| 0 | 1 | 1 | 0 | 6 | ú | ^ | & | 6 | F | V | f | v |
| 0 | 1 | 1 | 1 | 7 | í | \ | ' | 7 | G | W | g | w |
| 1 | 0 | 0 | 0 | 8 | ó | € | ( | 8 | H | X | h | x |
| 1 | 0 | 0 | 1 | 9 | ç | Ó | ) | 9 | I | Y | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | | | \* | : | J | Z | j | z |
| 1 | 0 | 1 | 1 | 11 | Ô | 1) | + | ; | K | Ã | k | ã |
| 1 | 1 | 0 | 0 | 12 | ô | Â | , | < | L | Õ | l | õ |
| 1 | 1 | 0 | 1 | 13 | CR | â | - | = | M | Ú | m | ` |
| 1 | 1 | 1 | 0 | 14 | Á | Ê | . | > | N | Ü | n | ü |
| 1 | 1 | 1 | 1 | 15 | á | É | / | ? | O | § | o | à |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |
|  | | | | | | | | | | | | |

## A.3.4 Bengali National Language Locking Shift Table

NOTE: In the table below, the Bengali characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0981 | 0990 | SP | 0 | 09AC | 09BE | 09CE | p |
| 0 | 0 | 0 | 1 | 1 | 0982 |  | ! | 1 | 09AD | 09BF | a | q |
| 0 | 0 | 1 | 0 | 2 | 0983 |  | 099F | 2 | 09AE | 09C0 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0985 | 0993 | 09A0 | 3 | 09AF | 09C1 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0986 | 0994 | 09A1 | 4 | 09B0 | 09C2 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0987 | 0995 | 09A2 | 5 |  | 09C3 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0988 | 0996 | 09A3 | 6 | 09B2 | 09C4 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0989 | 0997 | 09A4 | 7 |  |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 098A | 0998 | ) | 8 |  |  | h | x |
| 1 | 0 | 0 | 1 | 9 | 098B | 0999 | ( | 9 |  | 09C7 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 099A | 09A5 | : | 09B6 | 09C8 | j | z |
| 1 | 0 | 1 | 1 | 11 | 098C | 1) | 09A6 | ; | 09B7 |  | k | 09D7 |
| 1 | 1 | 0 | 0 | 12 |  | 099B | , |  | 09B8 |  | l | 09DC |
| 1 | 1 | 0 | 1 | 13 | CR | 099C | 09A7 | 09AA | 09B9 | 09CB | m | 09DD |
| 1 | 1 | 1 | 0 | 14 |  | 099D | . | 09AB | 09BC | 09CC | n | 09F0 |
| 1 | 1 | 1 | 1 | 15 | 098F | 099E | 09A8 | ? | 09BD | 09CD | o | 09F1 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.5 Gujarati National Language Locking Shift Table

NOTE: In the table below, the Gujarati characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0A81 | 0A90 | SP | 0 | 0AAC | 0ABE | 0AD0 | p |
| 0 | 0 | 0 | 1 | 1 | 0A82 | 0A91 | ! | 1 | 0AAD | 0ABF | a | q |
| 0 | 0 | 1 | 0 | 2 | 0A83 |  | 0A9F | 2 | 0AAE | 0AC0 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0A85 | 0A93 | 0AA0 | 3 | 0AAF | 0AC1 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0A86 | 0A94 | 0AA1 | 4 | 0AB0 | 0AC2 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0A87 | 0A95 | 0AA2 | 5 |  | 0AC3 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0A88 | 0A96 | 0AA3 | 6 | 0AB2 | 0AC4 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0A89 | 0A97 | 0AA4 | 7 | 0AB3 | 0AC5 | g | w |
| 1 | 0 | 0 | 0 | 8 | 0A8A | 0A98 | ) | 8 |  |  | h | x |
| 1 | 0 | 0 | 1 | 9 | 0A8B | 0A99 | ( | 9 | 0AB5 | 0AC7 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0A9A | 0AA5 | : | 0AB6 | 0AC8 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0A8C | 1) | 0AA6 | ; | 0AB7 | 0AC9 | k | 0AE0 |
| 1 | 1 | 0 | 0 | 12 | 0A8D | 0A9B | , |  | 0AB8 |  | l | 0AE1 |
| 1 | 1 | 0 | 1 | 13 | CR | 0A9C | 0AA7 | 0AAA | 0AB9 | 0ACB | m | 0AE2 |
| 1 | 1 | 1 | 0 | 14 |  | 0A9D | . | 0AAB | 0ABC | 0ACC | n | 0AE3 |
| 1 | 1 | 1 | 1 | 15 | 0A8F | 0A9E | 0AA8 | ? | 0ABD | 0ACD | o | 0AF1 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.6 Hindi National Language Locking Shift Table

NOTE: In the table below, the Hindi characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0901 | 0910 | SP | 0 | 092C | 093E | 0950 | p |
| 0 | 0 | 0 | 1 | 1 | 0902 | 0911 | ! | 1 | 092D | 093F | a | q |
| 0 | 0 | 1 | 0 | 2 | 0903 | 0912 | 091F | 2 | 092E | 0940 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0905 | 0913 | 0920 | 3 | 092F | 0941 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0906 | 0914 | 0921 | 4 | 0930 | 0942 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0907 | 0915 | 0922 | 5 | 0931 | 0943 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0908 | 0916 | 0923 | 6 | 0932 | 0944 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0909 | 0917 | 0924 | 7 | 0933 | 0945 | g | w |
| 1 | 0 | 0 | 0 | 8 | 090A | 0918 | ) | 8 | 0934 | 0946 | h | x |
| 1 | 0 | 0 | 1 | 9 | 090B | 0919 | ( | 9 | 0935 | 0947 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 091A | 0925 | : | 0936 | 0948 | j | z |
| 1 | 0 | 1 | 1 | 11 | 090C | 1) | 0926 | ; | 0937 | 0949 | k | 0972 |
| 1 | 1 | 0 | 0 | 12 | 090D | 091B | , | 0929 | 0938 | 094A | l | 097B |
| 1 | 1 | 0 | 1 | 13 | CR | 091C | 0927 | 092A | 0939 | 094B | m | 097C |
| 1 | 1 | 1 | 0 | 14 | 090E | 091D | . | 092B | 093C | 094C | n | 097E |
| 1 | 1 | 1 | 1 | 15 | 090F | 091E | 0928 | ? | 093D | 094D | o | 097F |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.7 Kannada National Language Locking Shift Table

NOTE: In the table below, the Kannada characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  | 0C90 | SP | 0 | 0CAC | 0CBE | 0CD5 | p |
| 0 | 0 | 0 | 1 | 1 | 0C82 |  | ! | 1 | 0CAD | 0CBF | a | q |
| 0 | 0 | 1 | 0 | 2 | 0C83 | 0C92 | 0C9F | 2 | 0CAE | 0CC0 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0C85 | 0C93 | 0CA0 | 3 | 0CAF | 0CC1 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0C86 | 0C94 | 0CAA | 4 | 0CB0 | 0CC2 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0C87 | 0C95 | 0CA2 | 5 | 0CB1 | 0CC3 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0C88 | 0C96 | 0CA3 | 6 | 0CB2 | 0CC4 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0C89 | 0C97 | 0CA4 | 7 | 0CB3 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0C8A | 0C98 | ) | 8 |  | 0CC6 | h | x |
| 1 | 0 | 0 | 1 | 9 | 0C8B | 0C99 | ( | 9 | 0CB5 | 0CC7 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0C9A | 0CA5 | : | 0CB6 | 0CC8 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0C8C | 1) | 0CA6 | ; | 0CB7 |  | k | 0CD6 |
| 1 | 1 | 0 | 0 | 12 |  | 0C9B | , |  | 0CB8 | 0CCA | l | 0CE0 |
| 1 | 1 | 0 | 1 | 13 | CR | 0C9C | 0CA7 | 0CAA | 0CB9 | 0CCB | m | 0CE1 |
| 1 | 1 | 1 | 0 | 14 | 0C8E | 0C9D | . | 0CAB | 0CBC | 0CCC | n | 0CE2 |
| 1 | 1 | 1 | 1 | 15 | 0C8F | 0C9E | 0CA8 | ? | 0CBD | 0CCD | o | 0CE3 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.8 Malayalam National Language Locking Shift Table

NOTE: In the table below, the Malayalam characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  | 0D10 | SP | 0 | 0D2C | 0D3E | 0D57 | p |
| 0 | 0 | 0 | 1 | 1 | 0D02 |  | ! | 1 | 0D2D | 0D3F | a | q |
| 0 | 0 | 1 | 0 | 2 | 0D03 | 0D12 | 0D1F | 2 | 0D2E | 0D40 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0D05 | 0D13 | 0D20 | 3 | 0D2F | 0D41 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0D06 | 0D14 | 0D21 | 4 | 0D30 | 0D42 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0D07 | 0D15 | 0D22 | 5 | 0D31 | 0D43 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0D08 | 0D16 | 0D23 | 6 | 0D32 | 0D44 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0D09 | 0D17 | 0D24 | 7 | 0D33 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0D0A | 0D18 | ) | 8 | 0D34 | 0D46 | h | x |
| 1 | 0 | 0 | 1 | 9 | 0D0B | 0D19 | ( | 9 | 0D35 | 0D47 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0D1A | 0D25 | : | 0D36 | 0D48 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0D0C | 1) | 0D26 | ; | 0D37 |  | k | 0D60 |
| 1 | 1 | 0 | 0 | 12 |  | 0D1B | , |  | 0D38 | 0D4A | l | 0D61 |
| 1 | 1 | 0 | 1 | 13 | CR | 0D1C | 0D27 | 0D2A | 0D39 | 0D4B | m | 0D62 |
| 1 | 1 | 1 | 0 | 14 | 0D0E | 0D1D | . | 0D2B |  | 0D4C | n | 0D63 |
| 1 | 1 | 1 | 1 | 15 | 0D0F | 0D1E | 0D28 | ? | 0D3D | 0D4D | o | 0D79 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.9 Oriya National Language Locking Shift Table

NOTE: In the table below, the Oriya characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0B01 | 0B10 | SP | 0 | 0B2C | 0B3E | 0B56 | p |
| 0 | 0 | 0 | 1 | 1 | 0B02 |  | ! | 1 | 0B2D | 0B3F | a | q |
| 0 | 0 | 1 | 0 | 2 | 0B03 |  | 0B1F | 2 | 0B2E | 0B40 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0B05 | 0B13 | 0B20 | 3 | 0B2F | 0B41 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0B06 | 0B14 | 0B21 | 4 | 0B30 | 0B42 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0B07 | 0B15 | 0B22 | 5 |  | 0B43 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0B08 | 0B16 | 0B23 | 6 | 0B32 | 0B44 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0B09 | 0B17 | 0B24 | 7 | ଼0B33 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0B0A | 0B18 | ) | 8 |  |  | h | x |
| 1 | 0 | 0 | 1 | 9 | 0B0B | 0B19 | ( | 9 | 0B35 | 0B47 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0B1A | 0B25 | : | 0B36 | 0B48 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0B0C | 1) | 0B26 | ; | 0B37 |  | k | 0B57 |
| 1 | 1 | 0 | 0 | 12 |  | 0B1B | , |  | 0B38 |  | l | 0B60 |
| 1 | 1 | 0 | 1 | 13 | CR | 0B1C | 0B27 | 0B2A | 0B39 | 0B4B | m | 0B61 |
| 1 | 1 | 1 | 0 | 14 |  | 0B1D | . | 0B2B | 0B3C | 0B4C | n | 0B62 |
| 1 | 1 | 1 | 1 | 15 | 0B0F | 0B1E | 0B28 | ? | 0B3D | 0B4D | o | 0B63 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.10 Punjabi National Language Locking Shift Table

NOTE: In the table below, the Punjabi characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0A01 | 0A10 | SP | 0 | 0A2C | 0A3E | 0A51 | p |
| 0 | 0 | 0 | 1 | 1 | 0A02 |  | ! | 1 | 0A2D | 0A3F | a | q |
| 0 | 0 | 1 | 0 | 2 | 0A03 |  | 0A1F | 2 | 0A2E | 0A40 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0A05 | 0A13 | 0A20 | 3 | 0A2F | 0A41 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0A06 | 0A14 | 0A21 | 4 | 0A30 | 0A42 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0A07 | 0A15 | 0A22 | 5 |  |  | e | u |
| 0 | 1 | 1 | 0 | 6 | 0A08 | 0A16 | 0A23 | 6 | 0A32 |  | f | v |
| 0 | 1 | 1 | 1 | 7 | 0A09 | 0A17 | 0A24 | 7 | 0A33 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0A0A | 0A18 | ) | 8 |  |  | h | x |
| 1 | 0 | 0 | 1 | 9 |  | 0A19 | ( | 9 | 0A35 | 0A47 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0A1A | 0A25 | : | 0A36 | 0A48 | j | z |
| 1 | 0 | 1 | 1 | 11 |  | 1) | 0A26 | ; |  |  | k | 0A70 |
| 1 | 1 | 0 | 0 | 12 |  | 0A1B | , |  | 0A38 |  | l | 0A71 |
| 1 | 1 | 0 | 1 | 13 | CR | 0A1C | 0A27 | 0A2A | 0A39 | 0A4B | m | 0A72 |
| 1 | 1 | 1 | 0 | 14 |  | 0A1D | . | 0A2B | 0A3C | 0A4C | n | 0A73 |
| 1 | 1 | 1 | 1 | 15 | 0A0F | 0A1E | 0A28 | ? |  | 0A4D | o | 0A74 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.11 Tamil National Language Locking Shift Table

NOTE: In the table below, the Tamil characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  | 0B90 | SP | 0 |  | 0BBE | 0BD0 | p |
| 0 | 0 | 0 | 1 | 1 | 0B82 |  | ! | 1 |  | 0BBF | a | q |
| 0 | 0 | 1 | 0 | 2 | 0B83 | 0B92 | 0B9F | 2 | 0BAE | 0BC0 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0B85 | 0B93 |  | 3 | 0BAF | 0BC1 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0B86 | 0B94 |  | 4 | 0BB0 | 0BC2 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0B87 | 0B95 |  | 5 | 0BB1 |  | e | u |
| 0 | 1 | 1 | 0 | 6 | 0B88 |  | 0BA3 | 6 | 0BB2 |  | f | v |
| 0 | 1 | 1 | 1 | 7 | 0B89 |  | 0BA4 | 7 | 0BB3 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0B8A |  | ) | 8 | 0BB4 | 0BC6 | h | x |
| 1 | 0 | 0 | 1 | 9 |  | 0B99 | ( | 9 | 0BB5 | 0BC7 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0B9A |  | : | 0BB6 | 0BC8 | j | z |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  | ; | 0BB7 |  | k | 0BD7 |
| 1 | 1 | 0 | 0 | 12 |  |  | , | 0BA9 | 0BB8 | 0BCA | l | 0BF0 |
| 1 | 1 | 0 | 1 | 13 | CR | 0B9C |  | 0BAA | 0BB9 | 0BCB | m | 0BF1 |
| 1 | 1 | 1 | 0 | 14 | 0B8E |  | . |  |  | 0BCC | n | 0BF2 |
| 1 | 1 | 1 | 1 | 15 | 0B8F | 0B9E | 0BA8 | ? |  | 0BCD | o | 0BF9 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.12 Telugu National Language Locking Shift Table

NOTE: In the table below, the Telugu characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0C01 | 0C10 | SP | 0 | 0C2C | 0C3E | 0C55 | p |
| 0 | 0 | 0 | 1 | 1 | 0C02 |  | ! | 1 | 0C2D | 0C3F | a | q |
| 0 | 0 | 1 | 0 | 2 | 0C03 | 0C12 | 0C1F | 2 | 0C2E | 0C40 | b | r |
| 0 | 0 | 1 | 1 | 3 | 0C05 | 0C13 | 0C20 | 3 | 0C2F | 0C41 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0C06 | 0C14 | 0C21 | 4 | 0C30 | 0C42 | d | t |
| 0 | 1 | 0 | 1 | 5 | 0C07 | 0C15 | 0C22 | 5 | 0C31 | 0C43 | e | u |
| 0 | 1 | 1 | 0 | 6 | 0C08 | 0C16 | 0C23 | 6 | 0C32 | 0C44 | f | v |
| 0 | 1 | 1 | 1 | 7 | 0C09 | 0C17 | 0C24 | 7 | 0C33 |  | g | w |
| 1 | 0 | 0 | 0 | 8 | 0C0A | 0C18 | ) | 8 |  | 0C46 | h | x |
| 1 | 0 | 0 | 1 | 9 | 0C0B | 0C19 | ( | 9 | 0C35 | 0C47 | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 0C1A | 0C25 | : | 0C36 | 0C48 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0C0C | 1) | 0C26 | ; | 0C37 |  | k | 0C56 |
| 1 | 1 | 0 | 0 | 12 |  | 0C1B | , |  | 0C38 | 0C4A | l | 0C60 |
| 1 | 1 | 0 | 1 | 13 | CR | 0C1C | 0C27 | 0C2A | 0C39 | 0C4B | m | 0C61 |
| 1 | 1 | 1 | 0 | 14 | 0C0E | 0C1D | . | 0C2B |  | 0C4C | n | 0C62 |
| 1 | 1 | 1 | 1 | 15 | 0C0F | 0C1E | 0C28 | ? | 0C3D | 0C4D | o | 0C63 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

## A.3.13 Urdu National Language Locking Shift Table

NOTE: In the table below, the Urdu characters are represented using Unicode.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 | 0627 | 062B | SP | 0 | 0635 | 06BA | 0654 | p |
| 0 | 0 | 0 | 1 | 1 | 0622 | 062C | ! | 1 | 0636 | 06BB | a | q |
| 0 | 0 | 1 | 0 | 2 | 0628 | 0681 | 068F | 2 | 0637 | 06BC | b | r |
| 0 | 0 | 1 | 1 | 3 | 067B | 0684 | 068D | 3 | 0638 | 0648 | c | s |
| 0 | 1 | 0 | 0 | 4 | 0680 | 0683 | 0630 | 4 | 0639 | 06C4 | d | t |
| 0 | 1 | 0 | 1 | 5 | 067E | 0685 | 0631 | 5 | 0641 | 06D5 | e | u |
| 0 | 1 | 1 | 0 | 6 | 06A6 | 0686 | 0691 | 6 | 0642 | 06C1 | f | v |
| 0 | 1 | 1 | 1 | 7 | 062A | 0687 | 0693 | 7 | 06A9 | 06BE | g | w |
| 1 | 0 | 0 | 0 | 8 | 06C2 | 062D | ) | 8 | 06AA | 0621 | h | x |
| 1 | 0 | 0 | 1 | 9 | 067F | 062E | ( | 9 | 06AB | 06CC | i | y |
| 1 | 0 | 1 | 0 | 10 | LF | 062F | 0699 | : | 06AF | 06D0 | j | z |
| 1 | 0 | 1 | 1 | 11 | 0679 | 1) | 0632 | ; | 06B3 | 06D2 | k | 0655 |
| 1 | 1 | 0 | 0 | 12 | 067D | 068C | , | 069A | 06B1 | 064D | l | 0651 |
| 1 | 1 | 0 | 1 | 13 | CR | 0688 | 0696 | 0633 | 0644 | 0650 | m | 0653 |
| 1 | 1 | 1 | 0 | 14 | 067A | 0689 | . | 0634 | 0645 | 064F | n | 0656 |
| 1 | 1 | 1 | 1 | 15 | 067C | 068A | 0698 | ? | 0646 | 0657 | o | 0670 |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

Annex B (informative):  
Guidelines for creating language tables

# B.1 Introduction

This annex provides guidelines for creating language tables.

It is recommended that the characters and their positions in the table are checked by people fluent in the appropriate language, and preferably endorsed by an appropriate responsible body.

It is recommended that character positions are carefully selected so that receiving entities, which do not support the specific table, display symbols (glyphs) similar to the wanted symbols (glyphs) as far as possible.

# B.2 Template for Single Shift Language Tables

The format and structure of the table below shall be used to document the Language specific character codes used in the National Language selection mechanism.

It is recommended that a National Language Single Shift Table includes the characters represented in the GSM 7 bit default alphabet extension table (as defined in subclause 6.2.1.1) in the same character position. This ensures the availability of these characters in case when the single shift mechanism is used.

Language – (Note. The actual Country and table content will be annotated when the country is known).

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  |  |  |  |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 0 | 4 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 0 | 8 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 |  |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 0 | 10 | 3) |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  |  |  |  |  |  |
| 1 | 1 | 0 | 0 | 12 |  |  |  |  |  |  |  |  |
| 1 | 1 | 0 | 1 | 13 | 4) |  |  |  |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 |  |  |  |  |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 |  |  |  |  |  |  |  |  |
| NOTE 1): This code is reserved for the extension to another extension table. On receipt of this code, a receiving entity shall display a space until another extension table is defined.  NOTE 2): Void  NOTE 3): This code is defined as a Page Break character and may be used for example in compressed CBS messages. Any mobile station which does not understand the GSM 7 bit default alphabet table extension mechanism will treat this character as Line Feed.  NOTE 4): This code represents a control character and therefore must not be used for language specific characters. | | | | | | | | | | | | |

# B.3 Template for Locking Shift Language Tables

The format and structure of the table below shall be used to document the Language specific character codes used in the National Language selection mechanism.

Language – (Note. The actual Country and table content will be annotated when the country is known).

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | b7 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
|  |  |  |  | b6 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
|  |  |  |  | b5 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| b4 | b3 | b2 | b1 |  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| 0 | 0 | 0 | 0 | 0 |  |  | SP |  |  |  |  |  |
| 0 | 0 | 0 | 1 | 1 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 0 | 2 |  |  |  |  |  |  |  |  |
| 0 | 0 | 1 | 1 | 3 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 0 | 4 |  |  |  |  |  |  |  |  |
| 0 | 1 | 0 | 1 | 5 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 0 | 6 |  |  |  |  |  |  |  |  |
| 0 | 1 | 1 | 1 | 7 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 0 | 8 |  |  |  |  |  |  |  |  |
| 1 | 0 | 0 | 1 | 9 |  |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 0 | 10 | LF |  |  |  |  |  |  |  |
| 1 | 0 | 1 | 1 | 11 |  | 1) |  |  |  |  |  |  |
| 1 | 1 | 0 | 0 | 12 |  |  |  |  |  |  |  |  |
| 1 | 1 | 0 | 1 | 13 | CR |  |  |  |  |  |  |  |
| 1 | 1 | 1 | 0 | 14 |  |  |  |  |  |  |  |  |
| 1 | 1 | 1 | 1 | 15 |  |  |  |  |  |  |  |  |
| NOTE 1): This code is an escape to an extension of this table (either to the GSM 7 bit default alphabet extension table, see subclause 6.2.1.1, or a National Language Single Shift Table, see subclause 6.2.1.2.2). A receiving entity which does not understand the meaning of this escape mechanism shall display it as a space character. | | | | | | | | | | | | |

Annex C (Informative):  
Example for locking shift and single shift mechanisms

# C.1 Introduction

This annex gives an overview on how the national language extension mechanism of the GSM 7 bit default alphabet works. This annex shows how a message with an indication of the Turkish National Language Identifier is decoded, but the same principles apply to other languages.

# C.2 Example of single shift

This example outlines the behaviour of both supporting and non-supporting receiving entities where the Turkish National Language Single Shift Table is indicated in the received message. In this example there is no locking shift mechanism used in parallel.

A non-supporting receiving entity will ignore the National Language Single Shift IE, and decode the message contents using the GSM 7 bit default alphabet table defined in subclause 6.2.1, including possible escape characters to the GSM 7 bit default alphabet extension table specified in subclause 6.2.1.1. For example the Turkish word "Türkçe" will be displayed as "Türkce".

A receiving entity that supports the Turkish National Language Single Shift Table will detect a National Language Single Shift IE in a TP User Data Header. This IE tells the receiving entity that the single shift mechanism is used.

A supporting receiving entity will notice the language code, in this example coded as '0000 0001', and therefore use the Turkish National Language Single Shift Table defined in subclause A.2.1 instead of the GSM 7 bit default alphabet extension table defined in subclause 6.2.1.

If the next character is any character except <escape>, then the GSM 7 bit default alphabet table is used for the decode. If the next character is <escape> then the Turkish language specific table is used for the decode of the one character that follows the <escape>. This process will be repeated until the end of the received message, or until the end of the current segment of a concatenated message.

The Language selection at the start of a message takes 4 octets which correspond to five 7 bit characters which reduces the maximum number of characters per single message to 155.

Thereafter, the number of characters within that single message will be dependent upon the number of times a character is used that is within the National Language Single Shift Table.

Every character used from the National Language Single Shift Table will need an additional character to identify the escape to the National Language Single Shift Table. The available 155 character capacity of a single message will therefore be reduced accordingly. This reduction of overall message length also applies when using characters from the GSM 7 bit default alphabet extension table (see subclause 6.2.1.1) when the National Language Single Shift IE is not used.

# C.3 Example of locking shift

This example outlines the behaviour of both supporting and non-supporting receiving entities where the Turkish National Language Locking Shift Table is indicated in the received message.

A non-supporting receiving entity will ignore the National Language Locking Shift IE, and decode the message contents using the GSM 7 bit default alphabet defined in subclause 6.2.1, including possible escape characters to the GSM 7 bit default alphabet extensions specified in subclause 6.2.1.1.

A receiving entity that supports the scheme will detect a National Language Locking Shift IE in a TP User Data Header. This IE tells the receiving entity that the locking shift mechanism is used. If no National Language Single Shift IE is indicated additionally to the National Language Locking Shift IE, then the whole message is decoded using the National Language Locking Shift Table defined for Turkish language in subclause 6.2.1.2.4.1.

If, in addition to the National Language Locking Shift IE (which may be for Turkish or another language), a National Language Single Shift IE for the Turkish language is indicated, then <escape> makes an exception to the use of the National Language Locking Shift Table for the Turkish or another language. In that case a character following <escape> is decoded using the National Language Single Shift Table for the Turkish language, after which the use of the National Language Locking Shift Table for the Turkish or another language is resumed until the next <escape> or the end of the message is met.

The Language selection at the start of a message takes 4 octets which corresponds to five 7 bit characters which reduces the maximum number of characters per single message to 155, unless the National Language Single Shift IE has also been included, in which case there is a further reduction of 3 octets making 7 octets in total, which corresponds to eight 7 bit characters, which reduces the maximum number of characters per single message to 152.

Thereafter, if the single shift mechanism is used additionally to the locking shift mechanism, the number of characters within that single message will be dependent upon the number of times a character is used that is within the National Language Single Shift Table.

Every character in the National Language Single Shift Table will use an additional character. The available 152 character single message length will therefore be reduced accordingly. This reduction of overall message length also applies when using characters from the GSM 7 bit default alphabet extension table (see subclause 6.2.1.1) when the National Language Single Shift IE is not used.

Annex D (informative):  
Document change history

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **TSG#** | **TDoc** | **VERS** | **NEW\_VERS** | **CR** | **REV** | **Rel** | **CAT** | **WORK ITEM** | **SUBJECT** |
| T#4 |  |  | 3.0.0 | New |  |  |  |  | Creation of 3GPP TS 23.038 v1.0.0 out of GSM 03.38 v7.1.0 |
| T#4 | TP-99124 | 3.0.0 | 3.1.0 | 001 |  | R99 | A | MExE | Data Coding Scheme for WAP over USSD and CB |
| T#5 | TP-99177 | 3.1.0 | 3.2.0 | 002 |  | R99 | B | TEI | Language codes for Hebrew,Arabic and Russian |
| T#6 | TP-99237 | 3.2.0 | 3.3.0 | 003 |  | R99 | F | TEI | Adaptations for UMTS |
| T#8 | TP-000074 | 3.3.0 | 4.0.0 | 004 |  | Rel4 | B | TEI | Automatic removal of ‘read’ SMS |
| T#10 | TP-000195 | 4.0.0 | 4.1.0 | 005 |  | Rel4 | B | TEI | Data coding scheme value for the Icelandic language |
| T#11 | TP-010029 | 4.1.0 | 4.2.0 | 006 |  | Rel4 | C | UICC1-CPHS | Message Waiting Indication Status storage on the USIM |
| T#13 | TP-010194 | 4.2.0 | 4.3.0 | 007 |  | Rel4 | F | TEI4 | Support to UCS2 and editorial corrections |
| T#14 | TP-010280 | 4.3.0 | 4.4.0 | 008 |  | Rel4 | F | TEI4 | Deletion of GSM 01.04 reference |
| T#15 | TP-020015 | 4.4.0 | 5.0.0 | 009 |  | Rel5 | F | TEI5 | User Data Header support over CBS |
| T#21 | TP-030173 | 5.0.0 | 6.0.0 | 010 |  | Rel6 | C | TEI6 | Additional Indications in SMS DCS |
| T#25 | TP-040205 | 6.0.0 | 6.1.0 | 013 | 2 | Rel6 | F | TEI6 | Message Waiting Indication – how to handle Multiple Subscriber Profiles |
| T#25 | TP-040171 | 6.0.0 | 6.1.0 | 014 |  | Rel6 | F | TEI6 | Enhanced Voice Mail Information – not applicable for CBS |
| CT#31 | CP-060126 | 6.1.0 | 7.0.0 | 015r1 |  | Rel-7 | F | TEI7 | CBS – Reference removal |
| CT-39 | CP-080223 | 7.0.0 | 8.0.0 | 0017 | 5 | Rel-8 | B | TEI8 | SMS default alphabet. Generic solution for all languages |
| CT-39 | CP-080138 | 7.0.0 | 8.0.0 | 0019 |  | Rel-8 | B | TEI8 | SMS-addition of turkish national language locking shift table |
| CT-40 | CP-080361 | 8.0.0 | 8.1.0 | 0020 |  | Rel-8 | F | TEI8 | Corrections to single shift language tables for Turkish and Spanish |
| CT-40 | CP-080361 | 8.0.0 | 8.1.0 | 0021 | 3 | Rel-8 | F | TEI8 | Addition of national language tables for Portuguese |
| CT-41 | CP-080536 | 8.1.0 | 8.2.0 | 0229 | 1 | Rel-8 | F | TEI8 | Clarification of Locking / Single shift IE’s for different languages in a single SM |
| CT-45 | CP-090682 | 8.2.0 | 9.0.0 | 0231 | 3 | Rel-9 | B | TEI9 | Addition of language tables for India |
| CT-45 | CP-090682 | 8.2.0 | 9.0.0 | 0232 |  | Rel-9 | F | TEI9 | CBS Message Class 0 |
| CT-46 | CP-090912 | 9.0.0 | 9.1.0 | 0235 | 3 | Rel-9 | F | ETWS | Define the use of data coding scheme for the ETWS warning message |
| CT-46 | CP-090925 | 9.0.0 | 9.1.0 | 0236 |  | Rel-9 | B | IMS\_SCC-ICS\_I1 | Uniquely identify the I1 protocol in USSD |
|  |  | 9.1.0 | 9.1.1 |  |  | Rel-9 |  |  | Correction of a typo error in the change history table (wrong version number) |
| CT-51 |  | 9.1.1 | 10.0.0 |  |  | Rel-10 |  |  | Upgrade to Rel-10 |
| CT-57 |  | 10.0.0 | 11.0.0 |  |  | Rel-11 |  |  | Upgrade to Rel-11 |
| CT-65 |  | 11.0.0 | 12.0.0 |  |  | Rel-12 |  |  | Upgrade to Rel-12 |
| CT-70 |  | 12.0.0 | 13.0.0 |  |  | Rel-13 |  |  | Upgrade to Rel-13 |
| CT-75 |  | 13.0.0 | 14.0.0 |  |  | Rel-14 |  |  | Upgrade to Rel-14 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-06 | SA-80 |  |  |  |  | Upgrade to Rel-15 | 15.0.0 |
| 2020-07 | SA-88e | - | - | - | - | Update to Rel-16 version (MCC) | 16.0.0 |
| 2022-03 | SA-95e | - | - | - | - | Update to Rel-17 version (MCC) | 17.0.0 |
| 2022-09 | SA-97e | CP-222172 | 0238 | 1 | F | Corrections to language handling in CBS | 18.0.0 |
| 2022-09 | SA-97e | CP-222172 | 0239 | 1 | F | Clarification of the codec of IEs in accordance to GSM 7 bit default alphabet included in NAS message | 18.0.0 |