**3GPP TSG-CT WG1 Meeting #137-eC1-225abc**

**E-Meeting, 18th – 26th August 2022 (was C1-224765)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.558** | **CR** | **0010** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction to the ACR request message | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | CT1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | EDGEAPP | | | | |  | ***Date:*** | | | 2022-08-23 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The specification provides specification of the ACR request message, i.e., operation Initiate of the Eees\_AppContextRelocation API.  However, there is need to update the attribute “easNotifInd” of the type “AcrInitReq” of the Eees\_AppContextRelocation as it is not aligned with stage 2 in TS 23.558. Quote of TS 23.558, clause 8.8.4.4: | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The “easNotifInd” attribute of the type “AcrInitReq” is made mandatory. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Specification not aligned with stage 2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.5.5.2.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

##### 6.5.5.2.3 Type: AcrInitReq

Table 6.5.5.2.3-1: Definition of type AcrInitReq

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| requestorId | string | M | 1 | Contains the identifier of the EEC that is sending the request. |  |
| easId | string | O | 0..1 | Contains the identifier of the EAS. |  |
| ueId | Gpsi | M | 1 | Contains the identifier of the concerned UE. |  |
| acId | string | O | 0..1 | Contains the identifier of the AC. |  |
| tEasEndpoint | EndPoint | M | 1 | Contains the endpoint information of the T-EAS. |  |
| sEasEndpoint | EndPoint | C | 0..1 | Contains the endpoint information of the S-EAS.  This attribute shall be provided when the "easNotifInd" attribute is set to "true" or when the "prevEasNotifInd" attribute is present and set to "true". |  |
| prevTEasEndpoint | EndPoint | C | 0..1 | Contains the endpoint information of the previous T-EAS.  This attribute shall be provided when the EEC re-sends the ACR request to indicate that a previous ACR is to be cancelled. |  |
| routeReq | RouteToLocation | O | 0..1 | Contains the T-EAS's DNAI information and the corresponding N6 traffic routing information and/or routing profile ID. |  |
| easNotifInd | boolean | M | 1 | Indicates whether the EAS should be notified about the need for ACR or ACR cancellation.  "true": Notification required.  "false" (default): Notification not required. |  |
| prevEasNotifInd | boolean | C | 0..1 | Indicates whether the EAS should be notified about ACR cancellation.  "true": Notification required.  "false" (default): Notification not required.  This attribute shall be provided when the EEC re-sends the ACR request to indicate that a previous ACR is to be cancelled. |  |
| eecCtxtReloc | EecCtxtReloc | O | 0..1 | Contains EEC context relocation information. |  |

\* \* \* End of Changes \* \* \* \*