**3GPP TSG-CT WG1 Meeting #137-eC1-225abc**

**E-Meeting, 18th – 26th August 2022 (was C1-224765)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.558** | **CR** | **0010** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction to the ACR request message  |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | CT1 |
|  |  |
| ***Work item code:*** | EDGEAPP |  | ***Date:*** | 2022-08-23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The specification provides specification of the ACR request message, i.e., operation Initiate of the Eees\_AppContextRelocation API.However, there is need to update the attribute “easNotifInd” of the type “AcrInitReq” of the Eees\_AppContextRelocation as it is not aligned with stage 2 in TS 23.558. Quote of TS 23.558, clause 8.8.4.4: |
|  |  |
| ***Summary of change:*** | The “easNotifInd” attribute of the type “AcrInitReq” is made mandatory. |
|  |  |
| ***Consequences if not approved:*** | Specification not aligned with stage 2. |
|  |  |
| ***Clauses affected:*** | 6.5.5.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

##### 6.5.5.2.3 Type: AcrInitReq

Table 6.5.5.2.3-1: Definition of type AcrInitReq

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| requestorId | string | M | 1 | Contains the identifier of the EEC that is sending the request. |  |
| easId | string | O | 0..1 | Contains the identifier of the EAS. |  |
| ueId | Gpsi | M | 1 | Contains the identifier of the concerned UE. |  |
| acId | string | O | 0..1 | Contains the identifier of the AC. |  |
| tEasEndpoint | EndPoint | M | 1 | Contains the endpoint information of the T-EAS. |  |
| sEasEndpoint | EndPoint | C | 0..1 | Contains the endpoint information of the S-EAS.This attribute shall be provided when the "easNotifInd" attribute is set to "true" or when the "prevEasNotifInd" attribute is present and set to "true". |  |
| prevTEasEndpoint | EndPoint | C | 0..1 | Contains the endpoint information of the previous T-EAS.This attribute shall be provided when the EEC re-sends the ACR request to indicate that a previous ACR is to be cancelled. |  |
| routeReq | RouteToLocation | O | 0..1 | Contains the T-EAS's DNAI information and the corresponding N6 traffic routing information and/or routing profile ID. |  |
| easNotifInd | boolean | M | 1 | Indicates whether the EAS should be notified about the need for ACR or ACR cancellation."true": Notification required."false" (default): Notification not required. |  |
| prevEasNotifInd | boolean | C | 0..1 | Indicates whether the EAS should be notified about ACR cancellation."true": Notification required."false" (default): Notification not required.This attribute shall be provided when the EEC re-sends the ACR request to indicate that a previous ACR is to be cancelled. |  |
| eecCtxtReloc | EecCtxtReloc | O | 0..1 | Contains EEC context relocation information. |  |

\* \* \* End of Changes \* \* \* \*