**3GPP TSG-CT WG1 Meeting #141eC1-232683**

**Online 17– 21 April 2023 (was C1-232051)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.575** | **CR** | **0002** | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** | Wrong format of the <X> node | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | |
| ***Source to TSG:*** | CT1 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | UEConfig5MBS | | | | |  | ***Date:*** | | 2023-04-01 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **F** | |  | | | | ***Release:*** | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | The specification provides a number of <X> nodes as a placeholder for one or more of other nodes providing necessary information. Hence, this <X> node does not carry any value/information itself.  However, the specification indicates in several places that <X> nodes are of character (i.e., “chr”) format instead of node (i.e., “node”) which is incorrect: | | | | | | | |
|  | |  | | | | | | | |
| ***Summary of change:*** | | The format of the <X> nodes of the RANInfo node and the PDUInfo node is corrected. | | | | | | | |
|  | |  | | | | | | | |
| ***Consequences if not approved:*** | | Wrong format of <X> nodes which leads to wrong implementation. | | | | | | | |
|  | | |  | | | | | | |
| ***Clauses affected:*** | | | 6.17, 6.21 | | | | | | |
|  | | |  | | | | | | |
|  | | | **Y** | **N** |  | | |  | |
| ***Other specs*** | | |  | **X** | Other core specifications | | | TS/TR ... CR ... | |
| ***affected:*** | | |  | **X** | Test specifications | | | TS/TR ... CR ... | |
| ***(show related CRs)*** | | |  | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | | |  | | | | | | |
| ***Other comments:*** | | |  | | | | | | |
|  | | |  | | | | | | |
| ***This CR's revision history:*** | | | V1: cover sheet updated; work item field. | | | | | | |

\* \* \* First Change \* \* \* \*

## 6.17 *<X>*/PLMNList/*<X>*/RANInfo/*<X>*

This node acts as a placeholder for one or more NR ARFCN values of one or more MBS frequencies.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get, Replace

- Values: N/A

\* \* \* Next Change \* \* \* \*

## 6.21 *<X>*/PLMNList/*<X>*/PDUInfo/PDUInfoList*/<X>*

This node acts as a placeholder for one or more PDU session-specific information values.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get, Replace

- Values: N/A

\* \* \* End of Changes \* \* \* \*