**3GPP TSG-CT WG1 Meeting #141eC1-232687**

**Online 17– 21 April 2023 (was C1-232053)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.575** | **CR** | **0004** | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| ***Title:*** |  | | | | | | | | |
|  |  | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | |
| ***Source to TSG:*** | CT1 | | | | | | | | |
|  |  | | | | | | | | |
| ***Work item code:*** | UEConfig5MBS | | | | |  | ***Date:*** | | 2023-04-19 |
|  |  | | | |  | |  | |  |
| ***Category:*** | **F** | |  | | | | ***Release:*** | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | |
| ***Reason for change:*** | | The specification lacks the DDF for the UE pre-configuration MO. | | | | | | | |
|  | |  | | | | | | | |
| ***Summary of change:*** | | The DDF is added. | | | | | | | |
|  | |  | | | | | | | |
| ***Consequences if not approved:*** | | Lack of DDF for the UE pre-configuration MO. | | | | | | | |
|  | | |  | | | | | | |
| ***Clauses affected:*** | | | (new) Annex A | | | | | | |
|  | | |  | | | | | | |
|  | | | **Y** | **N** |  | | |  | |
| ***Other specs*** | | |  | **X** | Other core specifications | | | TS/TR ... CR ... | |
| ***affected:*** | | |  | **X** | Test specifications | | | TS/TR ... CR ... | |
| ***(show related CRs)*** | | |  | **X** | O&M Specifications | | | TS/TR ... CR ... | |
|  | | |  | | | | | | |
| ***Other comments:*** | | |  | | | | | | |
|  | | |  | | | | | | |
| ***This CR's revision history:*** | | | V1: cover sheet updated; work item field. | | | | | | |

\* \* \* First Change \* \* \* \*

Annex A (informative):  
UE pre-configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version.

<?xml version="1.0" encoding="UTF-8"?>

<!DOCTYPE MgmtTree PUBLIC "-//OMA//DTD-DM-DDF 1.2//EN"

"http://www.openmobilealliance.org/tech/DTD/dm\_ddf-v1\_2.dtd">

<MgmtTree>

<VerDTD>1.2</VerDTD>

<Man>--The device manufacturer--</Man>

<Mod>--The device model--</Mod>

<Node>

<NodeName/>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<Description>UE pre-configuration for MBS</Description>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>The UE pre-configuration management object (MO).</DFTitle>

<DFType>

<DDFName>urn:oma:mo:ext-3gpp-UE-pre-config-MBS:1.0</DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>Name</NodeName>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>User displayable name for the node.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>PLMNList</NodeName>

<!-- The per-PLMN configuration starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>Per-PLMN configuration for MBS UE pre-configuration.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName></NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<DFType>

<DDFName></DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>PlmnId</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>PLMN identity.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>TMGIConfiguration</NodeName>

<!-- The TMGI configuration per PLMN starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>Per-PLMN TMGI configuration.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName>TMGIListForSA</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>TMGI provided via service announcement.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>TMGIList</NodeName>

<!-- The per-PLMN configuration starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>List of TMGI for service announcement information for MBS broadcast communication services.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName></NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<DFType>

<DDFName></DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>TMGI</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>TMGI for MBS broadcast communication services.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>USD</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>User service description.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>TMGIListForService</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>TMGI provided via MBS user service announcement.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

<Node>

<NodeName>TMGIList</NodeName>

<!-- The per-PLMN configuration starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>List of TMGI for MBS user service announcement information for MBS broadcast communication services.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName></NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<DFType>

<DDFName></DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>TMGI</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>TMGI for MBS broadcast communication services.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>USD</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<chr/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>User service description.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>RANInfo</NodeName>

<!-- The RAN configuration per PLMN starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>RAN-specific info for MBS broadcast communication services.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName></NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<DFType>

<DDFName></DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>NRARFCN</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<int/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>NRARFCN of one MBS broadcast frequency.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>PDUInfo</NodeName>

<!-- The PDU session configuration per PLMN starts here. -->

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>PDU session specific informnation for MBS multicast communication services.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

<Node>

<NodeName></NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<OneOrMore/>

</Occurrence>

<DFType>

<DDFName></DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>DNN</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<int/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>DNN of a PDU session for MBS multicast communication services.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>S-NSSAI</NodeName>

<DFProperties>

<AccessType>

<Get/>

<Replace/>

</AccessType>

<DFFormat>

<int/>

</DFFormat>

<Occurrence>

<One/>

</Occurrence>

<DFTitle>S-NSSAI of a PDU session for MBS multicast communication services.</DFTitle>

<DFType>

<MIME>text/plain</MIME>

</DFType>

</DFProperties>

</Node>

</Node>

</Node>

<Node>

<NodeName>Ext</NodeName>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<DFTitle>A collection of all extension objects.</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

</Node>

</Node>

</MgmtTree>

\* \* \* End of Changes \* \* \* \*