**3GPP TSG-CT WG1 Meeting #156C1-255701**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.559** | **CR** | **0016** | **rev** | **-** | **Current version:** | **19.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of info and externalDocs fields | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Lenovo | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI19 | | | | |  | ***Date:*** | | | 2025-09-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CR#0015 against TS 24.559 has modified the ADAE\_ServiceConfiguration API. Therefore TS version number included in the "description" field of the "externalDocs" object in the ADAE\_ServiceConfiguration API need to be updated.  TS 24.559 CR#0015 introduces backward compatible correction in Rel-19. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The ADAE\_ServiceConfiguration API version number set to value "1.1.0-alpha.4".  The TS version number in the "description" field of the "externalDocs" object is changed to "19.3.0". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* First Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# A.2 ADAE\_ServiceConfiguration API

openapi: 3.0.0

info:

title: ADAE\_ServiceConfiguration

version: 1.1.0-alpha.4

description: |

API for ADAE service configuration.

© 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 24.559 V19.3.0 Application Data Analytics Enablement Service; Stage 3.

url: https://www.3gpp.org/ftp/Specs/archive/24\_series/24.559/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/adae-sc/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/application-performance:

post:

description: >

Creates a new individual VAL performance analytics event subscription.

operationId: VALPerformanceSubscription

tags:

- VAL performance event subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: VAL performance event subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/application-performance/{appPerfId}:

delete:

description: Deletes an individual VAL performance event subscription.

operationId: DeleteIndValPerfEventSubsc

tags:

- Individual VAL performance event subscription

parameters:

- name: appPerfId

in: path

description: Identifier of an individual VAL performance event subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The individual VAL performance subscription matching the appPerfId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/ue2ue-session-performance/fetch:

post:

description: >

Obtain the UE-to-UE session performance analytics.

operationId: FetchUe2UeSessionPerformance

tags:

- Fetch UE-to-UE session performance analytics

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Ue2UePerfReq'

responses:

'200':

description: >

Successful case. The UE-to-UE session performance information is returned in

the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/Ue2UePerfResp'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/edge-load:

post:

description: >

Creates a new individual edge load data collection event subscription.

operationId: EdgeLoadDataCollectionSubscription

tags:

- Edge load data collection event subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Edge load data collection event subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/edge-load/{edgeLdId}:

delete:

description: Deletes an individual edge load data collection event subscription.

operationId: DeleteIndEdgeLdDataCollectEventSubsc

tags:

- Individual edge load data collection event subscription

parameters:

- name: edgeLdId

in: path

description: Identifier of an individual edge load data collection event subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The individual edge load data collection subscription matching the edgeLdId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/service-experience/pull:

post:

description: >

ADAE server pulls service experience report from the ADAE client.

operationId: PullSrvExpReport

tags:

- Pull service experienec report

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PullSrvExpInfo'

responses:

'200':

description: >

Successful case. The ADAE client provides service experience reporting to

the ADAE server.

content:

application/json:

schema:

$ref: '#/components/schemas/SrvExpInfoRep'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/collision-detection:

post:

description: >

Creates an individual collision detection analytics subscription.

operationId: CollisionDetAnalyticsSubsc

tags:

- Collision detection analytics subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Collision detection analytics subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/collision-detection/{collisionDetectionId}:

delete:

description: Removes the individual collision detection analytics subscription.

operationId: DeleteIndCollisionDetAnalyticsSubsc

tags:

- Individual collision detection analytics subscription

parameters:

- name: collisionDetectionId

in: path

description: Identifier of an individual collision detection analytics subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The Individual collision detection analytics subscription matching the

collisionDetectionId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/ue-group-loc-analytics:

post:

description: >

Creates an individual location-related UE group analytics subscription.

operationId: LocRelUeGroupSubscription

tags:

- Location-related UE group analytics subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: >

The location-related UE group analytics subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/ue-group-loc-analytics/{ueGroupLocId}:

delete:

description: Deletes the individual location-related UE group analytics subscription.

operationId: DeleteIndLocRelUeGroupSubsc

tags:

- Individual location-related UE group analytics subscription

parameters:

- name: ueGroupLocId

in: path

description: Identifier of an individual location-related UE group analytics subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The individual location-related UE group analytics subscription matching the

appPerfId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

Ue2UePerfReq:

description: ADAES requests ADAEC for the UE-to-UE session performance analytics.

type: object

properties:

serverId:

type: string

description: String identifying the ADAE server

analyticsId:

type: string

description: String identifying the UE-to-UE session analytics

valUeIds:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

description: >

One or more VAL UE IDs whose UE-to-UE session performance is requested.

pc5Qos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pc5QoSPara'

reportConfig:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

repThresholds:

description: >

Identifies reporting threshold corresponding to the analytics.

type: array

items:

$ref: '#/components/schemas/Ue2UeRepThreshold'

minItems: 1

dataAbstractReq:

description: >

Indicates whether the data abstraction is required (true) or not (false).

type: boolean

default: false

dataCollectReq:

$ref: '#/components/schemas/DataCollectReq'

area:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

timeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- serverId

- analyticsId

- valUeIds

- pc5Qos

Ue2UePerfResp:

description: >

ADAEC responds to ADAES with the UE-to-UE session performance analytics information.

type: object

properties:

dataOutputs:

type: array

items:

type: string

minItems: 1

description: >

UE-to-UE session performance analytics for prediction or statistics.

valUeIds:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

description: >

One or more VAL UE IDs whose UE-to-UE session performance has been requested.

analyticsId:

type: string

description: String identifying the UE-to-UE session analytics

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- dataOutputs

- valUeIds

Ue2UeRepThreshold:

description: Identifies reporting threshold corresponding to the analytics.

type: object

properties:

thrName:

$ref: 'TS29549\_SS\_ADAE\_Ue2UePerformanceAnalytics.yaml#/components/schemas/U2UAnalytics'

thrValue:

description: Indicates the value for the analytics threshold.

type: string

thrMatchDirect:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/MatchingDirection'

required:

- thrName

- thrValue

- thrMatchDirect

DataCollectReq:

description: Contains data collection requirements.

type: object

properties:

dataFormat:

description: Indicates the format of the requested data.

type: string

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

abstractLevel:

description: Indicates the desired level of abstraction of the requested data.

type: string

accuracyLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

required:

- dataFormat

PullSrvExpInfo:

description: Contains VAL server and service identities.

type: object

properties:

valServerId:

type: string

valServiceId:

type: string

required:

- valServerId

SrvExpInfoRep:

description: Allows ADAEC to provide the service experience report to the ADAES.

type: object

properties:

valUeId:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

valServerId:

type: string

description: String identifying the VAL server the service experience report applies.

valServiceId:

type: string

description: String identifying the VAL service

timeStamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

valSrvExpRep:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

required:

- valUeId

- valServerId

# Simple data types and Enumerations

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*