**3GPP TSG-CT WG1 Meeting #156C1-255701**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.559** | **CR** | **0016** | **rev** | **-** | **Current version:** | **19.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Lenovo |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-09-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | CRs modifying ADAE\_ServiceConfiguration API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CRs updates the ADAE\_ServiceConfiguration API for the present release:- TS 29.559 CR #0015 is a backward compatible correction in Rel-19.- TS 29.571 CR #0674 is a backward compatible correction in Rel-19.Since a new Rel-19 TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | The ADAE\_ServiceConfiguration API version number set to value "1.1.0-alpha.4".The TS version number in the "description" field of the "externalDocs" object is changed to "19.3.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* First Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# A.2 ADAE\_ServiceConfiguration API

openapi: 3.0.0

info:

 title: ADAE\_ServiceConfiguration

 version: 1.1.0-alpha.4

 description: |

 API for ADAE service configuration.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 24.559 V19.3.0 Application Data Analytics Enablement Service; Stage 3.

 url: https://www.3gpp.org/ftp/Specs/archive/24\_series/24.559/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/adae-sc/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

 /application-performance:

 post:

 description: >

 Creates a new individual VAL performance analytics event subscription.

 operationId: VALPerformanceSubscription

 tags:

 - VAL performance event subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

 callbacks:

 notificationUri:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfNotif'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: VAL performance event subscription resource created successfully.

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

 headers:

 Location:

 description: Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /application-performance/{appPerfId}:

 delete:

 description: Deletes an individual VAL performance event subscription.

 operationId: DeleteIndValPerfEventSubsc

 tags:

 - Individual VAL performance event subscription

 parameters:

 - name: appPerfId

 in: path

 description: Identifier of an individual VAL performance event subscription.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The individual VAL performance subscription matching the appPerfId is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /ue2ue-session-performance/fetch:

 post:

 description: >

 Obtain the UE-to-UE session performance analytics.

 operationId: FetchUe2UeSessionPerformance

 tags:

 - Fetch UE-to-UE session performance analytics

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/Ue2UePerfReq'

 responses:

 '200':

 description: >

 Successful case. The UE-to-UE session performance information is returned in

 the response body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/Ue2UePerfResp'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /edge-load:

 post:

 description: >

 Creates a new individual edge load data collection event subscription.

 operationId: EdgeLoadDataCollectionSubscription

 tags:

 - Edge load data collection event subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

 callbacks:

 notificationUri:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeNotif'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: Edge load data collection event subscription resource created successfully.

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

 headers:

 Location:

 description: Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /edge-load/{edgeLdId}:

 delete:

 description: Deletes an individual edge load data collection event subscription.

 operationId: DeleteIndEdgeLdDataCollectEventSubsc

 tags:

 - Individual edge load data collection event subscription

 parameters:

 - name: edgeLdId

 in: path

 description: Identifier of an individual edge load data collection event subscription.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The individual edge load data collection subscription matching the edgeLdId is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /service-experience/pull:

 post:

 description: >

 ADAE server pulls service experience report from the ADAE client.

 operationId: PullSrvExpReport

 tags:

 - Pull service experienec report

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PullSrvExpInfo'

 responses:

 '200':

 description: >

 Successful case. The ADAE client provides service experience reporting to

 the ADAE server.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SrvExpInfoRep'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /collision-detection:

 post:

 description: >

 Creates an individual collision detection analytics subscription.

 operationId: CollisionDetAnalyticsSubsc

 tags:

 - Collision detection analytics subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionSub'

 callbacks:

 notificationUri:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionNotif'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: Collision detection analytics subscription resource created successfully.

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_CollisionDetectionAnalytics.yaml#/components/schemas/CollisionDetectionSub'

 headers:

 Location:

 description: Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /collision-detection/{collisionDetectionId}:

 delete:

 description: Removes the individual collision detection analytics subscription.

 operationId: DeleteIndCollisionDetAnalyticsSubsc

 tags:

 - Individual collision detection analytics subscription

 parameters:

 - name: collisionDetectionId

 in: path

 description: Identifier of an individual collision detection analytics subscription.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The Individual collision detection analytics subscription matching the

 collisionDetectionId is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /ue-group-loc-analytics:

 post:

 description: >

 Creates an individual location-related UE group analytics subscription.

 operationId: LocRelUeGroupSubscription

 tags:

 - Location-related UE group analytics subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupSub'

 callbacks:

 notificationUri:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupNotif'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: >

 The location-related UE group analytics subscription resource created successfully.

 content:

 application/json:

 schema:

 $ref: 'TS29549\_SS\_ADAE\_LocationRelatedUeGroupAnalytics.yaml#/components/schemas/LocRelUeGroupSub'

 headers:

 Location:

 description: Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /ue-group-loc-analytics/{ueGroupLocId}:

 delete:

 description: Deletes the individual location-related UE group analytics subscription.

 operationId: DeleteIndLocRelUeGroupSubsc

 tags:

 - Individual location-related UE group analytics subscription

 parameters:

 - name: ueGroupLocId

 in: path

 description: Identifier of an individual location-related UE group analytics subscription.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: >

 The individual location-related UE group analytics subscription matching the

 appPerfId is deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 Ue2UePerfReq:

 description: ADAES requests ADAEC for the UE-to-UE session performance analytics.

 type: object

 properties:

 serverId:

 type: string

 description: String identifying the ADAE server

 analyticsId:

 type: string

 description: String identifying the UE-to-UE session analytics

 valUeIds:

 type: array

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 minItems: 1

 description: >

 One or more VAL UE IDs whose UE-to-UE session performance is requested.

 pc5Qos:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pc5QoSPara'

 reportConfig:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 repThresholds:

 description: >

 Identifies reporting threshold corresponding to the analytics.

 type: array

 items:

 $ref: '#/components/schemas/Ue2UeRepThreshold'

 minItems: 1

 dataAbstractReq:

 description: >

 Indicates whether the data abstraction is required (true) or not (false).

 type: boolean

 default: false

 dataCollectReq:

 $ref: '#/components/schemas/DataCollectReq'

 area:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

 timeWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - serverId

 - analyticsId

 - valUeIds

 - pc5Qos

 Ue2UePerfResp:

 description: >

 ADAEC responds to ADAES with the UE-to-UE session performance analytics information.

 type: object

 properties:

 dataOutputs:

 type: array

 items:

 type: string

 minItems: 1

 description: >

 UE-to-UE session performance analytics for prediction or statistics.

 valUeIds:

 type: array

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 minItems: 1

 description: >

 One or more VAL UE IDs whose UE-to-UE session performance has been requested.

 analyticsId:

 type: string

 description: String identifying the UE-to-UE session analytics

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - dataOutputs

 - valUeIds

 Ue2UeRepThreshold:

 description: Identifies reporting threshold corresponding to the analytics.

 type: object

 properties:

 thrName:

 $ref: 'TS29549\_SS\_ADAE\_Ue2UePerformanceAnalytics.yaml#/components/schemas/U2UAnalytics'

 thrValue:

 description: Indicates the value for the analytics threshold.

 type: string

 thrMatchDirect:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/MatchingDirection'

 required:

 - thrName

 - thrValue

 - thrMatchDirect

 DataCollectReq:

 description: Contains data collection requirements.

 type: object

 properties:

 dataFormat:

 description: Indicates the format of the requested data.

 type: string

 repPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 abstractLevel:

 description: Indicates the desired level of abstraction of the requested data.

 type: string

 accuracyLevel:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - dataFormat

 PullSrvExpInfo:

 description: Contains VAL server and service identities.

 type: object

 properties:

 valServerId:

 type: string

 valServiceId:

 type: string

 required:

 - valServerId

 SrvExpInfoRep:

 description: Allows ADAEC to provide the service experience report to the ADAES.

 type: object

 properties:

 valUeId:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 valServerId:

 type: string

 description: String identifying the VAL server the service experience report applies.

 valServiceId:

 type: string

 description: String identifying the VAL service

 timeStamp:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 valSrvExpRep:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 required:

 - valUeId

 - valServerId

# Simple data types and Enumerations

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*