**3GPP TSG-CT WG1 Meeting #156C1-255702**

**Göteborg, Sweden; 25th – 29th August 2025**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.549** | **CR** | **0049** | **rev** | **-** | **Current version:** | **18.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** | Lenovo |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2025-09-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | CR #0047 modifies ETC\_Configuration API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented.TS 24.549 CR#0047 introduces backward compatible correction in Rel-19.New TS version number is 19.0.0 and the "description" field of the "externalDocs" object in the ETC\_Configuration API and NSCE\_SliceInfo API are to be updated. |
| ***8*** |  |
| ***Summary of change:*** | The ETC\_Configuration API version number set to value "1.1.0-alpha.1".The TS version number in the "description" field of the "externalDocs" object is changed to "19.0.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | C.2, C.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# C.2 ETC\_Configuration API

openapi: 3.0.0

info:

 title: ETC\_Configuration

 version: 1.1.0-alpha.1

 description: |

 API for event triggered network slice adaptation configuration.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 24.549 V19.0.0 Application Data Analytics Enablement Service; Stage 3.

 url: https://www.3gpp.org/ftp/Specs/archive/24\_series/24.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/su\_nsc/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

 /val-services/{valServiceId}/configurations/{configurationId}:

 put:

 description: >

 Perfomrs event triggered network slice adaptation.

 operationId: EventTriggeredNetworkAdaptation

 tags:

 - Event triggered network adaptation (Document)

 parameters:

 - name: valServiceId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 - name: configurationId

 description: String identifying the resource.

 in: path

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NwSliceAdptEvent'

 responses:

 '204':

 description: >

 No Content. The requested network slice adaptation is successfullyprocessed.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 NwSliceAdptEvent:

 description: >

 Represents the event associated with triggered network slice adaptation

 with the underlying network.

 type: object

 properties:

 valUeIds:

 type: array

 minItems: 1

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 sliceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 appReqs:

 $ref: '#/components/schemas/AppReqs'

 required:

 - valUeIds

 - sliceId

 AppReqs:

 description: Represents requirements for the requested application.

 type: object

 properties:

 timeIntervals:

 type: array

 minItems: 1

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 area:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

\*\*\* End of Changes \*\*\*