**TSG-CT WG3 Meeting #108-e *C3-201xyz***

**E-Meeting, 19th – 28th February 2020 (Revision of C3-201298)**

**Source: Huawei**

**Title: Pseudo-CR on Procedure extension and data correction**

**Spec: 3GPP TS 29.517 1.0.1**

**Agenda item: 16.5**

**Document for: Agreement**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

- the attribute name used to indicate the Event Filter is incorrect;

- within the EventFilter data, application Id should be optional according to TS 23.288;

- in the OpenAPI file, the reference of appId is incorrect.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.517 v1.0.1.

\* \* \* First Change \* \* \* \*

#### 4.2.2.2 Creating a new subscription

Figure 4.2.2.2-1 illustrates the creation of a subscription.



Figure 4.2.2.2-1: Creation of a subscription

To subscribe to event notifications, the NF service consumer shall send an HTTP POST request to the AF with: "{apiRoot}/naf-eventexposure/{apiVersion}/subscriptions/" as request URI as shown in step 1 of figure 4.2.2.2-1, and the "AfEventExposureSubsc" data structure as request body.

The "AfEventExposureSubsc" data structure shall include:

- description of subscribed event information as "eventsSubs" attribute by using one or more "EventsSubs" data;

- description of the event reporting information as "eventsRepInfo" attribute;

- a URI where to receive the requested notifications as "notifUri" attribute;

- a Notification Correlation Identifier assigned by the NF service consumer for the requested notifications as "notifId" attribute.

The "EventsSubs" data shall include:

- a event to subscribe as a "event" attribute; and

- event filter information as "eventFilter" attribute associated with the event.

The "eventsRepInfo" attribute may include:

- event notification method (periodic, one time, on event detection) as "notifMethod" attribute;

- Maximum Number of Reports as "maxReportNbr" attribute;

- Monitoring Duration as "monDur" attribute;

- repetition period for periodic reporting as "repPeriod" attribute;

- immediate reporting indication as "immRep" attribute;

- sampling ratio as "sampRatio" attribute; and/or

- group reporting guard time as "grpRepTime" attribute.

The "eventFilter" shall include:

- identification of target UE(s) to which the subscription applies in the "tgtUe" attribute.

Depending on the event type:

- if the feature "ServiceExperience" is supported and the event is "SVC\_EXPERIENCE", the "eventFilter" attribute may provide:

1. identification of application to which the subscription applies via "appIds" attribute;
2. an area of interest via "locArea" attribute.

- if the feature "Exceptions" is supported and the event is "EXCEPTIONS", the "eventFilter" attribute may provide:

1) identification of application to which the subscription applies via "appIds" attribute;

Editor's note: Whether application identifier is mandatory is FFS.

Editor's note: Others Event Filter information for the feature "Exceptions" are FFS.

If the AF cannot successfully fulfil the received HTTP POST request due to the internal error or an error in the HTTP POST request, the AF shall send the HTTP error response as specified in subclause 5.7.

Upon successful reception of the HTTP POST request with "{apiRoot}/naf-eventexposure/{apiVersion}/subscriptions/" as request URI and "AfEventExposureSubsc" data structure as request body, the AF shall create a new "Individual Application Event Subscription" resource, shall store the subscription and shall send a HTTP "201 Created" response as shown in step 2 of figure 4.2.2.2-1. The AF shall include in the "201 Created" response:

- a Location header field; and

- an "AfEventExposureSubsc" data type in the payload body.

The Location header field shall contain the URI of the created individual application session context resource i.e. "{apiRoot}/naf-eventexposure/{apiVersion}/subscriptions/{subscriptionId}".

The "AfEventExposureSubsc" data type payload body shall contain the representation of the created "Individual Application Event Subscription".

When the "monDur" attribute is included in the response, it represents AF selected expiry time that is equal or less than the received expiry time in the request.

When the "immRep" attribute is included and sets to "true" in the subscription and the subscribed events are available, the AF shall immediately notify the NF service consumer using the Naf\_EventExposure\_Notify service operation, as described in subclause 4.2.4.2.

When the sampling ratio as the "sampRatio" attribute is included in the subscription, the AF shall select a random subset of UEs among target UEs according to the sampling ratio and only report the event(s) related to the selected subset UEs.

When the group reporting guard time as the "grpRepTime" attribute is included in the subscription, the AF shall accumulate all the event reports for the target UEs until the group reporting guard time expires. Then the AF shall notify the NF service consumer using the Naf\_EventExposure\_Notify service operation, as described in subclause 4.2.4.2.

\* \* \* Next Change \* \* \* \*

#### 5.6.2.5 Type EventFilter

Table 5.6.2.5-1: Definition of type EventFilter

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| gpsis | array(Gpsi) | O | 1..N | Each elements represents external UE identifier.  (NOTE 1, NOTE 2) |  |
| exterGroupIds | array(GroupId) | O | 1..N | Each element represents a group of UEs.  (NOTE 1, NOTE 2) |  |
| anyUeInd | boolean | O | 0..1 | Identifies whether the AF request applies to any UE.  This attribute shall set to "true" if applicable for any UE, otherwise, set to "false".  May only be present and sets to "true" if "AfEvent" sets to "SVC\_EXPERIENCE".  (NOTE 1) | ServiceExperience |
| appIds | array(ApplicationId) | O | 1..N | Each element indicates an application identifier.  Shall be present if "AfEvent" sets to "SVC\_EXPERIENCE" or "EXCEPTIONS".(NOTE 3) | ServiceExperience  Exceptions |
| locArea | LocationArea5G | O | 0..1 | Represents area of interest.  May only be present if "AfEvent" sets to "SVC\_EXPERIENCE". | ServiceExperience |
| NOTE 1: If "AfEvent" sets to "SVC\_EXPERIENCE", only one of the "gpsi", "exterGroupIds" or "anyUeInd" attributes shall be present.  NOTE 2: If "AfEvent" sets to "UeMobility" or "UeCommunication", either the "gpsis" or "exterGroupIds" attribute shall be present.  NOTE 3: For event "EXCEPTIONS", the "appIds" attribute shall include only one element. | | | | | |

\* \* \* Next Change \* \* \* \*

# A.2 Naf\_EventExposure API

openapi: 3.0.0

info:

version: 1.0.0.alpha-1

title: Naf\_EventExposure

description: |

AF Event Exposure Service.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.517 V0.5.0; 5G System; Application Function Event Exposure Service; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.517/

servers:

- url: '{apiRoot}/naf-eventexposure/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- naf-eventexposure

paths:

/subscriptions:

post:

summary: Creates a new Individual Application Event Exposure Subscription resource

operationId: PostAfEventExposureSubsc

tags:

- Application Event Subscription (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureSubsc'

responses:

'201':

description: Success

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureSubsc'

headers:

Location:

description: 'Contains the URI of the created individual application event subscription resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

AfEventExposureNotif:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureNotif'

responses:

'204':

description: No Content, Notification was succesfull

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

get:

summary: "Reads an existing Individual Application Event Subscription"

operationId: GetAfEventExposureSubsc

tags:

- Individual Application Event Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: Application Event Subscription ID

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureSubsc'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: "Modifies an existing Individual Application Event Subscription "

operationId: PutAfEventExposureSubsc

tags:

- Individual Application Event Subscription (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureSubsc'

parameters:

- name: subscriptionId

in: path

description: Application Event Subscription ID

required: true

schema:

type: string

responses:

'200':

description: OK. Resource was succesfully modified and representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/AfEventExposureSubsc'

'204':

description: No Content. Resource was succesfully modified

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: "Cancels an existing Individual Application Event Subscription "

operationId: DeleteAfEventExposureSubsc

tags:

- Individual Application Event Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: Application Event Subscription ID

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was succesfully deleted

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

naf-eventexposure: Access to the Naf\_EventExposure API.

schemas:

AfEventExposureNotif:

type: object

properties:

notifId:

type: string

eventNotifs:

type: array

items:

$ref: '#/components/schemas/AfEventNotification'

minItems: 1

required:

- notifId

- eventNotifs

AfEventExposureSubsc:

type: object

properties:

eventSubs:

type: array

items:

$ref: '#/components/schemas/EventsSubs'

minItems: 1

eventsRepInfo:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifId:

type: string

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- eventSubs

- eventsRepInfo

- notifId

- notifUri

- suppFeat

AfEventNotification:

type: object

properties:

event:

$ref: '#/components/schemas/AfEvent'

timeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

svcExprcInfos:

type: array

items:

$ref: '#/components/schemas/ServiceExperienceInfoPerApp'

minItems: 1

ueMobilityInfos:

type: array

items:

$ref: '#/components/schemas/UeMobilityCollection'

minItems: 1

ueCommInfos:

type: array

items:

$ref: '#/components/schemas/UeCommunicationCollection'

minItems: 1

excepInfos:

type: array

items:

$ref: '#/components/schemas/ExceptionInfo'

minItems: 1

required:

- event

- timeStamp

EventsSubs:

type: object

properties:

event:

$ref: '#/components/schemas/AfEvent'

eventFilter:

$ref: '#/components/schemas/EventFilter'

required:

- event

- eventFilter

EventFilter:

type: object

properties:

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

exterGroupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

anyUeInd:

type: string

appIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minItems: 1

locArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

ServiceExperienceInfoPerApp:

type: object

properties:

appId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

svcExpPerFlows:

type: array

items:

$ref: '#/components/schemas/ServiceExperienceInfoPerFlow'

minItems: 1

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

required:

- svcExpPerFlows

ServiceExperienceInfoPerFlow:

type: object

properties:

svcExprc:

$ref: '#/components/schemas/SvcExperience'

timeIntev:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

dnai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

ipTrafficFilter:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

ethTrafficFilter:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowDescription'

SvcExperience:

type: object

properties:

mos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

upperRange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

lowerRange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

UeMobilityCollection:

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

appId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

ueTrajs:

type: array

items:

$ref: '#/components/schemas/UeTrajectoryCollection'

minItems: 1

required:

- appId

- ueTrajs

UeCommunicationCollection:

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

appId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

comms:

type: array

items:

$ref: '#/components/schemas/CommunicationCollection'

minItems: 1

required:

- appId

- comms

UeTrajectoryCollection:

type: object

properties:

ts:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

locArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

required:

- ts

- locArea

CommunicationCollection:

type: object

properties:

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

ulVol:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

dlVol:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

required:

- startTime

- endTime

- ulVol

- dlVol

ExceptionInfo:

type: object

properties:

ipTrafficFilter:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

ethTrafficFilter:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/EthFlowDescription'

exceps:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/Exception'

minItems: 1

# Simple data types and Enumerations

AfEvent:

anyOf:

- type: string

enum:

- SVC\_EXPERIENCE

- UE\_MOBILITY

- UE\_COMM

- EXCEPTIONS

- type: string

\* \* \* End of Changes \* \* \* \*