**3GPP TSG-CT WG3 Meeting #108-eC3-201128**

**E-Meeting, 24th – 28th February 2020**

**Source: Huawei**

**Title: VAE\_DynamicGroup OpenAPI file**

**Spec: 29.486**

**Agenda item: 16.25**

**Document for: Decision**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

VAE\_DynamicGroup OpenAPI file shall be defined.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.486 V0.2.0.

\* \* \* First Change \* \* \* \*

## A.4 VAE\_DynamicGroup API

openapi: 3.0.0

info:

version: 1.0.0.alpha-1

title: VAE\_Dynamic\_Group

description: |

VAE\_Dynamic\_Group Service

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.486 V0.0.0 V2X Application Enabler (VAE) Services

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.486/'

security:

- {}

- oAuth2ClientCredentials: []servers:

- url: '{apiRoot}/vae-dynamic-group/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause clause 4.4 of 3GPP TS 29.501

paths:

/group-configurations:

post:

summary: VAE\_Dynamice\_Group resource create service Operation

tags:

- application requirements collection (Document)

operationId: CreateGroupConfiguration

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/GroupConfigurationData'

required: true

responses:

'201':

description: Application Requirement Resource Created

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/vae-group-configuration/v1/group-configurations/{configId}'

required: true

schema:

type: string

content:

application/json:

schema:

$ref: '#/components/schemas/GroupConfigurationData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

NotifyDynamicGroup:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DynamicGroupNotification'

responses:

'204':

description: No Content, Notification was succesfull

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/group-configuration/{configId}:

get:

summary: VAE Group Configuration resource read service Operation

tags:

- Individual Group Configuration(Document)

operationId: ReadDynamicGroupConfiguration

parameters:

- name: configId

in: path

description: Identifier of an group configuration resource

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/GroupConfigurationData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: VAE Group Configuration resource delete service Operation

tags:

- Individual group configuration (Document)

operationId: DeleteGroupConfiguration

parameters:

- name: configId

in: path

required: true

description: Unique ID of the group configuration to be deleted

schema:

type: string

responses:

'204':

description: The subscription was terminated successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

GroupConfigurationData:

type: object

properties:

groupId:

$ref: 'TS29486\_VAE\_MessageDelivery.yaml#/components/schemas/V2xGroupId'

definition:

type: string

leaderId:

$ref: 'TS29486\_VAE\_MessageDelivery.yaml#/components/schemas/V2xUeId'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

duration:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

requestTestNotification:

type: boolean

description: Set to true by the NF service consumer to request the VAE server to send a test notification as defined in clause 6.4.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- groupId

- defition

- leaderId

- notifUri

DynamicGroupNotification:

type: object

properties:

resourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

joinedUeIds:

type: array

items:

$ref: 'TS29486\_VAE\_MessageDelivery.yaml#/components/schemas/V2xUeId'

minItems: 1

leftUeIds:

type: array

items:

$ref: 'TS29486\_VAE\_MessageDelivery.yaml#/components/schemas/V2xUeId'

minItems: 1

required:

- resourceUri

\* \* \* End of Changes \* \* \* \*