**TSG-CT WG3 Meeting #111-e *C3-204324***

**E-Meeting, 19th – 28th August 2020 (Revision of C3-204205)**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **0208** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Resource correction |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eV2XARC |  | ***Date:*** | 2020-08-10 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In OpenAPI file of ServiceParameter API, the url part of servers field is ‘{apiRoot}/3gpp-service-parameter/v1’, which is inconsistent with the mainbody definition.Two alternative to solve the issue, 1. Change API name in the url part of servers field to 3gpp-serviceparameter to align with the mainbody definition;
2. Change API name in the main body definition to 3gpp-service-parameter to align with the OpenAPI file.

Since alternative 1 will introducd backward incompatible correction, alternative 2 is the solution goes forward. |
|  |  |
| ***Summary of change:*** | Change the API name in the main body definition to 3gpp-service-parameter to align with the OpenAPI file |
|  |  |
| ***Consequences if not approved:*** | Inconsistent API name definition. |
|  |  |
| ***Clauses affected:*** | 5.11.1.1; 5.11.1.2.2; 5.11.1.2.3.3; 5.11.1.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI file. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.11.1.1 Overview

All resource URIs of this API should have the following root:

**{apiRoot}/3gpp-service-parameter/v1/**

"apiRoot" is set as described in subclause 5.2.4 in 3GPP TS 29.122 [4]. "apiName" shall be set to "3gpp-service-parameter" and "apiVersion" shall be set to "v1" for the current version defined in the present document. All resource URIs in the subclauses below are defined relative to the above root URI.

This subclause describes the structure for the Resource URIs as shown in figure 5.11.1.1-1 and the resources and HTTP methods used for the ServiceParameter API.



Figure 5.9.1.1-1: Resource URI structure of the ServiceParameter API

Table 5.11.1.1-1 provides an overview of the resources and HTTP methods applicable for the ServiceParameter API.

Table 5.9.1.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Service Parameter Subscripions | {apiRoot}/3gpp-service-parameter/v1/{afId}/subscriptions | GET | Read all subscriptions for a given AF. |
| POST | Create a new service parameter subscription. |
| Individual Service Parameter Subscripion | {apiRoot}/3gpp-service-parameter/v1/{afId}/subscriptions/{subscriptionId} | GET | Read an existing subscription identified by {subscriptionId} |
| PUT | Modify all of the properties of an existing subscription. identified by {subscriptionId} |
| PATCH | Modify some of the properties of an existing subscription identified by {subscriptionId} |
| DELETE | Delete the subscription identified by {subscriptionId} |

\*\*\* Next Change \*\*\*

##### 5.11.1.2.2 Resource Definition

Resource URI: **{apiRoot}/3gpp-service-parameter/v1/{afId}/subscriptions**

This resource shall support the resource URI variables defined in table 5.11.1.2.2-1.

Table 5.11.1.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | Subclause 5.2.4 of 3GPP TS 29.122 [4]. |
| afId | string | Identifier of the AF. |

\*\*\* Next Change \*\*\*

###### 5.11.1.2.3.3 POST

The POST method creates a new resource to individual service parameter subscription for a given AF. The AF shall initiate the HTTP POST request message and the NEF shall respond to the message. The NEF shall construct the URI of the created resource.

This method shall support the request data structures specified in table 5.11.1.2.3.3-1 and the response data structures and response codes specified in table 5.11.1.2.3.3-2.

Table 5.11.1.2.3.3-1: Data structures supported by the POSTRequest Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| ServiceParameterData | M | 1 | Parameters to create a service parameter subscription resource. |

Table 5.11.1.2.3.3-2: Data structures supported by thePOST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| ServiceParameterData | M | 1 | 201 Created | The subscription resource was created successfully. The URI of the created resource shall be returned in the "Location" HTTP header. |
| n/a |  |  | 204 No Content | The subscription resource was created successfully. The URI of the created resource shall be returned in the "Location" HTTP header. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in table 5.2.6-1 of 3GPP TS 29.122 [4] also apply. |

Table 5.11.1.2.3.3-3: Headers supported by the 201 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/3gpp-service-parameter/v1/{afId}/subscriptions/{subscriptionId} |

\*\*\* Next Change \*\*\*

##### 5.11.1.3.2 Resource Definition

Resource URI: **{apiRoot}/3gpp-service-parameter/v1/{afId}/subscriptions/{subscriptionId}**

This resource shall support the resource URI variables defined in table 5.9.1.3.2-1.

Table 5.11.1.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | Subclause 5.2.4 of 3GPP TS 29.122 [4]. |
| afId | string | Identifier of the AF. |
| subscriptionId | string | Identifier of the subscription resource. |

\*\*\* End of Changes \*\*\*