**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Adding EAS IP replacement information in AppRelocationInfo |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | As specified in 23.501 5.6.7, 23.502 4.3.6.3, 23.503 6.3.1, 23.548 6.3.3.2, the AF can provide EAS (Edge Application Server) IP replacement information for the case of EAS relocation either in initial traffic influence requests (using Nnef\_TrafficInfluence\_Create/Update if untrusted or Npcf\_PolicyAuthorization\_Create/Update if trusted) or in its responses to Early/Late UP path change notifications of the SMF (in which the SMF may indicate its capability to support EAS IP replacement). |
|  |  |
| ***Summary of change:*** | Added EAS IP replacement support indication in EventNotification for UP path changes.Added the possibility to receive EAS IP replacement info in acknowledgements of the UP path change notifications.Extended the respective procedure descriptions and the OpenAPI accordingly.Added also the EAS abbreviation and corrected the example consumers of AppRelocationInfo (in 4.2.1, introduced in Rel-17). |
|  |  |
| ***Consequences if not approved:*** |  Stage 2 requirements not fulfilled. |
|  |  |
| ***Clauses affected:*** | 3.2, 4.2.1, 4.2.2.2, 4.2.5.2, 5.6.2.5, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces a backwards compatible feature in the Nsmf\_EventExposure OpenAPI |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First change \* \* \* \*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

AF Application Function

AMBR Aggregate Maximum Bit Rate

AMF Access and Mobility Management Function

API Application Programming Interface

DDD Downlink Data Delivery

DNAI DN Access Identifier

DNN Data Network Name

EAS Edge Application Server

FQDN Fully Qualified Domain Name

GPSI Generic Public Subscription Identifier

GUAMI Globally Unique AMF Identifier

HTTP Hypertext Transfer Protocol

H-SMF Home SMF

I-SMF Intermediate SMF

JSON JavaScript Object Notation

NEF Network Exposure Function

NF Network Function

NRF Network Repository Function

NSSAI Network Slice Selection Assistance Information

NWDAF Network Data Analytics Function

SMF Session Management Function

SUPI Subscription Permanent Identifier

S-NSSAI Single Network Slice Selection Assistance Information

PCF Policy Control Function

PRA Presence Reporting Area

QFI QoS Flow Identifier

UDM Unified Data Management

UPF User Plane Function

V-SMF Visited SMF

\* \* \* \* Next change \* \* \* \*

### 4.2.1 Introduction

Table 4.2.1-1: Operations of the Nsmf\_EventExposure Service

| Service operation name | Description | Initiated by |
| --- | --- | --- |
| Notify | Report UE PDU session related event(s) to the NF service consumer which has subscribed to the event report service. | (H-)SMF, V-SMF, I-SMF |
| Subscribe | This service operation is used by an NF service consumer to subscribe for event notifications on a specified PDU session, or for all PDU Sessions of one UE, a group of UE(s) or any UE, or to modify a subscription. | NF service consumers (e.g. AMF, NEF, AF, UDM, NWDAF) |
| UnSubscribe | This service operation is used by an NF service consumer to unsubscribe from event notifications. | NF service consumers (e.g. AMF, NEF, AF, UDM, NWDAF) |
| AppRelocationInfo | This service operation is used by an NF service consumer to acknowledge the notification from the SMF regarding UE PDU Session related event(s) | NF service consumers (e.g. NEF, AF) |

\* \* \* \* Next change \* \* \* \*

#### 4.2.2.2 Notification about subscribed events

The present "notification about subscribed events" procedure is performed by the SMF when any of the subscribed events occur.

The following applies with respect to the detection of subscribed events:

- If:

- the SMF supports the "downlink data delivery status" feature,

- the event "downlink data delivery status" is subscribed,

- the traffic descriptors of the downlink data source have been provided for that subscription, and

- the SMF is informed that the UE corresponding to that subscription is unreachable,

- if the data is buffered at the UPF, then the SMF shall interact with the UPF to notify that the UPF buffers the downlink packets. The SMF shall include the traffic descriptor of the subscriptions in the PDR with a higher priority if the PCC is not applied to the PDUsession or derive the PDR from the PCC rule received from the PCF as defined in subclause 4.2.4.27 of 3GPP TS 29.512 [14] if the PCC is applied to the PDU session and request the UPF to report when there are corresponding buffered downlink packets or discarded packets in the UPF as defined in subclause 5.28.1 of 3GPP TS 29.244 [23]. When receiving the report from the UPF, the SMF shall determine whether that subscribed event with delivery status "DISCARDED" or "BUFFERED" occurred. The SMF shall determine that subscribed event with delivery status "TRANSMITTED" occurred by the fact that the related PDU session becomes ACTIVE.

- if the data is buffered at the SMF, the SMF shall determine whether that subscribed event occurred by comparing the downlink packets with the traffic descriptors received in the corresponding event subscription. If the SMF decides to buffer the packets, the subscribed event with delivery status "BUFFERED" occurred. If the SMF decides to discard the packets, the subscribed event with delivery status "DISCARDED" occurred. The SMF shall determine that subscribed event with delivery status "TRANSMITTED" occurred by the fact that the related PDU session becomes ACTIVE.

Figure 4.2.2.2-1 illustrates the notification about subscribed events.



Figure 4.2.2.2-1: Notification about subscribed events

If the SMF observes PDU Session related event(s) for which an NF service consumer has subscribed, the SMF shall send an HTTP POST request with "{notifUri}", as previously provided by the NF service consumer within the corresponding subscription, as URI and NsmfEventExposureNotification data structure as request body that shall include:

- Notification correlation ID provided by the NF service consumer during the subscription, or as provided by the PCF for implicit subscription of UP path change as defined in subclause 4.2.6.2.6.2 of 3GPP TS 29.512 [14], or as provided by the PCF for implicit subscription of QoS Monitoring as defined in subclause 4.2.3.25 of 3GPP TS 29.512 [14], as "notifId" attribute; and

- information about the observed event(s) within the "eventNotifs" attribute that shall contain for each observed event an "EventNotification" data structure that shall include:

1. the Event Trigger as "event" attribute;

2. for a UP path change notification:

a) type of notification ("EARLY" or "LATE") as "dnaiChgType" attribute;

b) source DNAI and/or target DNAI as "sourceDnai" attribute and "targetDnai" attribute if DNAI is changed, respectively (NOTE 3); and

c) if the PDU Session type is IP, for the source DNAI IP address/prefix of the UE as "sourceUeIpv4Addr" attribute or "sourceUeIpv6Prefix" attribute; and

d) if the PDU Session type is IP, for the target DNAI IP address/prefix of the UE as "targetUeIpv4Addr" attribute or "targetUeIpv6Prefix" attribute;

e) if available (NOTE 3), for the source DNAI, N6 traffic routing information related to the UE as "sourceTraRouting" attribute;

f) if available (NOTE 3), for the target DNAI, N6 traffic routing information related to the UE as "targetTraRouting" attribute;

g) if the PDU Session type is Ethernet, the MAC address of the UE in the "ueMac" attribute; and

x) optionally an indication of the capability of supporting EAS IP replacement in 5GC in the "easIpReplSupport" attribute, if the "EnEDGE" feature is supported;

NOTE 1: UP path change notification, i.e. DNAI change notification and/or N6 traffic routing information change notification, can be the result of an implicit subscription of the PCF on behalf of the NEF/AF as part of setting PCC rule(s) via the Npcf\_SMPolicyControl service (see subclause 4.2.6.2.6.2 of 3GPP TS 29.512 [14]).

NOTE 2: If the DNAI is not changed while the N6 traffic routing information change, the source DNAI and target DNAI are not provided.

NOTE 3: The change from the UP path status where no DNAI applies to a status where a DNAI applies indicates the activation of the related AF request and therefore only the target DNAI and N6 traffic routing information is provided in the event notification; the change from the UP path status where a DNAI applies to a status where no DNAI applies indicates the de-activation of the related AF request and therefore only the source DNAI and N6 traffic routing information is provided in the event notification.

3. for a UE IP address change:

a) added new UE IP address or prefix as "adIpv4Addr" attribute or "adIpv6Prefix" attribute, respectively; and/or

b) released UE IP address or prefix as "reIpv4Addr" attribute or "reIpv6Prefix" attribute, respectively;

4. for an access type change:

a) new access type as "accType" attribute;

5. for a PLMN Change:

a) new PLMN as "plmnId" attribute;

6. for a PDU Session Release:

a) ID of the released PDU session as "pduSeId" attribute;

b) DNN of the release PDU session as "dnn" attribute, if the "PduSessionStatus" feature is supported;

c) The type of the release PDU session as "pduSessType" attribute, if the "PduSessionStatus" feature is supported; and

d) UE IPv4 address as "ipv4Addr" attribute and/or IPv6 information (IPv6 prefix(es) or IPv6 address(es)) as "ipv6Prefixes" or "ipv6Addrs" attributes, if the released PDU session type is IP and the "PduSessionStatus" feature is supported;

7. the time at which the event was observed encoded as "timeStamp" attribute;

8. the SUPI as the "supi" attribute if the subscription applies to a group of UE(s) or any UE;

9. if available, the GPSI as the "gpsi" attribute if the subscription applies to a group of UE(s) or any UE;

10. for a Downlink Data Delivery Status:

a) the downlink data delivery status as "dddStatus" attribute;

b) the downlink data descriptors impacted by the downlink data delivery status change within the "dddTraDescriptor" attribute; and

c) for downlink data delivery status "BUFFERED". the estimated maximum waiting time as "maxWaitTime" attribute;

11. for a Communication Failure:

a) the detailed communication failure information (e.g. 5G SM cause) as "commFailure" attribute; and

12. for QoS Monitoring:

a) one or two uplink packet delays within the "ulDelays" attribute; or

b) one or two downlink packet delays within the "dlDelays" attribute; or

c) one or two round trip packet delays within the "rtDelays" attribute.

NOTE 4: QoS Monitoring notification can be the result of an implicit subscription of the PCF on behalf of the NEF/AF as part of setting PCC rule(s) via the Npcf\_SMPolicyControl service (see subclause 4.2.3.25 of 3GPP TS 29.512 [14]).

13. for a PDU Session Establishment, if the "PduSessionStatus" feature is supported:

a) ID of the established PDU session as "pduSeId" attribute;

b) DNN of the release PDU session as "dnn" attribute;

c) The type of the release PDU session as "pduSessType" attribute; and

d) UE IPv4 address as "ipv4Addr" attribute and/or IPv6 information (IPv6 prefix(es) or IPv6 address(es)) as "ipv6Prefixes" or "ipv6Addrs" attributes if available at PDU session establishment;

14. for a QFI allocation:

a) QFI of the allocated QoS Flow ID for the application as "qfi" attribute;

b) DNN of the allocated PDU session as "dnn" attribute;

c) Slice of the allocated PDU session as "snssai" attribute;

d) The description of the application traffic as "appId", "fDescs" or "ethfDescs" attribute; and

e) ID of the allocated PDU session as "pduSeId" attribute if the subscription was for a UE, a group of UEs, or any UE, and not for a specific PDU Session;

15. for an RAT type change:

a) new RAT type as "ratType" attribute;

- an URI for further AF acknowledgement in the "ackUri" attribute if the SMF determines to wait for the AF acknowledgement before activating the new UP path associated with the new DNAI.

NOTE 5: Based on the indication of AF acknowledgment to be expected in the PCC rules received from the PCF and local configuration, the SMF may determine to wait for the AF acknowledgement before activating the new UP path associated with the new DNAI.

Upon the reception of an HTTP POST request with "{notifUri}" as URI and an NsmfEventExposureNotification data structure as request body, the NF service consumer shall send an HTTP "204 No Content" response for a successful processing.

If errors occur when processing the HTTP POST request, the NF service consumer shall send the HTTP error response as specified in subclause 5.7.

If the feature "ES3XX" is not supported and,

- if the NF service consumer is not able to handle the Notification but another unknown NF service consumer could possibly handle the notification, it shall reply with an HTTP "404 Not found" error response.

NOTE 6: An AMF as NF service consumer can change.

- if the SMF becomes aware that a new NF service consumer is requiring notifications (e.g. via the "404 Not found" response, or via Namf\_Communication service AMFStatusChange Notifications, see 3GPP TS 29.518 [13], or via link level failures or via the Nnrf\_NFDiscovery Service (using the service name and GUAMI obtained during the creation of the subscription) to discover the other AMFs within the AMF set) specified in 3GPP TS 29.510 [12]), and the SMF knows alternate or backup IPv4 Address(es), IPv6 Address(es) or FQDN(s) where to send Notifications (e.g. via "altNotifIpv4Addrs", "altNotifIpv6Addrs" or "altNotifFqdns" attributes received when the subscription was created), the SMF shall exchange the authority part of the Notification URI with one of those addresses and shall use that URI in any subsequent communication. If the SMF received a "404 Not found" response, the SMF should resend the failed notification to that URI.

If the feature "ES3XX" is supported, and the NF service consumer determines the received HTTP POST request needs to be redirected, the NF service consumer shall send an HTTP redirect response as specified in subclause 6.10.9 of 3GPP TS 29.500 [4] and,

- if the SMF receives a "307 Temporary Redirect" response, the SMF shall resend the failed event notification request using the received URI in the Location header field as Notification URI. Subsequent event notifications, triggered after the failed one, shall be sent to the Notification URI provided by the NF service consumer during the corresponding subscription creation/update; or

- if the SMF receives a "308 Permanent Redirect" response, the SMF shall resend the failed event notification request and send the subsequent event notification using the received URI in the Location header field as Notification URI.

If the SMF in the VPLMN needs to send an event notification to the NEF in the HPLMN, it may normalize the event based on roaming agreements when required before provisioning the event report to the NEF of the HPLMN.

\* \* \* \* Next change \* \* \* \*

#### 4.2.5.2 Acknowledgement of Notification about subscribed events

Figure 4.2.5.2-1 illustrates the acknowledgement of notification about subscribed events.



Figure 4.2.5.2-1: Acknowledgement of Notification about subscribed events

In order to acknowledge the SMF of the application relocation information after the handling of a notification about UP path change event, an NF service consumer shall send an HTTP POST request to the callback URI "{ackUri}" as previously provided by the SMF in an attribute within the NsmfEventExposureNotification data during UP path change notification procedure as defined in subclause  4.2.2.2.

The request body contains the AckOfNotify data structure that shall include:

- Notification correlation ID provided by the NF service consumer during UP path change notification, as "notifId" attribute;

- an identifier of UE (i.e. SUPI or GPSI), if available and the subscription does not applies to a group of UE(s) or any UE; and

- information about the AF acknowledgement within the "ackResult" attribute that shall contain result status of the application relocation as "afStatus" attribute. If the "afStatus" attribute sets to "SUCCESS", the N6 traffic routing information associated to the target DNAI may be included as "trafficRoute" attribute and, if the "EnEDGE" feature is supported, an indication that buffering of uplink traffic to the target DNAI is needed may be included as "upBuffInd" attribute and EAS IP replacement information may be included as "easIpReplaceInfos" attribute. If the application relocation is not completed on time, the "afStatus" attribute shall set to the corresponding failure cause.

Upon the reception of an HTTP POST request with AckOfNotify data structure as request body, the SMF shall send an HTTP "204 No Content" response for a succesfull processing.

If errors occur when processing the HTTP POST request, the SMF shall send an HTTP error response as specified in subclause 5.7.

If the feature "ES3XX" is supported, and the SMF determines the received HTTP POST request needs to be redirected, the SMF shall send an HTTP redirect response as specified in subclause 6.10.9 of 3GPP TS 29.500 [4].

\* \* \* \* Next change \* \* \* \*

#### 5.6.2.5 Type EventNotification

Table 5.6.2.5-1: Definition of type EventNotification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| event | SmfEvent | M | 1 | Event that is notified. |  |
| timeStamp | DateTime | M | 1 | Time at which the event is observed. |  |
| supi | Supi | C | 0..1 | Subscription Permanent Identifier. It is included when the subscription applies to a group of UE(s) or any UE. |  |
| gpsi | Gpsi | C | 0..1 | Identifies a GPSI. It shall contain an MSISDN. It is included when it is available and the subscription applies to a group of UE(s) or any UE. |  |
| sourceDnai | Dnai | C | 0..1 | Source DN Access Identifier. Shall be included for event "UP\_PATH\_CH" if the DNAI changed (NOTE 1, NOTE 2). |  |
| targetDnai | Dnai | C | 0..1 | Target DN Access Identifier. Shall be included for event "UP\_PATH\_CH" if the DNAI changed (NOTE 1, NOTE 2). |  |
| dnaiChgType | DnaiChangeType | C | 0..1 | DNAI Change Type. Shall be included for event "UP\_PATH\_CH". |  |
| sourceUeIpv4Addr | Ipv4Addr | O | 0..1 | The IPv4 Address of the served UE for the source DNAI. May be included for event "UP\_PATH\_CH". |  |
| sourceUeIpv6Prefix | Ipv6Prefix | O | 0..1 | The Ipv6 Address Prefix of the served UE for the source DNAI. May be included for event "UP\_PATH\_CH". |  |
| targetUeIpv4Addr | Ipv4Addr | O | 0..1 | The IPv4 Address of the served UE for the target DNAI. May be included for event "UP\_PATH\_CH". |  |
| targetUeIpv6Prefix | Ipv6Prefix | O | 0..1 | The Ipv6 Address Prefix of the served UE for the target DNAI. May be included for event "UP\_PATH\_CH". |  |
| sourceTraRouting | RouteToLocation | C | 0..1 | N6 traffic routing information for the source DNAI. Shall be included for event "UP\_PATH\_CH" if available (NOTE 2). |  |
| targetTraRouting | RouteToLocation | C | 0..1 | N6 traffic routing information for the target DNAI. Shall be included for event "UP\_PATH\_CH" if available (NOTE 2). |  |
| easIpReplSupport | boolean | O | 0..1 | Indicates the capability of supporting EAS IP replacement in 5GC. If "true" then EAS IP replacement is supported. Default value is "false". | EnEDGE |
| ueMac | MacAddr48 | O | 0..1 | UE MAC address. May be included for event "UP\_PATH\_CH". |  |
| adIpv4Addr | Ipv4Addr | O | 0..1 | Added IPv4 Address(es). May be included for event "UE\_IP\_CH". |  |
| adIpv6Prefix | Ipv6Prefix | O | 0..1 | Added Ipv6 Address Prefix(es). May be included for event "UE\_IP\_CH". |  |
| reIpv4Addr | Ipv4Addr | O | 0..1 | Removed IPv4 Address(es). May be included for event "UE\_IP\_CH". |  |
| reIpv6Prefix | Ipv6Prefix | O | 0..1 | Removed Ipv6 Address Prefix(es). May be included for event "UE\_IP\_CH". |  |
| plmnId | PlmnId | C | 0..1 | New PLMN ID. Shall be included for event "PLMN\_CH". |  |
| accType | AccessType | C | 0..1 | New Access Type. Shall be included for event "AC\_TY\_CH". |  |
| pduSeId | PduSessionId | C | 0..1 | PDU session ID. Shall be included for event "PDU\_SES\_REL" and "PDU\_SES\_EST". It shall also be included for event "QFI\_ALLOC" if the subscription was for a UE, a group of UEs, or any UE, and not for a specific PDU Session. |  |
| ratType | RatType | C | 0..1 | New RAT Type. Shall be included for event ‘RAT\_TY\_CH’. | EneNA |
| dddStatus | DlDataDeliveryStatus | C | 0..1 | Downlink data delivery status (discarded, transmitted, buffered). Shall be included for event "downlink data delivery status", | DownlinkDataDeliveryStatus |
| maxWaitTime | DateTime | C | 0..1 | The estimated maximum waiting time for downlink data delivery, Shall be included for event "downlink data delivery status" with status "BUFFERED". | DownlinkDataDeliveryStatus |
| dddTraDescriptor | DddTrafficDescriptor | C | 0..1 | The downlink data descriptor impacted by downlink data delivery status change. Shall be included for event "downlink data delivery status" | DownlinkDataDeliveryStatus |
| commFailure | CommunicationFailure | C | 0..1 | Describes the communication failure cause for the UE. Shall be included for event "COMM\_FAIL". | CommunicationFailure |
| ipv4Addr | Ipv4Addr | O | 0..1 | IPv4 address. May be included for event "PDU\_SES\_REL" or "PDU\_SES\_EST". | PduSessionStatus |
| ipv6Prefixes | array(Ipv6Prefix) | O | 1..N | IPv6 prefixes. May be included for event "PDU\_SES\_REL" or "PDU\_SES\_EST". (NOTE 3) | PduSessionStatus |
| ipv6Addrs | array(Ipv6Addr) | O | 1..N | IPv6 addresses. May be included for event "PDU\_SES\_REL" or "PDU\_SES\_EST". (NOTE 3) | PduSessionStatus |
| pduSessType | PduSessionType | C | 0..1 | PDU session type. Shall be included if the PduSessionStatus feature is supported. | PduSessionStatus |
| qfi | Qfi | C | 0..1 | QoS flow identifier. Shall be included for event "QFI\_ALLOC". | QfiAllocation |
| appId | ApplicationId | O | 0..1 | Contains the application identifier. May be included for event "QFI\_ALLOC". (NOTE 4) | QfiAllocation |
| ethfDescs | array(EthFlowDescription) | O | 1..2 | Contains the flow description for the Uplink and/or Downlink Ethernet flows. May be included for event "QFI\_ALLOC". (NOTE 4) | QfiAllocation |
| fDescs | array(FlowDescription) | O | 1..2 | Contains the flow description for the Uplink and/or Downlink IP flows. May be included for event "QFI\_ALLOC". (NOTE 4) | QfiAllocation |
| dnn | Dnn | C | 0..1 | Data network name, Shall be included for event "QFI\_ALLOC". May be included for event "PDU\_SES\_REL" or "PDU\_SES\_EST". | QfiAllocation, PduSessionStatus |
| snssai | Snssai | C | 0..1 | Identifies the slice information. Shall be included for event "QFI\_ALLOC". | QfiAllocation |
| ulDelays | array(Uinteger) | O | 1..N | Uplink packet delay in units of milliseconds. (NOTE 5) | QoSMonitoring |
| dlDelays | array(Uinteger) | O | 1..N | Downlink packet delay in units of milliseconds. (NOTE 5) | QoSMonitoring |
| rtDelays | array(Uinteger) | O | 1..N | Round trip delay in units of milliseconds. (NOTE 5) | QoSMonitoring |
| NOTE 1: If the DNAI is not changed while the N6 traffic routing information is changed, the "sourceDnai" attribute and "targetDnai" attribute shall not be provided.NOTE 2: The change from the UP path status where no DNAI applies to a status where a DNAI applies indicates the activation of the related AF request and therefore only the target DNAI and N6 traffic routing information is provided in the event notification; the change from the UP path status where a DNAI applies to a status where no DNAI applies indicates the de-activation of the related AF request and therefore only the source DNAI and N6 traffic routing information is provided in the event notification. NOTE 3: If provided, either ipv6Prefixes or ipv6Addrs shall be present. NOTE 4: Only one of the appId, ethfDescs or fDescs shall be provided. NOTE 5: In this release of the specification the maximum number of elements in the array is 2. If more than one value is received at one given point of time for UL packet delay, DL packet delay or round trip packet delay respectively, the SMF reports the minimum and maximum packet delays to the NEF/AF. |

\* \* \* \* Next change \* \* \* \*

# A.2 Nsmf\_EventExposure API

openapi: 3.0.0

info:

 version: 1.2.0-alpha.3

 title: Nsmf\_EventExposure

 description: |

 Session Management Event Exposure Service.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.508 V17.4.0; 5G System; Session Management Event Exposure Service.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.508/

servers:

 - url: '{apiRoot}/nsmf\_event-exposure/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - nsmf-event-exposure

paths:

 /subscriptions:

 post:

 operationId: CreateIndividualSubcription

 summary: Create an individual subscription for event notifications from the SMF

 tags:

 - Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 responses:

 '201':

 description: Created.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nsmf-event-exposure/v1/subscriptions/{subId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposureNotification'

 responses:

 '204':

 description: No Content, Notification was successful.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 afAcknowledgement:

 '{request.body#/ackUri}':

 post:

 requestBody: # contents of the callback message

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AckOfNotify'

 responses:

 '204':

 description: No Content (successful acknowledgement)

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subId}:

 get:

 operationId: GetIndividualSubcription

 summary: Read an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 operationId: ReplaceIndividualSubcription

 summary: Replace an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was successfully modified and representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '204':

 description: No Content. Resource was successfully modified

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualSubcription

 summary: Delete an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nsmf-event-exposure: Access to the Nsmf\_EventExposure API

 schemas:

 NsmfEventExposure:

 description: Represents an Individual SMF Notification Subscription resource. The serviveName property corresponds to the serviceName in the main body of the specification.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 anyUeInd:

 type: boolean

 description: Any UE indication. This IE shall be present if the event subscription is applicable to any UE. Default value "false" is used, if not present.

 groupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 pduSeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 subId:

 $ref: '#/components/schemas/SubId'

 notifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 description: Alternate or backup IPv4 address(es) where to send Notifications.

 minItems: 1

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 description: Alternate or backup IPv6 address(es) where to send Notifications.

 minItems: 1

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 eventSubs:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 ImmeRep:

 type: boolean

 notifMethod:

 $ref: '#/components/schemas/NotificationMethod'

 maxReportNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 serviveName:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 partitionCriteria:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PartitioningCriteria'

 minItems: 1

 description: Criteria for partitioning the UEs before applying the sampling ratio.

 grpRepTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 notifFlag:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NotificationFlag'

 required:

 - notifId

 - notifUri

 - eventSubs

 NsmfEventExposureNotification:

 description: Represents notifications on events that occurred.

 type: object

 properties:

 notifId:

 type: string

 description: Notification correlation ID

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 ackUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - notifId

 - eventNotifs

 EventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/SmfEvent'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 dddTraDescriptors:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 minItems: 1

 dddStati:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 required:

 - event

 EventNotification:

 description: Represents a notification related to a single event that occurred.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/SmfEvent'

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 sourceDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 targetDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 sourceUeIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 sourceUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 targetUeIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 targetUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 sourceTraRouting:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 targetTraRouting:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 easIpReplSupport:

 type: boolean

 description: Indicates the capability of supporting EAS IP replacement in 5GC.

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 adIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 adIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 reIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 reIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 accType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 pduSeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dddStatus:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 dddTraDescriptor:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 maxWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 commFailure:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CommunicationFailure'

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Prefixes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 pduSessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 qfi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ethfDescs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 fDescs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ulDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 dlDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 rtDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 required:

 - event

 - timeStamp

 SubId:

 type: string

 format: SubId

 description: Identifies an Individual SMF Notification Subscription. To enable that the value is used as part of a URI, the string shall only contain characters allowed according to the "lower-with-hyphen" naming convention defined in 3GPP TS 29.501. In an OpenAPI schema, the format shall be designated as "SubId".

 AckOfNotify:

 description: Represents an acknowledgement information of an event notification.

 type: object

 properties:

 notifId:

 type: string

 ackResult:

 $ref: 'TS29522\_TrafficInfluence.yaml#/components/schemas/AfResultInfo'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 required:

 - notifId

 - ackResult

 SmfEvent:

 anyOf:

 - type: string

 enum:

 - AC\_TY\_CH

 - UP\_PATH\_CH

 - PDU\_SES\_REL

 - PLMN\_CH

 - UE\_IP\_CH

 - RAT\_TY\_CH

 - DDDS

 - COMM\_FAIL

 - PDU\_SES\_EST

 - QFI\_ALLOC

 - QOS\_MON

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - AC\_TY\_CH: Access Type Change

 - UP\_PATH\_CH: UP Path Change

 - PDU\_SES\_REL: PDU Session Release

 - PLMN\_CH: PLMN Change

 - UE\_IP\_CH: UE IP address change

 - RAT\_TY\_CH: RAT Type Change

 - DDDS: Downlink data delivery status

 - COMM\_FAIL: Communication Failure

 - PDU\_SES\_EST: PDU Session Establishment

 - QFI\_ALLOC: QFI allocation

 - QOS\_MON: QoS Monitoring

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - ONE\_TIME

 - ON\_EVENT\_DETECTION

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PERIODIC

 - ONE\_TIME

 - ON\_EVENT\_DETECTION

\* \* \* \* End of changes \* \* \* \*