**3GPP TSG-CT3 Meeting #119e C3-216249**

**E-Meeting, 11th – 19th November 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.514** | **CR** | **0368** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | AF Request for Simultaneous Connectivity over Source and Target PSA at Edge Relocation |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eEDGE\_5GC |  | ***Date:*** | 2021-11-11 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature)****C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | AF may influence that certain traffic is redirected through a certain UL CL/BP and PSA, however it is unspecified how the relocation procedure happens, i.e., whether simultaneous connectivity should be temporarily maintained for source and target PSAs. SA2 agreed that the AF could indicate to the 5GC that the re-anchoring procedure should provide simultaneous connectivity over the source and the target PSA temporarily, where the AF could also indicate this temporality as the minimum time interval to be considered for inactivity for the concerned traffic. |
|  |  |
| ***Summary of change:*** | * Include a new indication “simConnInd” within the traffic routing requirements which when set to true indicates that simmultaneous connectivity should be temporarily maintained for source and target PSA during the re-anchoring procedure.
* Include a new duration related attribute “simConnTerm”, that indicates the minimum time interval to be considered for inactivity for the traffic routed via the source PSA before the simultaneous connectivity is terminated and the source PSA is removed.
 |
| ***U*** |  |
| ***Consequences if not approved:*** | The edge relocation feature specified in TS 23.548 is not fully implemented. |
|  |  |
| ***Clauses affected:*** | 3.2, 4.2.2.8, 4.2.3.8, 5.6.1, 5.6.2.13, 5.6.2.24, 5.8, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR impacts the OpenAPI file with a backwards compatible feature. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5G-RG 5G Residential Gateway

AF Application Function

ARP Allocation and Retention Priority

ATSSS Access Traffic Steering, Switching and Splitting

BBF Broadband Forum

BSSID Basic Service Set IDentifier

CHEM Coverage and Handoff Enhancements using Multimedia error robustness feature

CHF Charging Function

DEI Drop Eligible Indicator

DNAI DN Access Identifier

DNN Data Network Name

DS-TT Device-side TSN translator

DSL Digital Subscriber Line

DTS Data Transport Service

E-UTRA Evolved Universal Terrestrial Radio Access

FLUS Framework for Live Uplink Streaming

FN-RG Fixed Network Residential Gateway

GEO Geosynchronous Orbit

GPSI Generic Public Subscription Identifier

HFC Hybrid Fiber-Coaxial

H-PCF PCF in the HPLMN

IMS IP-Multimedia Subsystem

JSON JavaScript Object Notation

LEO Low Earth Orbit

MA Multi-Access

MCPTT Mission Critical Push to Talk Service

MCVideo Mission Critical Video

MEO Medium Earth Orbit

MPS Multimedia Priority Service

NEF Network Exposure Function

NID Network Identifier

NR New Radio

NRF Network Repository Function

NWDAF Network Data Analytics Function

NW-TT Network-side TSN translator

PCC Policy and Charging Control

PCF Policy Control Function

PCP Priority Code Point

P-CSCF Proxy Call Session Control Function

PEI Permanent Equipment Identifier

PMIC Port Management Information Container

PON Passive Optical Network

PRA Presence Reporting Area

PSA PDU Session Anchor

QoS Quality of Service

RFSP RAT Frequency Selection Priority

RTCP Real Time Control Protocol

RTP Real Time Protocol

SDF Service Data Flow

SDP Session Description Protocol

SIP Session Initiation Protocol

SMF Session Management Function

S-NSSAI Single Network Slice Selection Assistance Information

SNPN Stand-alone Non-Public Network

SSID Service Set IDentifier

SUPI Subscription Permanent Identifier

TNAP Trusted Non-3GPP Access Point

TSC Time Sensitive Communication

TSCAI Time Sensitive Communication Assistance Information

TSCTSF Time Sensitive Communication and Time Synchronization Function

TSN Time Sensitive Networking

UDR Unified Data Repository

UMIC User plane node Management Information Container

UPF User Plane Function

URSP UE Route Selection Policy

VID VLAN Identifier

VLAN Virtual Local Area Network

V-PCF PCF in the VPLMN

W-5GAN Wireline 5G Access Network

W-5GBAN Wireline 5G BBF Access Network

W-5GCAN Wireline 5G Cable Access Network

W-AGF Wireline Access Gateway Function

\*\*\* 2nd Change \*\*\*

#### 4.2.2.8 Initial provisioning of traffic routing information

This procedure is used by a NF service consumer to:

- influence SMF traffic routing decisions to a local access to a Data Network identified by a DNAI; and/or

- request subscriptions to notifications about UP path management events related to the PDU session,

when "InfluenceOnTrafficRouting" feature is supported.

NOTE 1: The NF service consumer uses the Npcf\_PolicyAuthorization service for requests targeting specific on-going PDU sessions of individual UE(s). The NF service consumer requests that target existing or future PDU Sessions of multiple UE(s) or any UE are sent via the NEF and may target multiple PCF(s), as described in 3GPP TS 29.513 [7].

The NF service consumer shall include in the HTTP POST request message described in subclause 4.2.2.2 the "afRoutReq" attribute of "AfRoutingRequirement" data type with specific routing requirements for the application traffic flows either within "AppSessionContextReqData" data type for the service indicated in the "afAppId" attribute, or within the "medComponents" attribute. When provided at both levels, the "afRoutReq" attribute value in the "medComponents" attribute shall have precedence over the "afRoutReq" attribute included in the "AppSessionContextReqData" data type.

The NF service consumer may include traffic routing requirements together with service information.

The NF service consumer may request to influence SMF traffic routing decisions to a DNAI. The NF service consumer shall include in the "afRoutReq" attribute:

a) A list of routes to locations of applications in the "routeToLocs" attribute. Each element of the list shall contain:

- a DNAI in the "dnai" attribute to indicate the location of the application towards which the traffic routing is applied; and

- either a routing profile identifier in the "routeProfId" attribute, or the explicit routing information in the "routeInfo" attribute.

The NF service consumer may include in the "afRoutReq" attribute:

a) Indication of application relocation possibility in the "appReloc" attribute.

b) Temporal validity during which the NF service consumer request is valid shall be indicated with the "startTime" and "stopTime" attributes.

c) Spatial validity during which the NF service consumer request is valid shall be indicated in terms of validity areas encoded in the "spVal" attribute of "SpatialValidity" data type. The "SpatialValidity" data type consists of a list of presence areas included in the "presenceInfoList" attribute, where each element shall include the presence reporting area identifier in the "praId" attribute and may include the elements composing a presence area encoded in the attributes: "trackingAreaList", "ecgList", "ncgList", "globalRanNodeIdList".

d) Indication of UE IP address preservation in the "addrPreserInd" attribute if the URLLC feature is supported.

e) If the EnEDGE feature is supported:

- indication of simultaneous connectivity temporarily maintained in the source and target PSA during the edge re-location procedure in the "simConnInd" attribute; and

- if the "simConnInd" attribute is set to true, the minimum time interval to be considered for inactivity of the traffic routed via the source PSA in the "simConnTerm" attribute.

The NF service consumer may also subscribe to notifications about UP path management events. The NF service consumer shall include in the "upPathChgSub" attribute:

- notifications of early and/or late DNAI change, using the attribute "dnaiChgType" indicating whether the subscription is for "EARLY", "LATE" or "EARLY\_LATE";

- the notification URI where the NF service consumer is receiving the Nsmf\_EventExposure\_Notify service operation in the "notificationUri" attribute; and

- the notification correlation identifier assigned by the NF service consumer in the "notifCorreId" attribute.

If the URLLC feature is supported, the NF service consumer may include an indication of NF service consumer acknowledgement to be expected as an "afAckInd" attribute within the "upPathChgSub" attribute.

When the feature "RoutingReqOutcome" is supported:

- the PCF may set the "servAuthInfo" attribute in the HTTP response message to "ROUT\_REQ\_NOT\_AUTHORIZED" when the PCF determines, e.g. based on subscription, the AF influence on traffic routing is not allowed for the PDU session;

- when the NF service consumer requests the steering of traffic to a DNAI and/or the subscription to notifications about UP path management events, the NF service consumer may subscribe to notifications of failures in the enforcement of UP path changes including within the "evSubsc" attribute the "event" attribute value "UP\_PATH\_CHG\_FAILURE" in an entry of the "events" array.

NOTE 2: In the case that the PCF determines that the requested AF routing requirements cannot be applied and returns the "servAuthInfo" attribute in the HTTP response, the PCF makes the decision without considering the requested AF routing requirements.

The PCF shall reply to the NF service consumer as described in subclause 4.2.2.2.

The PCF shall store the routing requirements included in the "afRoutReq" attribute.

The PCF shall check whether the received routing requirements requires PCC rules to be created or provisioned to include or modify traffic steering policies, the AF transaction identifier and the application relocation possibility as specified in 3GPP TS 29.513 [7]. Provisioning of PCC rules to the SMF shall be carried out as specified in 3GPP TS 29.512 [8].

NOTE 3: The NF service consumer receives the notification about UP path management events by the Nsmf\_EventExposure\_Notify service operation as defined in subclause 4.2.2.2 of 3GPP TS 29.508 [13].

\*\*\* 3rd Change \*\*\*

#### 4.2.3.8 Update of traffic routing information

This procedure is used by NF service consumer to modify in the PCF the traffic routing information to a local access to a DNN, and/or to modify the subscription to notifications about UP path management when "InfluenceOnTrafficRouting" feature is supported.

When the "EnEDGE" feature is supported this procedure may be used to modify (create, delete, update) the indication of simultaneous connectivity temporarily maintained for the source and target PSA and/or the indication of the minimum time interval to be considered for inactivity for the traffic routed via the source PSA.

The NF service consumer shall use the HTTP PATCH method.

To modify traffic routing information, the NF service consumer shall include in the HTTP PATCH request message described in subclause 4.2.3.2, in the "ascReqData" attribute, an updated "afRoutReq" attribute(s) with the modified traffic routing information. To modify the indication of simultaneous connectivity and/or the termination of the simultaneous connectivity, the NF service consumer shall include an updated "simConnInd" attribute and/or an updated "simConnTem" attribute, if applicable.

To modify the subscription to notifications about UP path management events (create, delete or modify), the NF service consumer shall include in the HTTP PATCH request message described in subclause 4.2.3.2, in the "ascReqData" attribute, the updated values of the "upPathChgSub" attribute with the modified subscription to UP path management events.

When the feature "RoutingReqOutcome" is supported:

- and the NF service consumer is creating or modifying AF routing information, the PCF may set the "servAuthInfo" attribute in the HTTP response message to "ROUT\_REQ\_NOT\_AUTHORIZED" when the PCF determines, e.g. based on subscription, the AF influence on traffic routing is not allowed for the PDU session;

- when the NF service consumer requests the update of the steering of traffic to a DNAI and/or the subscription to notifications about UP path management events, the NF service consumer may subscribe to notifications of failures in the enforcement of UP path changes including within the "evSubsc" attribute the "event" attribute value "UP\_PATH\_CHG\_FAILURE" in an entry of the "events" array, or may remove the subscription to notification of failures in the enforcement of UP path changes by not including the the "event" attribute value "UP\_PATH\_CHG\_FAILURE" in an entry of the "events" array of the "evSubsc" attribute.

NOTE: In the case that the PCF determines that the requested AF routing requirements cannot be applied and returns the "servAuthInfo" attribute in the HTTP response, the PCF makes the decision without considering the requested AF routing requirements.

The PCF shall reply to the NF service consumer as described in subclause 4.2.3.2.

The PCF shall store the application routing requirements included in the "afRoutReq" attribute.

The PCF shall check whether the updated application routing requirements require PCC rules to be created or modified to include updated traffic steering policies, or the AF transaction identifier, or to update the application relocation possibility as specified in 3GPP TS 29.513 [7]. Provisioning of PCC rules to the SMF shall be carried out as specified at 3GPP TS 29.512 [8].

\*\*\* 4th Change \*\*\*

### 5.6.1 General

This subclause specifies the application data model supported by the API.

Table 5.6.1-1 specifies the data types defined for the Npcf\_PolicyAuthorization service based interface protocol.

Table 5.6.1-1: Npcf\_PolicyAuthorization specific Data Types

| Data type | Section defined | Description | Applicability |
| --- | --- | --- | --- |
| AcceptableServiceInfo | 5.6.2.30 | Acceptable maximum requested bandwidth. |  |
| AccessNetChargingIdentifier | 5.6.2.32 | Contains the access network charging identifier. | IMS\_SBI |
| AfAppId | 5.6.3.2 | Contains an AF application identifier. |  |
| AfEvent | 5.6.3.7 | Represents an event to notify to the NF service consumer. |  |
| AfEventNotification | 5.6.2.11 | Represents the notification of an event. |  |
| AfEventSubscription | 5.6.2.10 | Represents the subscription to events. |  |
| AfNotifMethod | 5.6.3.8 | Represents the notification methods that can be subscribed for an event. |  |
| AfRequestedData | 5.6.3.18 | Represents the information the NF service consumer requested to be exposed. | IMS\_SBI |
| AfRoutingRequirement | 5.6.2.13 | Describes the routing requirements for the application traffic flows. | InfluenceOnTrafficRouting |
| AfRoutingRequirementRm | 5.6.2.24 | This data type is defined in the same way as the "AfRoutingRequirement" data type, but with the OpenAPI "nullable: true" property. | InfluenceOnTrafficRouting |
| AnGwAddress | 5.6.2.20 | Carries the control plane address of the access network gateway. |  |
| AppDetectionReport | 5.6.2.44 | Indicates the start or stop of the detected application traffic and the detected AF application identifier. | ApplicationDetectionEvents |
| AppDetectionNotifType | 5.6.3.23 | Represents the types of reports bound to the notification of application detection information. | ApplicationDetectionEvents |
| AppSessionContext | 5.6.2.2 | Represents an Individual Application Session Context resource. |  |
| AppSessionContextReqData | 5.6.2.3 | Represents the Individual Application Session Context resource data received in an HTTP POST request message. |  |
| AppSessionContextRespData | 5.6.2.4 | Represents the Individual Application Session Context resource data produced by the server and returned in an HTTP response message. |  |
| AppSessionContextUpdateData | 5.6.2.5 | Describes the modifications to the "ascReqData" property of an Individual Application Session Context resource. |  |
| AppSessionContextUpdateDataPatch | 5.6.2.43 | Describes the modifications to an Individual Application Session Context resource | PatchCorrection |
| AspId | 5.6.3.2 | Contains an identity of an application service provider. | SponsoredConnectivity |
| CodecData | 5.6.3.2 | Contains a codec related information. |  |
| ContentVersion | 5.6.3.2 | Represents the version of a media component. | MediaComponentVersioning |
| EthFlowDescription | 5.6.2.17 | Defines a packet filter for an Ethernet flow. |  |
| EventsNotification | 5.6.2.9 | Describes the notification about the events occurred within an Individual Application Session Context resource. |  |
| EventsSubscPutData | 5.6.2.42 | Identifies the events the application subscribes to within an Events Subscription sub-resource data. It may also include the attributes of the notification about the events already met at the time of subscription. It is represented as a non-exclusive list of two data types: EventsSubscReqData and EventsNotification. |  |
| EventsSubscReqData | 5.6.2.6 | Identifies the events the application subscribes to within an Individual Application Session Context resource. |  |
| EventsSubscReqDataRm | 5.6.2. 25 | This data type is defined in the same way as the "EventsSubscReqData" data type, but with the OpenAPI "nullable: true" property. |  |
| ExtendedProblemDetails | 5.6.2.29 | Data type that extends ProblemDetails. |  |
| FlowDescription | 5.6.3.2 | Defines a packet filter for an IP flow. |  |
| Flows | 5.6.2.21 | Identifies the flows related to a media component. |  |
| FlowStatus | 5.6.3.12 | Describes whether the IP flow(s) are enabled or disabled. |  |
| FlowUsage | 5.6.3.14 | Describes the flow usage of the flows described by a media subcomponent. |  |
| MediaComponent | 5.6.2.7 | Contains service information for a media component of an AF session. |  |
| MediaComponentRm | 5.6.2.26 | This data type is defined in the same way as the "MediaComponent" data type, but with the OpenAPI "nullable: true" property. |  |
| MediaComponentResourcesStatus | 5.6.3.13 | Indicates whether the media component is active or inactive. |  |
| MediaSubComponent | 5.6.2.8 | Contains the requested bitrate and filters for the set of IP flows identified by their common flow identifier. |  |
| MediaSubComponentRm | 5.6.2.27 | This data type is defined in the same way as the "MediaSubComponent" data type, but with the OpenAPI "nullable: true" property. |  |
| MediaType | 5.6.3.3 | Indicates the media type of a media component. |  |
| MpsAction | 5.6.3.22 | Indicates whether the it is an invocation or a revocation of the MPS for DTS service. | MPSforDTS |
| OutOfCreditInformation | 5.6.2.33 | Indicates the service data flows without available credit and the corresponding termination action. | IMS\_SBI |
| PcscfRestorationRequestData | 5.6.2.36 | Indicates P-CSCF restoration. | PCSCF-Restoration-Enhancement |
| PduSessionTsnBridge | 5.6.2.40 | Contains the TSC user plane node Information and DS-TT port and/or NW-TT ports management information of a new detected TSC user plane node in the context of a new PDU session. | TimeSensitiveNetworkingTimeSensitiveCommunication |
| PreemptionControlInformation | 5.6.3.19 | Pre-emption control information. | MCPTT-Preemption |
| PreemptionControlInformationRm | 5.6.3.21 | This data type is defined in the same way as the "PreemptionControlInformation" data type, but with the OpenAPI "nullable: true" property. | MCPTT-Preemption |
| PrioritySharingIndicator | 5.6.3.20 | Priority sharing indicator. | PrioritySharing |
| QosMonitoringInformation | 5.6.2.34 | QoS monitoring for UL, DL or round trip delay. | QoSMonitoring |
| QosMonitoringInformationRm | 5.6.2.41 | This data type is defined in the same way as the "QosMonitoringInformation" data type, but with the OpenAPI "nullable: true" property. | QoSMonitoring |
| QosMonitoringReport | 5.6.2.37 | Contains QoS monitoring reporting information. | QoSMonitoring |
| QosNotificationControlInfo | 5.6.2.15 | Indicates whether the QoS targets related to certain media component are not guaranteed or are guaranteed again. |  |
| QosNotifType | 5.6.3.9 | Indicates type of notification for QoS Notification Control. |  |
| RequiredAccessInfo | 5.6.3.15 | Indicates the access network information required for an AF session. | NetLoc |
| ReservPriority | 5.6.3.4 | Indicates the reservation priority. |  |
| ResourcesAllocationInfo | 5.6.2.14 | Indicates the status of the PCC rule(s) related to certain media component. |  |
| ServAuthInfo | 5.6.3.5 | Indicates the result of the Policy Authorization service request from the NF service consumer. |  |
| ServiceInfoStatus | 5.6.3.16 | Preliminary or final service information status. | IMS\_SBI |
| ServiceUrn | 5.6.3.2 | Service URN. | IMS\_SBI |
| SipForkingIndication | 5.6.3.17 | Describes if several SIP dialogues are related to an "Individual Application Session Context" resource. | IMS\_SBI |
| SpatialValidity | 5.6.2.16 | Describes the spatial validity of an NF service consumer request for influencing traffic routing. | InfluenceOnTrafficRouting |
| SpatialValidityRm | 5.6.2.28 | This data type is defined in the same way as the "SpatialValidity" data type, but with the OpenAPI "nullable: true" property. | InfluenceOnTrafficRouting |
| SponId | 5.6.3.2 | Contains an Identity of a sponsor. | SponsoredConnectivity |
| SponsoringStatus | 5.6.3.6 | Represents whether sponsored data connectivity is enabled or disabled/not enabled. | SponsoredConnectivity |
| TemporalValidity | 5.6.2.22 | Indicates the time interval during which the NF service consumer request is to be applied. | InfluenceOnTrafficRouting |
| TerminationCause | 5.6.3.10 | Indicates the cause for requesting the deletion of the Individual Application Session Context resource. |  |
| TerminationInfo | 5.6.2.12 | Includes information related to the termination of the Individual Application Session Context resource. |  |
| TosTrafficClass | 5.6.3.2 | Contains the IPv4 Type-of-Service or the IPv6 Traffic-Class field and the ToS/Traffic Class mask field. |  |
| TosTrafficClassRm | 5.6.3.2 | This data type is defined in the same way as the "TosTrafficClass" data type, but with the OpenAPI "nullable: true" property. |  |
| TscPriorityLevel | 5.6.3.2 | Priority of TSC Flows | TimeSensitiveNetworking |
| TscPriorityLevelRm | 5.6.3.2 | This data type is defined in the same way as the "TscPriorityLevel" data type, but with the OpenAPI "nullable: true" property | TimeSensitiveNetworking |
| TscaiInputContainer | 5.6.2.39 | TSCAI Input information container. | TimeSensitiveNetworking |
| TsnQosContainer | 5.6.2.35 | TSC traffic QoS parameters. | TimeSensitiveNetworking |
| TsnQosContainerRm | 5.6.2.38 | This data type is defined in the same way as the "TsnQosContainer" data type, but with the OpenAPI "nullable: true" property. | TimeSensitiveNetworking |
| UeIdentityInfo | 5.6.2.31 | Represents 5GS-Level UE Identities. | IMS\_SBI |

Table 5.6.1-2 specifies data types re-used by the Npcf\_PolicyAuthorization service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Npcf\_PolicyAuthorization service based interface.

Table 5.6.1-2: Npcf\_PolicyAuthorization re-used Data Types

| Data type | Reference | Comments | Applicability |
| --- | --- | --- | --- |
| AccNetChargingAddress | 3GPP TS 29.512 [8] | Indicates the IP address of the network entity within the access network performing charging. | IMS\_SBI |
| AccessType | 3GPP TS 29.571 [12] | The identification of the type of access network. |  |
| AccumulatedUsage | 3GPP TS 29.122 [15] | Accumulated Usage. | SponsoredConnectivity |
| AdditionalAccessInfo | 3GPP TS 29.512 [8] | Indicates the combination of additional Access Type and RAT Type for MA PDU session | ATSSS |
| AfSigProtocol | 3GPP TS 29.512 [8] | Represents the protocol used for signalling between the UE and the NF service consumer. | ProvAFsignalFlow |
| ApplicationChargingId | 3GPP TS 29.571 [12] | Application provided charging identifier allowing correlation of charging information. | IMS\_SBI |
| BdtReferenceId | 3GPP TS 29.122 [15] | Identifies transfer policies. |  |
| BitRate | 3GPP TS 29.571 [12] | Specifies bitrate in kbits per second. |  |
| BitRateRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |  |
| BridgeManagementContainer | 3GPP TS 29.512 [8] | Contains TSC user plane node management information. | TimeSensitiveNetworking |
| Bytes | 3GPP TS 29.571 [12] | String with format "byte". |  |
| ChargingId | 3GPP TS 29.571 [12] | Charging identifier allowing correlation of charging information. | IMS\_SBI |
| DateTime | 3GPP TS 29.571 [12] | String with format "date-time" as defined in OpenAPI Specification [11]. | InfluenceOnTrafficRouting, TimeSensitiveNetworking |
| Dnn | 3GPP TS 29.571 [12] | Data Network Name. |  |
| DurationSec | 3GPP TS 29.571 [12] | Identifies a period of time in units of seconds. | TimeSensitiveNetworking, EnhancedSubscriptionToNotification,EnEDGE  |
| DurationSecRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "DurationSec" data type, but with the OpenAPI "nullable: true" property. | EnEDGE  |
| FinalUnitAction | 3GPP TS 32.291 [22] | Indicates the action to be taken when the user's account cannot cover the service cost. |  |
| Float | 3GPP TS 29.571 [12] | Number with format "float" as defined in OpenAPI Specification [11]. | FLUS |
| FloatRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "Float" data type, but with the OpenAPI "nullable: true" property. | FLUS |
| FlowDirection | 3GPP TS 29.512 [8] | Flow Direction. |  |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [12] | Maximum Burst Size. | TimeSensitiveNetworking |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property | TimeSensitiveNetworking |
| Gpsi | 3GPP TS 29.571 [12] | Identifies the GPSI. |  |
| Ipv4Addr | 3GPP TS 29.571 [12] | Identifies an IPv4 address. |  |
| Ipv6Addr | 3GPP TS 29.571 [12] | Identifies an IPv6 address. |  |
| MacAddr48 | 3GPP TS 29.571 [12] | MAC Address. |  |
| NetLocAccessSupport | 3GPP TS 29.512 [8] | Indicates the access network does not support the report of the requested access network information. | NetLoc |
| NullValue | 3GPP TS 29.571 [12] | JSON's null value, used as an explicit value of an enumeration. | MCPTT-Preemption |
| PacketDelBudget | 3GPP TS 29.571 [12] | Packet Delay Budget. | TimeSensitiveNetworking |
| PacketDelBudgetRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "PacketDelBudget" data type, but with the OpenAPI "nullable: true" property | TimeSensitiveNetworking |
| PacketLossRateRm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "PacketLossRate" data type, but with the OpenAPI "nullable: true" property. | CHEM |
| Pei | 3GPP TS 29.571 [12] | Identifies the PEI. | IMS\_SBI |
| PlmnIdNid | 3GPP TS 29.571 [12] | Identifies the network: the PLMN Identifier (the mobile country code and the mobile network code) or the SNPN Identifier (the PLMN Identifier and the NID). |  |
| PreemptionCapability | 3GPP TS 29.571 [12] | Pre-emption capability. | MCPTT-Preemption |
| PreemptionVulnerability | 3GPP TS 29.571 [12] | Pre-emption vulnerability. | MCPTT-Preemption |
| PreemptionCapabilityRm | 3GPP TS 29.571 [12] | It is defined in the same way as the "PreemptionCapability" data type, but with the OpenAPI "nullable: true" property. | MCPTT-Preemption |
| PreemptionVulnerabilityRm | 3GPP TS 29.571 [12] | It is defined in the same way as the "PreemptionVulnerability" data type, but with the OpenAPI "nullable: true" property. | MCPTT-Preemption |
| PresenceInfo | 3GPP TS 29.571 [12] | Represents an area of interest, e.g. a Presence Reporting Area. | InfluenceOnTrafficRouting |
| PortManagementContainer | 3GPP TS 29.512 [8] | Contains port management information for a related port. | TimeSensitiveNetworking |
| ProblemDetails | 3GPP TS 29.571 [12] | Contains a detailed information about an error. |  |
| RanNasRelCause | 3GPP TS 29.512 [8] | Indicates RAN and/or NAS release cause code information. | RAN-NAS-Cause |
| RedirectResponse | 3GPP TS 29.571 [12] | Contains redirection related information. | ES3XX |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicate the UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for URLLC is enabled for the service data flow. | QoSMonitoring |
| RatType | 3GPP TS 29.571 [12] | RAT Type. |  |
| RouteToLocation | 3GPP TS 29.571 [12] | Identifies routes to locations of applications. | InfluenceOnTrafficRouting |
| SatelliteBackhaulCategory | 3GPP TS 29.512 [8] | Indicates the satellite or non-satellite backhaul category | SatelliteBackhaul |
| Snssai | 3GPP TS 29.571 [12] | Identifies the S-NSSAI. |  |
| Supi | 3GPP TS 29.571 [12] | Identifies the SUPI. |  |
| SupportedFeatures | 3GPP TS 29.571 [12] | Used to negotiate the applicability of the optional features defined in table 5.8-1. |  |
| TimeZone | 3GPP TS 29.571 [12] | Time Zone. | NetLoc |
| TsnBridgeInfo | 3GPP TS 29.512 [8] | TSC user plane node information. | TimeSensitiveNetworking |
| Uinteger | 3GPP TS 29.571 [12] | Unsigned Integer. | TimeSensitiveNetworking |
| Uint32 | 3GPP TS 29.571 [12] | Unsigned 32-bit integers, i.e. only value 0 and 32-bit integers above 0 are permissible. | ResourceSharing |
| Uint32Rm | 3GPP TS 29.571 [12] | This data type is defined in the same way as the "Uint32" data type, but with the OpenAPI "nullable: true" property. | ResourceSharing |
| Uinteger | 3GPP TS 29.571 [12] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible.Minimum = 0. | TimeSensitiveCommunication |
| UpPathChgEvent | 3GPP TS 29.512 [8] | Contains the subscription information to be delivered to SMF for the UP path management events. | InfluenceOnTrafficRouting |
| Uri | 3GPP TS 29.571 [12] | String providing an URI. |  |
| UsageThreshold | 3GPP TS 29.122 [15] | Usage Thresholds. | SponsoredConnectivity |
| UsageThresholdRm | 3GPP TS 29.122 [15] | This data type is defined in the same way as the "UsageThreshold" data type, but with the OpenAPI "nullable: true" property. | SponsoredConnectivity |
| UserLocation | 3GPP TS 29.571 [12] | User Location(s). | NetLoc |

\*\*\* 5th Change \*\*\*

#### 5.6.2.13 Type AfRoutingRequirement

Table 5.6.2.13-1: Definition of type AfRoutingRequirement

| Attribute name | Data type | P | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- | --- |
| appReloc | boolean | O | 0..1 | Indication of application relocation possibility.When it is included and set to "true", it indicates that the application cannot be relocated once a location of the application is selected by the 5GC. The default value is "false". | InfluenceOnTrafficRouting |
| routeToLocs | array(RouteToLocation) | O | 1..N | A list of traffic routes to applications locations. | InfluenceOnTrafficRouting |
| spVal | SpatialValidity | O | 0..1 | Indicates where the traffic routing requirements apply. The absence of this attribute indicates no spatial restrictions. | InfluenceOnTrafficRouting |
| tempVals | array(TemporalValidity) | O | 1..N | Indicates the time interval(s) during which the NF service consumer request is to be applied. | InfluenceOnTrafficRouting |
| upPathChgSub | UpPathChgEvent | O | 0..1 | Subscription to UP path management events. | InfluenceOnTrafficRouting |
| addrPreserInd | boolean | O | 0..1 | Indicates whether UE IP address should be preserved.This attribute shall set to "true" if preserved, otherwise, set to "false".Default value is false if omitted. | URLLC |
| simConnInd | boolean | O | 0..1 | Indication of simultaneous connectivity temporarily maintained for the source and target PSA. If it is included and set to "true", temporary simultaneous connectivity should be kept. The default value "false" applies, if the attribute is not present and has not been supplied previously. | EnEDGE |
| simConnTerm | DurationSec | C | 0..1 | Indication of the minimum time interval to be considered for inactivity of the traffic routed via the source PSA during the edge re-location procedure. It may be included when the "simConnInd" attribute is set to true.  | EnEDGE |

\*\*\* 6th Change \*\*\*

#### 5.6.2.24 Type AfRoutingRequirementRm

This data type is defined in the same way as the "AfRoutingRequirement" data type, but:

- with the OpenAPI "nullable: true" property;

- the removable attribute "spVal" is defined with the data type "SpatialValidityRm"; and

- the removable attributes "tempVals", "routeToLocs", "addrPreserInd", "simConnInd" and "simConnTerm" are defined as nullable in the OpenAPI.

Table 5.6.2.24-1: Definition of type AfRoutingRequirementRm

| Attribute name | Data type | P | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- | --- |
| appReloc | boolean | O | 0..1 | Indication of application relocation possibility. When it is set to "true", it indicates that the application cannot be relocated once a location of the application is selected by the 5GC. | InfluenceOnTrafficRouting |
| routeToLocs | array(RouteToLocation) | O | 1..N | A list of traffic routes to applications locations. | InfluenceOnTrafficRouting |
| spVal | SpatialValidityRm | O | 0..1 | Indicates where the traffic routing requirements apply. | InfluenceOnTrafficRouting |
| tempVals | array(TemporalValidity) | O | 1..N | Indicates the time interval(s) during which the NF service consumer request is to be applied. | InfluenceOnTrafficRouting |
| upPathChgSub | UpPathChgEvent | O | 0..1 | Subscription to UP path management events. | InfluenceOnTrafficRouting |
| addrPreserInd | boolean | O | 0..1 | Indicates whether UE IP address should be preserved. | URLLC |
| simConnInd | boolean | O | 0..1 | Indication of simultaneous connectivity temporarily maintained for the source and target PSA. If it is included and set to "true", temporary simultaneous connectivity should be kept.  | EnEDGE |
| simConnTerm | DurationSecRm | C | 0..1 | Indication of the minimum time interval to be considered for inactivity of the traffic routed via the source PSA during the edge re-location procedure. | EnEDGE |

\*\*\* 7th Change \*\*\*

## 5.8 Feature negotiation

The optional features in table 5.8-1 are defined for the Npcf\_PolicyAuthorization API. They shall be negotiated using the extensibility mechanism defined in subclause 6.6.2 of 3GPP TS 29.500 [5].

When requesting the PCF to create an Individual Application Session Context resource the NF service consumer shall indicate the optional features the NF service consumer supports for the Npcf\_PolicyAuthorization service by including the "suppFeat" attribute in the "AppSessionContextReqData" data type of the HTTP POST request.

The PCF shall determine the supported features for the created Individual Application Session Context resource as specified in subclause 6.6.2 of 3GPP TS 29.500 [5]. The PCF shall indicate the supported features in the HTTP response confirming the creation of the Individual Application Session Context resource by including the "suppFeat" attribute in the "AppSessionContextRespData" data type.

Table 5.8-1: Supported Features

| Feature number | Feature Name | Description |
| --- | --- | --- |
| 1 | InfluenceOnTrafficRouting | Indicates support of Application Function influence on traffic routing. If the PCF supports this feature, the NF service consumer may influence SMF routing to applications or subscribe to notifications of UP path management for the traffic flows of an active PDU session. |
| 2 | SponsoredConnectivity | Indicates support of sponsored data connectivity. If the PCF supports this feature, the NF service consumer may provide sponsored data connectivity to the SUPI. |
| 3 | MediaComponentVersioning | Indicates the support of the media component versioning. |
| 4 | URLLC | Indicates support of Ultra-Reliable Low-Latency Communication (URLLC) requirements, i.e. AF application relocation acknowledgement and UE address(es) preservation. The InfluenceOnTrafficRouting feature shall be supported in order to support this feature. |
| 5 | IMS\_SBI | Indicates support of the communication with the 5GC IMS NF service consumer via Service Based Interfaces. |
| 6 | NetLoc | Indicates the support of access network information reporting. |
| 7 | ProvAFsignalFlow | This indicates support for the feature of provisioning of AF signalling flow information as described in subclauses 4.2.2.16 and 4.2.3.17. If the PCF supports this feature the NF service consumer may provision AF signalling flow information.NOTE: This feature is used by the IMS Restoration Procedures to provide to the SMF the address of the P-CSCF selected by the UE, refer to 3GPP TS 23.380 [39].The IMS\_SBI feature shall be supported in order to support this feature. |
| 8 | ResourceSharing | This feature indicates the support of resource sharing across several "Individual Application Session Context" resources. The IMS\_SBI feature shall be supported in order to support this feature. |
| 9 | MCPTT | This feature indicates the support of Mission Critical Push To Talk services as described in 3GPP TS 24.379 [41]. |
| 10 | MCVideo | This feature indicates the support of Mission Critical Video services as described in 3GPP TS 24.281 [43]. |
| 11 | PrioritySharing | This feature indicates that Priority Sharing is supported as described in 3GPP TS 23.503 [4], subclause 6.1.3.15. |
| 12 | MCPTT-Preemption | This feature indicates the support of service pre-emption based on the information provided by the NF service consumer. It requires that both PrioritySharing and MCPTT features are also supported. |
| 13 | MacAddressRange | Indicates the support of a set of MAC addresses with a specific range in the traffic filter. |
| 14 | RAN-NAS-Cause | This feature indicates the support for the release cause code information from the access network. |
| 15 | EnhancedSubscriptionToNotification | Indicates the support of:- Subscription to periodic notifications.- Definition of a waiting time between the reporting of two event triggered events.- Indication of whether the event has to be reported at PDU Session termination.- Notification Correlation Id for a subscription to an event. |
| 16 | QoSMonitoring | Indicates the support of QoS monitoring information. This feature requires the support of the EnhancedSubscriptionToNotification feature. |
| 17 | AuthorizationWithRequiredQoS | Indicates support of policy authorization for the AF session with required QoS. |
| 18 | TimeSensitiveNetworking | Indicates that the 5G System is integrated within the external network as a TSN bridge. |
| 19 | PCSCF-Restoration-Enhancement | This feature indicates support of P-CSCF Restoration Enhancement. It is used for the PCF and the P-CSCF to indicate if they support P-CSCF Restoration Enhancement. |
| 20 | CHEM | This feature indicates the support of Coverage and Handover Enhancements for Media (CHEM). |
| 21 | FLUS | This feature indicates the support of FLUS functionality as described in 3GPP TS 26.238 [51]. |
| 22 | EPSFallbackReport | This feature indicates the support of the report of EPS Fallback as defined in subclauses 4.2.2.30, 4.2.3.29 and 4.2.5.15. |
| 23 | ATSSS | Indicates the support of the report of the multiple access types of a MA PDU session. |
| 24 | QoSHint | This feature indicates the support of specific QoS hint parameters as described in 3GPP TS 26.114 [30], subclause 6.2.10. |
| 25 | ReallocationOfCredit | This feature indicates the support of notifications of reallocation of credits events. It requires the support of IMS\_SBI feature. |
| 26 | ES3XX | Extended Support for 3xx redirections. This feature indicates the support of redirection for any service operation, according to Stateless NF procedures as specified in subclauses 6.5.3.2 and 6.5.3.3 of 3GPP TS 29.500 [5] and according to HTTP redirection principles for indirect communication, as specified in subclause 6.10.9 of 3GPP TS 29.500 [5].  |
| 27 | DisableUENotification | Indicates the support of disabling QoS flow parameters signalling to the UE when the SMF is notified by the NG-RAN of changes in the fulfilled QoS situation. This feature requires that the AuthorizationWithRequiredQoS featute is also supported. |
| 28 | PatchCorrection | Indicates support of the correction to the PATCH method:When this feature is not supported, the interoperability between a NF service consumer and the PCF can only be ensured when it is not required the update of the Individual Application Session Context resource. |
| 29 | MPSforDTS | Indicates support for MPS for DTS as described in subclauses 4.2.2.12.2 and 4.2.3.12. |
| 30 | ApplicationDetectionEvents | This feature indicates the support of the subscription to notifications of the detection of the start and stop of an application's traffic. |
| 31 | TimeSensitiveCommunication | Indicates that the 5G System is integrated within the external network as a TSC user plane node to enable the Time Sensitive Communications and Time Synchronization. This feature requires that the TimeSensitiveNetworking feature is also supported. |
| 32 | EnEDGE | This feature indicates the support of:- The indication of direct event notification of QoS monitoring events from the UPF to the Local NEF or AF in 5GC. This indication requires that the QoSMonitoring feature is supported.- The indication of temporary simultaneous connectivity over source and target PSA at edge relocation. This indication requires that the InfluenceOnTrafficRouting feature is supported. |
| 33 | SatelliteBackhaul | Indicates the support of the report of the satellite or non-satellite backhaul category of the PDU session. |
| f1 | RoutingReqOutcome | Indicates the support of:- the report of UP path change failures; and - the indication of whether AF routing requirements are applied.It requires the support of InfluenceOnTrafficRouting feature. |

\*\*\* 8th Change \*\*\*

# A.2 Npcf\_PolicyAuthorization API

openapi: 3.0.0

info:

 title: Npcf\_PolicyAuthorization Service API

 version: 1.2.0-alpha.3

 description: |

 PCF Policy Authorization Service.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.514 V17.2.0; 5G System; Policy Authorization Service;Stage 3.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.514/'

#

servers:

 - url: '{apiRoot}/npcf-policyauthorization/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-policyauthorization

paths:

 /app-sessions:

 post:

 summary: Creates a new Individual Application Session Context resource

 operationId: PostAppSessions

 tags:

 - Application Sessions (Collection)

 requestBody:

 description: Contains the information for the creation the resource

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 responses:

 '201':

 description: Successful creation of the resource

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 headers:

 Location:

 description: 'Contains the URI of the created individual application session context resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId} or the URI of the created events subscription sub-resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

 required: true

 schema:

 type: string

 '303':

 description: See Other. The result of the HTTP POST request would be equivalent to the existing Application Session Context.

 headers:

 Location:

 description: 'Contains the URI of the existing individual Application Session Context resource.'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: '#/components/schemas/ExtendedProblemDetails'

 headers:

 Retry-After:

 description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

 schema:

 anyOf:

 - type: integer

 - type: string

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 terminationRequest:

 '{$request.body#/ascReqData/notifUri}/terminate':

 post:

 requestBody:

 description: Request of the termination of the Individual Application Session Context

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TerminationInfo'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 eventNotification:

 '{$request.body#/ascReqData/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 detected5GsBridgeForPduSession:

 '{$request.body#/ascReqData/evSubsc/notifUri}/new-bridge':

 post:

 requestBody:

 description: Notification of a new TSC user plane node detected in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PduSessionTsnBridge'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /app-sessions/pcscf-restoration:

 post:

 summary: "Indicates P-CSCF restoration and does not create an Individual Application Session Context"

 operationId: PcscfRestoration

 tags:

 - PCSCF Restoration Indication

 requestBody:

 description: PCSCF Restoration Indication

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcscfRestorationRequestData'

 responses:

 '204':

 description: The deletion is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

 /app-sessions/{appSessionId}:

 get:

 summary: "Reads an existing Individual Application Session Context"

 operationId: GetAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the resource

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of the resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: "Modifies an existing Individual Application Session Context"

 operationId: ModAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: modification of the resource.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/AppSessionContextUpdateDataPatch'

 responses:

 '200':

 description: successful modification of the resource and a representation of that resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '204':

 description: The successful modification

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: '#/components/schemas/ExtendedProblemDetails'

 headers:

 Retry-After:

 description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

 schema:

 anyOf:

 - type: integer

 - type: string

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/ascReqData/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

#

 /app-sessions/{appSessionId}/delete:

 post:

 summary: "Deletes an existing Individual Application Session Context"

 operationId: DeleteAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Individual Application Session Context resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: deletion of the Individual Application Session Context resource, req notification

 required: false

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '200':

 description: The deletion of the resource is confirmed and a resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '204':

 description: The deletion is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

 /app-sessions/{appSessionId}/events-subscription:

 put:

 summary: "creates or modifies an Events Subscription subresource"

 operationId: updateEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Events Subscription resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Creation or modification of an Events Subscription resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '201':

 description: The creation of the Events Subscription resource is confirmed and its representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscPutData'

 headers:

 Location:

 description: 'Contains the URI of the created Events Subscription resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

 required: true

 schema:

 type: string

 '200':

 description: The modification of the Events Subscription resource is confirmed its representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscPutData'

 '204':

 description: The modification of the Events Subscription subresource is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/notifUri}/notify':

 post:

 requestBody:

 description: Contains the information for the notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: deletes the Events Subscription subresource

 operationId: DeleteEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Individual Application Session Context resource

 in: path

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The deletion of the of the Events Subscription sub-resource is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-policyauthorization: Access to the Npcf\_PolicyAuthorization API

 schemas:

 AppSessionContext:

 description: Represents an Individual Application Session Context resource.

 type: object

 properties:

 ascReqData:

 $ref: '#/components/schemas/AppSessionContextReqData'

 ascRespData:

 $ref: '#/components/schemas/AppSessionContextRespData'

 evsNotif:

 $ref: '#/components/schemas/EventsNotification'

 AppSessionContextReqData:

 description: Identifies the service requirements of an Individual Application Session Context.

 type: object

 required:

 - notifUri

 - suppFeat

 oneOf:

 - required: [ueIpv4]

 - required: [ueIpv6]

 - required: [ueMac]

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afChargId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 afReqData:

 $ref: '#/components/schemas/AfRequestedData'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirement'

 aspId:

 $ref: '#/components/schemas/AspId'

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqData'

 mcpttId:

 description: indication of MCPTT service request

 type: string

 mcVideoId:

 description: indication of MCVideo service request

 type: string

 medComponents:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponent'

 minProperties: 1

 description: Contains media component information. The key of the map is the medCompN attribute.

 ipDomain:

 type: string

 mpsAction:

 $ref: '#/components/schemas/MpsAction'

 mpsId:

 description: indication of MPS service request

 type: string

 mcsId:

 description: indication of MCS service request

 type: string

 preemptControlInfo:

 $ref: '#/components/schemas/PreemptionControlInformation'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 servInfStatus:

 $ref: '#/components/schemas/ServiceInfoStatus'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 servUrn:

 $ref: '#/components/schemas/ServiceUrn'

 sliceInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 sponId:

 $ref: '#/components/schemas/SponId'

 sponStatus:

 $ref: '#/components/schemas/SponsoringStatus'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 AppSessionContextRespData:

 description: Describes the authorization data of an Individual Application Session Context created by the PCF.

 type: object

 properties:

 servAuthInfo:

 $ref: '#/components/schemas/ServAuthInfo'

 ueIds:

 type: array

 items:

 $ref: '#/components/schemas/UeIdentityInfo'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 AppSessionContextUpdateDataPatch:

 description: Identifies the modifications to an Individual Application Session Context and/or the modifications to the sub-resource Events Subscription.

 type: object

 properties:

 ascReqData:

 $ref: '#/components/schemas/AppSessionContextUpdateData'

 AppSessionContextUpdateData:

 description: Identifies the modifications to the "ascReqData" property of an Individual Application Session Context which may include the modifications to the sub-resource Events Subscription.

 type: object

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirementRm'

 aspId:

 $ref: '#/components/schemas/AspId'

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqDataRm'

 mcpttId:

 description: indication of MCPTT service request

 type: string

 mcVideoId:

 description: indication of modification of MCVideo service

 type: string

 medComponents:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponentRm'

 minProperties: 1

 description: Contains media component information. The key of the map is the medCompN attribute.

 mpsAction:

 $ref: '#/components/schemas/MpsAction'

 mpsId:

 description: indication of MPS service request

 type: string

 mcsId:

 description: indication of MCS service request

 type: string

 preemptControlInfo:

 $ref: '#/components/schemas/PreemptionControlInformationRm'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 servInfStatus:

 $ref: '#/components/schemas/ServiceInfoStatus'

 sipForkInd:

 $ref: '#/components/schemas/SipForkingIndication'

 sponId:

 $ref: '#/components/schemas/SponId'

 sponStatus:

 $ref: '#/components/schemas/SponsoringStatus'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 EventsSubscReqData:

 description: Identifies the events the application subscribes to.

 type: object

 required:

 - events

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/AfEventSubscription'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqQosMonParams:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

 minItems: 1

 qosMon:

 $ref: '#/components/schemas/QosMonitoringInformation'

 reqAnis:

 type: array

 items:

 $ref: '#/components/schemas/RequiredAccessInfo'

 minItems: 1

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

 notifCorreId:

 type: string

 afAppIds:

 type: array

 items:

 $ref: '#/components/schemas/AfAppId'

 minItems: 1

 directNotifInd:

 type: boolean

 EventsSubscReqDataRm:

 description: this data type is defined in the same way as the EventsSubscReqData data type, but with the OpenAPI nullable property set to true.

 type: object

 required:

 - events

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/AfEventSubscription'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqQosMonParams:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

 minItems: 1

 qosMon:

 $ref: '#/components/schemas/QosMonitoringInformationRm'

 reqAnis:

 type: array

 items:

 $ref: '#/components/schemas/RequiredAccessInfo'

 minItems: 1

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

 notifCorreId:

 type: string

 directNotifInd:

 type: boolean

 nullable: true

 MediaComponent:

 description: Identifies a media component.

 type: object

 required:

 - medCompN

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirement'

 qosReference:

 type: string

 disUeNotif:

 type: boolean

 altSerReqs:

 type: array

 items:

 type: string

 minItems: 1

 contVer:

 $ref: '#/components/schemas/ContentVersion'

 codecs:

 type: array

 items:

 $ref: '#/components/schemas/CodecData'

 minItems: 1

 maxItems: 2

 desMaxLatency:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 desMaxLoss:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 flusId:

 type: string

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxPacketLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxSuppBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxSuppBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 medCompN:

 type: integer

 medSubComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaSubComponent'

 minProperties: 1

 description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

 medType:

 $ref: '#/components/schemas/MediaType'

 minDesBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minDesBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 preemptCap:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapability'

 preemptVuln:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerability'

 prioSharingInd:

 $ref: '#/components/schemas/PrioritySharingIndicator'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 rrBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 rsBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 sharingKeyDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sharingKeyUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 tsnQos:

 $ref: '#/components/schemas/TsnQosContainer'

 tscaiInputDl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiTimeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 MediaComponentRm:

 description: This data type is defined in the same way as the MediaComponent data type, but with the OpenAPI nullable property set to true

 type: object

 required:

 - medCompN

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirementRm'

 qosReference:

 type: string

 nullable: true

 altSerReqs:

 type: array

 items:

 type: string

 minItems: 1

 nullable: true

 disUeNotif:

 type: boolean

 contVer:

 $ref: '#/components/schemas/ContentVersion'

 codecs:

 type: array

 items:

 $ref: '#/components/schemas/CodecData'

 minItems: 1

 maxItems: 2

 desMaxLatency:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

 desMaxLoss:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

 flusId:

 type: string

 nullable: true

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxPacketLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxSuppBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxSuppBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 medCompN:

 type: integer

 medSubComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaSubComponentRm'

 minProperties: 1

 description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

 medType:

 $ref: '#/components/schemas/MediaType'

 minDesBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 minDesBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 preemptCap:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapabilityRm'

 preemptVuln:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerabilityRm'

 prioSharingInd:

 $ref: '#/components/schemas/PrioritySharingIndicator'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 rrBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 rsBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 sharingKeyDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

 sharingKeyUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

 tsnQos:

 $ref: '#/components/schemas/TsnQosContainerRm'

 tscaiInputDl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiTimeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 nullable: true

 MediaSubComponent:

 description: Identifies a media subcomponent

 type: object

 required:

 - fNum

 properties:

 afSigProtocol:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

 ethfDescs:

 type: array

 items:

 $ref: '#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 fNum:

 type: integer

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 tosTrCl:

 $ref: '#/components/schemas/TosTrafficClass'

 flowUsage:

 $ref: '#/components/schemas/FlowUsage'

 MediaSubComponentRm:

 description: This data type is defined in the same way as the MediaSubComponent data type, but with the OpenAPI nullable property set to true. Removable attributes marBwDl and marBwUl are defined with the corresponding removable data type.

 type: object

 required:

 - fNum

 properties:

 afSigProtocol:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

 ethfDescs:

 type: array

 items:

 $ref: '#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 nullable: true

 fNum:

 type: integer

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 nullable: true

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 tosTrCl:

 $ref: '#/components/schemas/TosTrafficClassRm'

 flowUsage:

 $ref: '#/components/schemas/FlowUsage'

 nullable: true

 EventsNotification:

 description: describes the notification of a matched event

 type: object

 required:

 - evSubsUri

 - evNotifs

 properties:

 adReports:

 type: array

 items:

 $ref: '#/components/schemas/AppDetectionReport'

 minItems: 1

 description: includes the detected application report.

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 addAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 relAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 anChargAddr:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AccNetChargingAddress'

 anChargIds:

 type: array

 items:

 $ref: '#/components/schemas/AccessNetChargingIdentifier'

 minItems: 1

 anGwAddr:

 $ref: '#/components/schemas/AnGwAddress'

 evSubsUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 evNotifs:

 type: array

 items:

 $ref: '#/components/schemas/AfEventNotification'

 minItems: 1

 failedResourcAllocReports:

 type: array

 items:

 $ref: '#/components/schemas/ResourcesAllocationInfo'

 minItems: 1

 succResourcAllocReports:

 type: array

 items:

 $ref: '#/components/schemas/ResourcesAllocationInfo'

 minItems: 1

 noNetLocSupp:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/NetLocAccessSupport'

 outOfCredReports:

 type: array

 items:

 $ref: '#/components/schemas/OutOfCreditInformation'

 minItems: 1

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 qncReports:

 type: array

 items:

 $ref: '#/components/schemas/QosNotificationControlInfo'

 minItems: 1

 qosMonReports:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 1

 ranNasRelCauses:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

 minItems: 1

 description: Contains the RAN and/or NAS release cause.

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 satBackhaulCategory:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SatelliteBackhaulCategory'

 ueLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueLocTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 usgRep:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 AfEventSubscription:

 description: describes the event information delivered in the subscription

 type: object

 required:

 - event

 properties:

 event:

 $ref: '#/components/schemas/AfEvent'

 notifMethod:

 $ref: '#/components/schemas/AfNotifMethod'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 waitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 AfEventNotification:

 description: describes the event information delivered in the notification

 type: object

 required:

 - event

 properties:

 event:

 $ref: '#/components/schemas/AfEvent'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 TerminationInfo:

 description: indicates the cause for requesting the deletion of the Individual Application Session Context resource

 type: object

 required:

 - termCause

 - resUri

 properties:

 termCause:

 $ref: '#/components/schemas/TerminationCause'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 AfRoutingRequirement:

 description: describes the event information delivered in the subscription

 type: object

 properties:

 appReloc:

 type: boolean

 routeToLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 spVal:

 $ref: '#/components/schemas/SpatialValidity'

 tempVals:

 type: array

 items:

 $ref: '#/components/schemas/TemporalValidity'

 minItems: 1

 upPathChgSub:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

 addrPreserInd:

 type: boolean

 simConnInd:

 type: boolean

 description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

 simConnTerm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 SpatialValidity:

 description: describes explicitly the route to an Application location

 type: object

 required:

 - presenceInfoList

 properties:

 presenceInfoList:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

 SpatialValidityRm:

 description: this data type is defined in the same way as the SpatialValidity data type, but with the OpenAPI nullable property set to true

 type: object

 required:

 - presenceInfoList

 properties:

 presenceInfoList:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

 nullable: true

 AfRoutingRequirementRm:

 description: this data type is defined in the same way as the AfRoutingRequirement data type, but with the OpenAPI nullable property set to true and the spVal and tempVals attributes defined as removable.

 type: object

 properties:

 appReloc:

 type: boolean

 routeToLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 nullable: true

 spVal:

 $ref: '#/components/schemas/SpatialValidityRm'

 tempVals:

 type: array

 items:

 $ref: '#/components/schemas/TemporalValidity'

 minItems: 1

 nullable: true

 upPathChgSub:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

 addrPreserInd:

 type: boolean

 nullable: true

 simConnInd:

 type: boolean

 nullable: true

 description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

 simConnTerm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 nullable: true

 AnGwAddress:

 description: describes the address of the access network gateway control node

 type: object

 anyOf:

 - required: [anGwIpv4Addr]

 - required: [anGwIpv6Addr]

 properties:

 anGwIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 anGwIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 Flows:

 description: Identifies the flows

 type: object

 required:

 - medCompN

 properties:

 contVers:

 type: array

 items:

 $ref: '#/components/schemas/ContentVersion'

 minItems: 1

 fNums:

 type: array

 items:

 type: integer

 minItems: 1

 medCompN:

 type: integer

 EthFlowDescription:

 description: Identifies an Ethernet flow

 type: object

 required:

 - ethType

 properties:

 destMacAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 ethType:

 type: string

 fDesc:

 $ref: '#/components/schemas/FlowDescription'

 fDir:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowDirection'

 sourceMacAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 vlanTags:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 2

 srcMacAddrEnd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 destMacAddrEnd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 ResourcesAllocationInfo:

 description: describes the status of the PCC rule(s) related to certain media components.

 type: object

 properties:

 mcResourcStatus:

 $ref: '#/components/schemas/MediaComponentResourcesStatus'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 altSerReq:

 type: string

 TemporalValidity:

 description: Indicates the time interval(s) during which the AF request is to be applied

 type: object

 properties:

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

 QosNotificationControlInfo:

 description: Indicates whether the QoS targets for a GRB flow are not guaranteed or guaranteed again

 type: object

 required:

 - notifType

 properties:

 notifType:

 $ref: '#/components/schemas/QosNotifType'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 altSerReq:

 type: string

#

 AcceptableServiceInfo:

 description: Indicates the maximum bandwidth that shall be authorized by the PCF.

 type: object

 properties:

 accBwMedComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponent'

 description: Indicates the maximum bandwidth that shall be authorized by the PCF for each media component of the map. The key of the map is the media component number.

 minProperties: 1

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 UeIdentityInfo:

 description: Represents 5GS-Level UE identities.

 type: object

 anyOf:

 - required: [gpsi]

 - required: [pei]

 - required: [supi]

 properties:

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

#

 AccessNetChargingIdentifier:

 description: Describes the access network charging identifier.

 type: object

 required:

 - accNetChaIdValue

 properties:

 accNetChaIdValue:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

#

 OutOfCreditInformation:

 description: Indicates the SDFs without available credit and the corresponding termination action.

 type: object

 required:

 - finUnitAct

 properties:

 finUnitAct:

 $ref: 'TS32291\_Nchf\_ConvergedCharging.yaml#/components/schemas/FinalUnitAction'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

#

 QosMonitoringInformation:

 description: Indicates the QoS Monitoring information to report, i.e. UL and/or DL and or round trip delay.

 type: object

 properties:

 repThreshDl:

 type: integer

 repThreshUl:

 type: integer

 repThreshRp:

 type: integer

#

#

 PduSessionTsnBridge:

 description: Contains the new TSC user plane node information and may contain the DS-TT port and/or NW-TT port management information.

 type: object

 required:

 - tsnBridgeInfo

 properties:

 tsnBridgeInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/TsnBridgeInfo'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

#

 QosMonitoringInformationRm:

 description: this data type is defined in the same way as the QosMonitoringInformation data type, but with the OpenAPI nullable property set to true.

 type: object

 properties:

 repThreshDl:

 type: integer

 repThreshUl:

 type: integer

 repThreshRp:

 type: integer

 nullable: true

#

 PcscfRestorationRequestData:

 description: Indicates P-CSCF restoration.

 type: object

 oneOf:

 - required: [ueIpv4]

 - required: [ueIpv6]

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ipDomain:

 type: string

 sliceInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

#

#

 QosMonitoringReport:

 description: QoS Monitoring reporting information

 type: object

 properties:

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 ulDelays:

 type: array

 items:

 type: integer

 minItems: 1

 dlDelays:

 type: array

 items:

 type: integer

 minItems: 1

 rtDelays:

 type: array

 items:

 type: integer

 minItems: 1

#

 TsnQosContainer:

 description: Indicates TSC Traffic QoS.

 type: object

 properties:

 maxTscBurstSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

 tscPackDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 tscPrioLevel:

 $ref: '#/components/schemas/TscPriorityLevel'

#

#

 TsnQosContainerRm:

 description: Indicates removable TSC Traffic QoS.

 type: object

 properties:

 maxTscBurstSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

 tscPackDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

 tscPrioLevel:

 $ref: '#/components/schemas/TscPriorityLevelRm'

 nullable: true

#

 TscaiInputContainer:

 description: Indicates TSC Traffic pattern.

 type: object

 properties:

 periodicity:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 burstArrivalTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 surTimeInNumMsg:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 surTimeInTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 nullable: true

#

#

 AppDetectionReport:

 description: Indicates the start or stop of the detected application traffic and the application identifier of the detected application traffic.

 type: object

 required:

 - adNotifType

 - afAppId

 properties:

 adNotifType:

 $ref: '#/components/schemas/AppDetectionNotifType'

 afAppId:

 $ref: '#/components/schemas/AfAppId'

#

 EventsSubscPutData:

 description: Identifies the events the application subscribes to within an Events Subscription sub-resource data. It may contain the notification of the already met events

 anyOf:

 - $ref: '#/components/schemas/EventsSubscReqData'

 - $ref: '#/components/schemas/EventsNotification'

#

# EXTENDED PROBLEMDETAILS

#

 ExtendedProblemDetails:

 description: Extends ProblemDetails to also include the acceptable service info.

 allOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - type: object

 properties:

 acceptableServInfo:

 $ref: '#/components/schemas/AcceptableServiceInfo'

#

# SIMPLE DATA TYPES

#

 AfAppId:

 description: Contains an AF application identifier.

 type: string

 AspId:

 description: Contains an identity of an application service provider.

 type: string

 CodecData:

 description: Contains codec related information.

 type: string

 ContentVersion:

 description: Represents the content version of some content.

 type: integer

 FlowDescription:

 description: Defines a packet filter of an IP flow.

 type: string

 SponId:

 description: Contains an identity of a sponsor.

 type: string

 ServiceUrn:

 description: Contains values of the service URN and may include subservices.

 type: string

 TosTrafficClass:

 description: 2-octet string, where each octet is encoded in hexadecimal representation. The first octet contains the IPv4 Type-of-Service or the IPv6 Traffic-Class field and the second octet contains the ToS/Traffic Class mask field.

 type: string

 TosTrafficClassRm:

 description: this data type is defined in the same way as the TosTrafficClass data type, but with the OpenAPI nullable property set to true

 type: string

 nullable: true

 TscPriorityLevel:

 description: Represents the priority level of TSC Flows.

 type: integer

 minimum: 1

 maximum: 8

 TscPriorityLevelRm:

 description: This data type is defined in the same way as the TscPriorityLevel data type, but with the OpenAPI nullable property set to true.

 type: integer

 minimum: 1

 maximum: 8

 nullable: true

#

# ENUMERATIONS DATA TYPES

#

 MediaType:

 description: Indicates the media type of a media component.

 anyOf:

 - type: string

 enum:

 - AUDIO

 - VIDEO

 - DATA

 - APPLICATION

 - CONTROL

 - TEXT

 - MESSAGE

 - OTHER

 - type: string

#

 MpsAction:

 anyOf:

 - type: string

 enum:

 - DISABLE\_MPS\_FOR\_DTS

 - ENABLE\_MPS\_FOR\_DTS

 - AUTHORIZE\_AND\_ENABLE\_MPS\_FOR\_DTS

 - type: string

#

 ReservPriority:

 description: Indicates the reservation priority.

 anyOf:

 - type: string

 enum:

 - PRIO\_1

 - PRIO\_2

 - PRIO\_3

 - PRIO\_4

 - PRIO\_5

 - PRIO\_6

 - PRIO\_7

 - PRIO\_8

 - PRIO\_9

 - PRIO\_10

 - PRIO\_11

 - PRIO\_12

 - PRIO\_13

 - PRIO\_14

 - PRIO\_15

 - PRIO\_16

 - type: string

#

 ServAuthInfo:

 description: Indicates the result of the Policy Authorization service request from the AF.

 anyOf:

 - type: string

 enum:

 - TP\_NOT\_KNOWN

 - TP\_EXPIRED

 - TP\_NOT\_YET\_OCURRED

 - ROUT\_REQ\_NOT\_AUTHORIZED

 - type: string

#

 SponsoringStatus:

 description: Indicates whether sponsored data connectivity is enabled or disabled/not enabled.

 anyOf:

 - type: string

 enum:

 - SPONSOR\_DISABLED

 - SPONSOR\_ENABLED

 - type: string

#

 AfEvent:

 description: Represents an event to notify to the AF.

 anyOf:

 - type: string

 enum:

 - ACCESS\_TYPE\_CHANGE

 - ANI\_REPORT

 - APP\_DETECTION

 - CHARGING\_CORRELATION

 - EPS\_FALLBACK

 - FAILED\_QOS\_UPDATE

 - FAILED\_RESOURCES\_ALLOCATION

 - OUT\_OF\_CREDIT

 - PLMN\_CHG

 - QOS\_MONITORING

 - QOS\_NOTIF

 - RAN\_NAS\_CAUSE

 - REALLOCATION\_OF\_CREDIT

 - SAT\_CATEGORY\_CHG

 - SUCCESSFUL\_QOS\_UPDATE

 - SUCCESSFUL\_RESOURCES\_ALLOCATION

 - TSN\_BRIDGE\_INFO

 - UP\_PATH\_CHG\_FAILURE

 - USAGE\_REPORT

 - type: string

#

 AfNotifMethod:

 description: Represents the notification methods that can be subscribed for an event.

 anyOf:

 - type: string

 enum:

 - EVENT\_DETECTION

 - ONE\_TIME

 - PERIODIC

 - PDU\_SESSION\_RELEASE

 - type: string

#

 QosNotifType:

 description: Indicates the notification type for QoS Notification Control.

 anyOf:

 - type: string

 enum:

 - GUARANTEED

 - NOT\_GUARANTEED

 - type: string

#

 TerminationCause:

 description: Indicates the cause behind requesting the deletion of the Individual Application Session Context resource.

 anyOf:

 - type: string

 enum:

 - ALL\_SDF\_DEACTIVATION

 - PDU\_SESSION\_TERMINATION

 - PS\_TO\_CS\_HO

 - INSUFFICIENT\_SERVER\_RESOURCES

 - INSUFFICIENT\_QOS\_FLOW\_RESOURCES

 - SPONSORED\_DATA\_CONNECTIVITY\_DISALLOWED

 - type: string

#

 MediaComponentResourcesStatus:

 description: Indicates whether the media component is active or inactive.

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

#

#

 FlowUsage:

 description: Describes the flow usage of the flows described by a media subcomponent.

 anyOf:

 - type: string

 enum:

 - NO\_INFO

 - RTCP

 - AF\_SIGNALLING

 - type: string

 FlowStatus:

 description: Describes whether the IP flow(s) are enabled or disabled.

 anyOf:

 - type: string

 enum:

 - ENABLED-UPLINK

 - ENABLED-DOWNLINK

 - ENABLED

 - DISABLED

 - REMOVED

 - type: string

#

 RequiredAccessInfo:

 description: Indicates the access network information required for an AF session.

 anyOf:

 - type: string

 enum:

 - USER\_LOCATION

 - UE\_TIME\_ZONE

 - type: string

#

 SipForkingIndication:

 description: Indicates whether several SIP dialogues are related to an "Individual Application Session Context" resource.

 anyOf:

 - type: string

 enum:

 - SINGLE\_DIALOGUE

 - SEVERAL\_DIALOGUES

 - type: string

#

 AfRequestedData:

 description: Represents the information that the AF requested to be exposed.

 anyOf:

 - type: string

 enum:

 - UE\_IDENTITY

 - type: string

#

 ServiceInfoStatus:

 description: Represents the preliminary or final service information status.

 anyOf:

 - type: string

 enum:

 - FINAL

 - PRELIMINARY

 - type: string

#

 PreemptionControlInformation:

 description: Represents Pre-emption control information.

 anyOf:

 - type: string

 enum:

 - MOST\_RECENT

 - LEAST\_RECENT

 - HIGHEST\_BW

 - type: string

#

 PrioritySharingIndicator:

 description: Represents the Priority sharing indicator.

 anyOf:

 - type: string

 enum:

 - ENABLED

 - DISABLED

 - type: string

#

 PreemptionControlInformationRm:

 description: This data type is defined in the same way as the PreemptionControlInformation data type, but with the OpenAPI nullable property set to true.

 anyOf:

 - $ref: '#/components/schemas/PreemptionControlInformation'

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

#

 AppDetectionNotifType:

 description: Indicates the notification type for Application Detection Control.

 anyOf:

 - type: string

 enum:

 - APP\_START

 - APP\_STOP

 - type: string

\*\*\* End of Changes \*\*\*