**3GPP TSG-CT WG3 Meeting #130 C3-234650**

**Xiamen, China, 9 - 13 October,2023 (Revision of C3-234321)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.580** | **CR** | **0043** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Notification events alighment with SA4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI18, 5MBS | | | | |  | ***Date:*** | | | 2023-09-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | SA4 TS 26.502 has further specified new Notification Events over interface Nmb10/Nmb5, and alignment has been done in the last meeting.  However, further study indicates that there are still misalignments between the SA4 and CT3. We illustrate the problem as the table below:   |  |  | | --- | --- | | CT3 implemented events | SA4 events over reference point Nmb10/Nmb5 | | USER\_DATA\_ING\_SESS\_STARTING |  | | USER\_DATA\_ING\_SESS\_STARTED | User Data Ingest Session established | | USER\_DATA\_ING\_SESS\_TERMINATED | User Data Ingest Session terminated | | DIST\_SESS\_STARTING | Distribution Session starting | | DIST\_SESS\_STARTED | Distribution Session established | | DIST\_SESS\_TERMINATED | Distribution Session deactivated | | DIST\_SESS\_SERV\_MNGT\_FAILURE | Distribution Session service management failure | | DIST\_SESS\_POL\_CRTL\_FAILURE | Distribution Session policy control failure | | DATA\_INGEST\_FAILURE | User data ingest failure | | DELIVERY\_STARTED | User Data Ingest Session established | | SESSION\_TERMINATED | User Data Ingest Session terminated | |  | session started | |  | session released | | DIST\_SESS\_ACTIVATED | Distribution Session activated | | DIST\_SESS\_DEACTIVATED | Distribution Session deactivated | | DIST\_SESS\_EST\_FAILURE | Distribution Session establishment failure | | DIST\_SESS\_ESTABLISHED | Distribution Session established | | USER\_SER\_AD | User Service advertisement |   We can conclude:   1. The highlighted green events are well aligned with the SA4 defined events 2. The highlighted event (USER\_DATA\_ING\_SESS\_STARTING) is defined in the stage 3 events but not defined in the SA4 events. 3. The two highlighted events (USER\_DATA\_ING\_SESS\_STARTED and DELIVERY\_STARTED) have different namings but the descriptions correspond to the same SA4 event of User Data Ingest Session Established. 4. The two highlighted events (USER\_DATA\_ING\_SESS\_TERMINATED and SESSION\_TERMINATED) have different namings but the descriptions correspond to the same SA4 event of User Data Ingest Session Terminated. 5. The two highlighed events (DIST\_SESS\_STARTED and DIST\_SESS\_ESTABLISHED) have different namings but the descriptions correspond to the same SA4 event of Distribution Session established. 6. The two highlighed events (DIST\_SESS\_TERMINATED and DIST\_SESS\_DEACTIVATED) have different namings but the descriptions can be interpreted as corresponding to the same SA4 event of Distribution Session deactivated. 7. The two highlighted events (Session started and Session released) indicating the MBS session is started/released are not defined in TS 29.580   Therefore, we proposed a modification to the Notification events and also clarify that the events are not one to one mapping between stage 3 and stage 2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | 1. Add NOTES to clarify the notification events 2. Add the two missing event in stage 3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Notification events are not aligned with SA4 requirements and cause implementation errors. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.6.3.4, A3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR has backward compatible corrections to the OpenAPI Nmbsf\_MBSUserDataIngestSession | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* First Change \*\*\*

##### 6.2.6.3.4 Enumeration: Event

The enumeration Event represents the MBS User Data Ingest Session Status events. It shall comply with the provisions of table 6.2.6.3.4-1.

Table 6.2.6.3.4-1: Enumeration Event

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| USER\_DATA\_ING\_SESS\_STARTING | Indicates that the MBS User Data Ingest Session is starting.  This is an "MBS User Data Ingest Session" level event. |  |
| USER\_DATA\_ING\_SESS\_STARTED | Indicates that the MBS User Data Ingest Session started. This corresponds to the “user data ingest session established” event defined in the clause 4.6.2 of 3GPP TS 26.502 [15].  This is an "MBS User Data Ingest Session" level event. |  |
| USER\_DATA\_ING\_SESS\_TERMINATED | Indicates that the MBS User Data Ingest Session is terminated.  This is an "MBS User Data Ingest Session" level event.  (NOTE) |  |
| DIST\_SESS\_STARTING | Indicates that the MBS Distribution Session is starting.  This is an "MBS Distribution Session" level event. |  |
| DIST\_SESS\_STARTED | Indicates that the MBS Distribution Session is established.  This is an "MBS Distribution Session" level event. |  |
| DIST\_SESS\_TERMINATED | Indicates that the MBS Distribution Session is deactivated.  This is an "MBS Distribution Session" level event. |  |
| DIST\_SESS\_SERV\_MNGT\_FAILURE | Indicates that the MBS Distribution Session could not be started (e.g. the necessary resources could not be allocated by the MBS system).  This is an "MBS Distribution Session" level event. |  |
| DIST\_SESS\_POL\_CRTL\_FAILURE | Indicates that the MBS Distribution Session could not be started because of a policy authorization/control failure or rejection.  This is an "MBS Distribution Session" level event. |  |
| DATA\_INGEST\_FAILURE | The MBS User Data Ingest failed because the MBSTF is expecting data (the MBS Session is active), but not receiving it.  This is an "MBS Distribution Session" level event. |  |
| DELIVERY\_STARTED | The MBS User Data delivery is started. |  |
| SESSION\_TERMINATED | The MBS User Data Ingest Session is terminated.  (NOTE) |  |
| SESSION\_STARTED | The MBS Session is started. | EventExt |
| SESSION\_RELEASED | The MBS Session is released. | EventExt |
| DIST\_SESS\_ACTIVATED | The MBS Distribution Session is activated successfully. | EventExt |
| DIST\_SESS\_EST\_FAILURE | Indicates that the MBSF failed to establish the MBS Distribution Session at the MBSTF.  This is an “MBS Distribution Session" level event. | EventExt |
| USER\_SER\_AD | Indicates that the MBSF advertises the User Service Announcement information to the MBS Application Provider. | EventExt |
| NOTE: These two enumeration values correspond to the same event, which is defined in the clause 4.6.2 of 3GPP TS 26.502 [15]. |

\*\*\* Next Change \*\*\*

# A.3 Nmbsf\_MBSUserDataIngestSession API

openapi: 3.0.0

info:

title: nmbsf-mbs-ud-ingest

version: 1.1.0-alpha.4

description: |

API for MBS User Data Ingest Session Service.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.580 V18.3.0; 5G System; Multicast/Broadcast Service Function Services.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.580/'

servers:

- url: '{apiRoot}/nmbsf-mbs-ud-ingest/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials: []

paths:

/sessions:

get:

summary: Retrieve all the active MBS User Data Ingest Sessions managed by the MBSF.

tags:

- MBS User Data Ingest Sessions (Collection)

operationId: RetrieveMBSUserDataIngSessions

responses:

'200':

description: >

OK. All the active MBS User Data Ingest Sessions managed by the MBSF are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MBSUserDataIngSession'

minItems: 0

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

post:

summary: Request the creation of a new MBS User Data Ingest Session.

tags:

- MBS User Data Ingest Sessions (Collection)

operationId: CreateMBSUserDataIngSession

requestBody:

description: >

Contains the parameters to request the creation of a new MBS User Data Ingest Session

at the MBSF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

responses:

'201':

description: >

Created. A new MBS User Data Ingest Session is successfully created and a representation

of the created Individual MBS User Data Ingest Session resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nmbs-mbs-ud-ingest/v1/sessions/{sessionId}

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sessions/{sessionId}:

parameters:

- name: sessionId

in: path

description: Identifier of the Individual MBS User Data Ingest Session resource.

required: true

schema:

type: string

get:

summary: Retrieve an existing Individual MBS User Data Ingest Session resource.

tags:

- Individual MBS User Data Ingest Session (Document)

operationId: RetrieveIndMBSUserDataIngSession

responses:

'200':

description: >

OK. The requested Individual MBS User Data Ingest Session resource is successfully

returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Request the update of an existing Individual MBS User Data Ingest Session resource.

tags:

- Individual MBS User Data Ingest Session (Document)

operationId: UpdateIndMBSUserDataIngSession

requestBody:

description: >

Contains the updated representation of the Individual MBS User Data Ingest Session

resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

responses:

'200':

description: >

OK. The concerned Individual MBS User Data Ingest Session resource is successfully

updated and a representation of the updated resource is returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

'204':

description: >

No Content. The concerned Individual MBS User Data Ingest Session resource is

successfully updated and no content is returned in the response body.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Request the modification of an existing Individual MBS User Data Ingest Session resource.

tags:

- Individual MBS User Data Ingest Session (Document)

operationId: ModifyIndMBSUserDataIngSession

requestBody:

description: >

Contains the parameters to request the modification of the Individual MBS User Data Ingest

Session resource.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSessionPatch'

responses:

'200':

description: >

OK. The concerned Individual MBS User Data Ingest Session resource is successfully

modified and a representation of the updated resource is returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngSession'

'204':

description: >

No Content. The concerned Individual MBS User Data Ingest Session resource is

successfully modified and no content is returned in the response body.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Request the deletion of an existing Individual MBS User Data Ingest Session resource.

tags:

- Individual MBS User Data Ingest Session (Document)

operationId: DeleteIndMBSUserDataIngSession

responses:

'204':

description: >

No Content. The Individual MBS User Data Ingest Session resource is successfully

deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/status-subscriptions:

get:

summary: Retrieve all the active MBS User Data Ingest Session Status Subscription resources managed by the MBSF.

tags:

- MBS User Data Ingest Session Status Subscriptions (Collection)

operationId: RetrieveMBSUserDataIngStatSubscs

responses:

'200':

description: >

OK. All the active MBS User Data Ingest Session Status Subscriptions managed by the MBSF

are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

minItems: 0

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

post:

summary: Request the creation of a new MBS User Data Ingest Session Status Subscription.

tags:

- MBS User Data Ingest Session Status Subscriptions (Collection)

operationId: CreateMBSUserDataIngStatSubsc

requestBody:

description: >

Contains the parameters to request the creation of a new MBS User Data Ingest Session

Status Subscription.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

responses:

'201':

description: >

Created. Successful creation of a new Individual MBS User Data Ingest Session

Status Subscription resource.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

headers:

Location:

description: >

Contains the URI of the newly created resource, according to the structure

{apiRoot}/nmbs-mbs-ud-ingest/v1/status-subscriptions/{subscriptionId}

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

mbsUserDataIngestSessionStatusNotif:

'{request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatNotif'

responses:

'204':

description: No Content. Successful reception of the notification.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/status-subscriptions/{subscriptionId}:

parameters:

- name: subscriptionId

in: path

description: >

Identifier of the Individual MBS User Data Ingest Session Status Subscription resource.

required: true

schema:

type: string

get:

summary: Retrieve an existing Individual MBS User Data Ingest Session Status Subscription resource.

tags:

- Individual MBS User Data Ingest Session Status Subscription (Document)

operationId: RetrieveIndMBSUserDataIngStatSubsc

responses:

'200':

description: >

OK. Successful retrieval of the requested Individual MBS User Data Ingest Session

Status Subscription resource.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Request the update of an existing Individual MBS User Data Ingest Session Status Subscription resource.

tags:

- Individual MBS User Data Ingest Session Status Subscription (Document)

operationId: UpdateIndMBSUserDataIngStatSubsc

requestBody:

description: >

Contains the updated representation of the Individual MBS User Data Ingest Session Status

Subscription resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

responses:

'200':

description: >

OK. The concerned Individual MBS User Data Ingest Session Status Subscription resource

is successfully updated and a representation of the updated resource is returned in the

response body.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

'204':

description: >

No Content. The concerned Individual MBS User Data Ingest Session Status Subscription

resource is successfully updated and no content is returned in the response body.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Request the modification of an existing Individual MBS User Data Ingest Session Status Subscription resource.

tags:

- Individual MBS User Data Ingest Session Status Subscription (Document)

operationId: ModifyIndMBSUserDataIngStatSubsc

requestBody:

description: >

Contains the parameters to request the modification of the Individual MBS User Data Ingest

Session Status Subscription resource.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubscPatch'

responses:

'200':

description: >

OK. The concerned Individual MBS User Data Ingest Session Status Subscription resource

is successfully modified and a representation of the updated resource is returned in the

response body.

content:

application/json:

schema:

$ref: '#/components/schemas/MBSUserDataIngStatSubsc'

'204':

description: >

No Content. The concerned Individual MBS User Data Ingest Session Status Subscription

resource is successfully modified and no content is returned in the response body.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Request the deletion of an existing Individual MBS User Data Ingest Session Status Subscription resource.

tags:

- Individual MBS User Data Ingest Session Status Subscription (Document)

operationId: DeleteMBSUserDataIngStatSubsc

responses:

'204':

description: >

No Content. Successful deletion of the existing Individual MBS User Data Ingest Session

Status Subscription resource.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

description: >

When the Nmbsf\_MBSUserDataIngestSession is consumed by a trusted or internal AF, then

'nmbsf-mbs-ud-ingest' shall be used as the scope (i.e. with the 'scopes' property) and

'{nrfApiRoot}/oauth2/token' shall be used as the URI to retrieve the token

(i.e. 'tokenUri').

#

# STRUCTURED DATA TYPES

#

schemas:

MBSUserDataIngSession:

description: Represents MBS User Data Ingest Session information.

type: object

properties:

mbsUserServId:

type: string

mbsDisSessInfos:

type: object

additionalProperties:

$ref: '#/components/schemas/MBSDistributionSessionInfo'

minProperties: 1

nullable: true

description: >

Represents one or more MBS Distribution Session(s) composing the MBS User Data Ingest

Session.

The key of the map shall be any unique string encoded value.

actPeriods:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

minItems: 1

mbsUserServAnmt:

$ref: '#/components/schemas/MBSUserServAnmt'

mbsUserServiceAnmt:

$ref: 'TS26517\_MBSUserServiceAnnouncement.yaml#/components/schemas/UserServiceDescription'

mbsUserServiceAnmtUrl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- mbsUserServId

- mbsDisSessInfos

MBSDistributionSessionInfo:

description: Represents MBS Distribution Session information.

type: object

properties:

mbsDistSessionId:

type: string

mbsDistSessState:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/DistSessionState'

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

associatedSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AssociatedSessionId'

mbsServInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceInfo'

maxContBitRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxContDelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

distrMethod:

$ref: '#/components/schemas/DistributionMethod'

fecConfig:

$ref: '#/components/schemas/FECConfig'

objDistrInfo:

$ref: '#/components/schemas/ObjectDistrMethInfo'

pckDistrInfo:

$ref: '#/components/schemas/PacketDistrMethInfo'

trafficMarkingInfo:

type: string

tgtServAreas:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceArea'

extTgtServAreas:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalMbsServiceArea'

mbsFSAId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsFsaId'

locationDependent:

type: boolean

description: >

Represents an indication that this MBS Distribution Session belongs to a location-

dependent MBS. This attribute shall be set to "true" to indicate that the MBS

Distribution Session belongs to a location-dependent MBS; or set to "false" to

indicate that the MBS Distribution Session does not belong to a location-dependent MBS.

The default value is "false", if omitted.

default: false

multiplexedServFlag:

type: boolean

description: >

Represents an indication that this MBS Distribution Session belongs to a multiplex, i.e.

forms part of a set of MBS Distribution Sessions under the same parent MBS User Data

Ingest Session with identical or empty sets of target service areas and multiplexed onto

the same MBS Session at the MB-SMF.

default: false

restrictedFlag:

type: boolean

description: >

Represents an indication that this MBS Distribution Session is not open to any UE, i.e.

restricted to a set of UEs according to their MBS related subscription information.

This attribute may be included only if the parent MBS User Service is of Multicast

service type. This attribute shall be set to "true" to indicate that this MBS

Distribution Session is restricted to a set of UE(s); or set to "false" to indicate that

this MBS Distribution Session is open to any UE.

The default value is "false", if omitted.

default: false

required:

- distrMethod

- maxContBitRate

MBSUserDataIngSessionPatch:

description: >

Represents the requested modifications to an MBS User Data Ingest Session Status

Subscription.

type: object

properties:

mbsDisSessInfos:

type: object

additionalProperties:

$ref: '#/components/schemas/MBSDistributionSessionInfo'

minProperties: 1

nullable: true

description: >

Contains the requested modifications to one or more MBS Distribution Session(s)

composing the MBS User Data Ingest Session.

The key of the map shall be any unique string encoded value.

actPeriods:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

minItems: 1

ObjectDistrMethInfo:

description: >

Represents additional MBS Distribution Session parameters for the case of an Object

Distribution Method.

type: object

properties:

operatingMode:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/ObjDistributionOperatingMode'

objAcqMethod:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/ObjAcquisitionMethod'

objAcqIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 0

objIngUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

objDistrUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

objRepairUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

required:

- operatingMode

- objAcqMethod

- objAcqIds

PacketDistrMethInfo:

description: >

Represents additional MBS Distribution Session parameters for the case of Packet

Distribution Method.

type: object

properties:

operatingMode:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/PktDistributionOperatingMode'

pckIngMethod:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/PktIngestMethod'

ingEndpointAddrs:

$ref: 'TS29581\_Nmbstf\_DistSession.yaml#/components/schemas/MbStfIngestAddr'

required:

- operatingMode

- pckIngMethod

- ingEndpointAddrs

MBSUserDataIngStatSubsc:

description: >

Represents an MBS User Data Ingest Session Status Subscription.

type: object

properties:

mbsIngSessionId:

type: string

eventSubscs:

type: array

items:

$ref: '#/components/schemas/SubscribedEvent'

minItems: 1

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

required:

- mbsIngSessionId

- eventSubscs

- notifUri

MBSUserDataIngStatSubscPatch:

description: >

Represents the requested modifications to an MBS User Data Ingest Session Status

Subscription.

type: object

properties:

eventSubscs:

type: array

items:

$ref: '#/components/schemas/SubscribedEvent'

minItems: 1

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

SubscribedEvent:

description: >

Represents a subscribed MBS User Data Ingest Session Status event and the related

information.

type: object

properties:

statusEvent:

$ref: '#/components/schemas/Event'

mbsDistSessionId:

type: string

required:

- statusEvent

MBSUserDataIngStatNotif:

description: >

Represents an MBS User Data Ingest Session Status Notification.

type: object

properties:

mbsIngSessionId:

type: string

eventNotifs:

type: array

items:

$ref: '#/components/schemas/EventNotification'

minItems: 1

required:

- mbsIngSessionId

- eventNotifs

EventNotification:

description: Represents Event Notification.

type: object

properties:

statusEvent:

$ref: '#/components/schemas/Event'

mbsDisSessionId:

type: string

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

statusAddInfo:

type: string

timeStamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- statusEvent

- timeStamp

MBSUserServAnmt:

deprecated: true

description: >

Represents the MBS User Service Announcement currently associated with the MBS User Data

Ingest Session.

type: object

properties:

extServiceId:

type: array

items:

type: string

minItems: 1

servClass:

type: string

startTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

endTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

servNameDescs:

type: array

items:

$ref: 'TS29580\_Nmbsf\_MBSUserService.yaml#/components/schemas/ServiceNameDescription'

minItems: 1

mainServLang:

type: string

mbsDistSessAnmt:

additionalProperties:

$ref: '#/components/schemas/MBSDistSessionAnmt'

minProperties: 1

description: >

Represents the set of MBS Distribution Session Announcements currently associated with

this MBS User Service Announcement.

required:

- extServiceId

- servClass

- servNameDescs

MBSDistSessionAnmt:

description: >

Represents the set of MBS Distribution Session Announcements currently associated with this

MBS User Service Announcement.

type: object

properties:

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

mbsFSAId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsFsaId'

distrMethod:

$ref: '#/components/schemas/DistributionMethod'

objDistrAnnInfo:

$ref: '#/components/schemas/ObjectDistMethAnmtInfo'

sesDesInfo:

type: array

items:

type: string

minItems: 1

required:

- distrMethod

- sesDesInfo

ObjectDistMethAnmtInfo:

description: >

Represents MBS Distribution Session Announcement parameters for Object Distribution Method.

type: object

properties:

objDistrSched:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

objDistrBaseUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

objRepBaseUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

FECConfig:

description: Represents FEC configuration information.

type: object

properties:

fecScheme:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

fecOverHead:

type: integer

additionalParams:

type: array

items:

$ref: '#/components/schemas/AddFecParams'

minItems: 1

required:

- fecScheme

- fecOverHead

AddFecParams:

description: Represents additional scheme-specific parameters for AL-FEC configuration.

type: object

properties:

paramName:

type: string

paramValue:

type: string

required:

- paramName

- paramValue

# SIMPLE DATA TYPES

#

#

# ENUMERATIONS

#

DistributionMethod:

anyOf:

- type: string

enum:

- OBJECT

- PACKET

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the MBS Distribution method.

Possible values are:

- OBJECT: Indicates the Object Distribution Method.

- PACKET: Indicates the Packet Distribution Method.

Event:

anyOf:

- type: string

enum:

- USER\_DATA\_ING\_SESS\_STARTING

- USER\_DATA\_ING\_SESS\_STARTED

- USER\_DATA\_ING\_SESS\_TERMINATED

- DIST\_SESS\_STARTING

- DIST\_SESS\_STARTED

- DIST\_SESS\_TERMINATED

- DIST\_SESS\_SERV\_MNGT\_FAILURE

- DIST\_SESS\_POL\_CRTL\_FAILURE

- DATA\_INGEST\_FAILURE

- DELIVERY\_STARTED

- SESSION\_TERMINATED

- SESSION\_STARTED

- SESSION\_RELEASED

- DIST\_SESS\_ACTIVATED

- DIST\_SESS\_EST\_FAILURE

- USER\_SER\_AD

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the MBS User Data Ingest Session Status events.

Possible values are:

- USER\_DATA\_ING\_SESS\_STARTING: >

Indicates that the MBS User Data Ingest Session is starting. This is an "MBS User Data

Ingest Session" level event.

- USER\_DATA\_ING\_SESS\_STARTED: >

Indicates that the MBS User Data Ingest Session started. This is an "MBS User Data

Ingest Session" level event.

- USER\_DATA\_ING\_SESS\_TERMINATED: >

Indicates that the MBS User Data Ingest Session is terminated. This is an "MBS User Data

Ingest Session" level event.

- DIST\_SESS\_STARTING: >

Indicates that the MBS Distribution Session is starting. This is an "MBS Distribution

Session" level event.

- DIST\_SESS\_STARTED: >

Indicates that the MBS Distribution Session started. This is an "MBS Distribution

Session" level event.

- DIST\_SESS\_TERMINATED: >

Indicates that the MBS Distribution Session is terminated. This is an "MBS Distribution

Session" level event.

- DIST\_SESS\_SERV\_MNGT\_FAILURE: >

Indicates that the MBS Distribution Session could not be started (e.g. the necessary

resources could not be allocated by the MBS system). This is an "MBS Distribution

Session" level event.

- DIST\_SESS\_POL\_CRTL\_FAILURE: >

Indicates that the MBS Distribution Session could not be started because of a policy

authorization/control failure or rejection. This is an "MBS Distribution Session"

level event.

- DATA\_INGEST\_FAILURE: >

The MBS User Data Ingest is failed because the MBSTF is expecting data (the MBS Session

is active), but not receiving it. This is an "MBS Distribution Session" level event.

- DELIVERY\_STARTED: >

The MBS User Data delivery is started.

- SESSION\_TERMINATED: >

The MBS User Data Ingest Session is terminated.

- SESSION\_STARTED: >

The MBS Session is started.

- SESSION\_RELEASED: >

The MBS Session is released.

- DIST\_SESS\_ACTIVATED:

Indicates that the MBS Distribution Session is activated successfully.

- DIST\_SESS\_EST\_FAILURE:

Indicates that the MBSF failed to successfully establish the MBS Distribution Session at

the MBSTF. This is an "MBS Distribution Session" level event.

- USER\_SER\_AD:

Indicates that the MBSF advertises the User Service Announcement information to the MBS

Application Provider.

\*\*\* End of Changes \*\*\*