**3GPP TSG-CT WG3 Meeting #131 *C3-235xxx***

**Chicago, United States, 13 - 17 November, 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.508** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **16.11.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction of anyUeInd attribute | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GS\_Ph1-CT | | | | |  | ***Date:*** | | | 2023-11-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The boolean value of anyUeInd attribute is not defined in Table 5.6.2.2-1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The boolean value of anyUeInd attribute is defined. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.6.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR has no impact to the openAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.6.2.2 Type NsmfEventExposure

Table 5.6.2.2-1: Definition of type NsmfEventExposure

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | | P | Cardinality | | Description | | Applicability | |
| supi | | Supi | | | C | 0..1 | | Subscription Permanent Identifier (NOTE 1) | |  | |
| gpsi | | Gpsi | | | C | 0..1 | | Generic Public Subscription Identifier (NOTE 1) | |  | |
| anyUeInd | | boolean | | | C | 0..1 | | This IE shall be present if the event subscription is applicable to any UE.  It indicates whether the event subscription is applicable to any UE:  - true: applicable  - false(default): not applicable. (NOTE 1) | |  | |
| groupId | | GroupId | | | C | 0..1 | | Identifies a group of UEs. (NOTE 1) | |  | |
| pduSeId | | PduSessionId | | | C | 0..1 | | PDU session ID (NOTE 1) | |  | |
| dnn | | Dnn | | O | 0..1 | | | Data Network Name. | |  | |
| snssai | | Snssai | | O | 0..1 | | | A single Network Slice Selection Assistance Information. | |  | |
| subId | | SubId | | | C | 0..1 | | Subscription ID. This parameter shall be supplied by the SMF in HTTP responses that include an object of NsmfEventExposure type. | |  | |
| notifId | | string | | | M | 1 | | Notification Correlation ID provided by the NF service consumer. (NOTE 2) | |  | |
| notifUri | | Uri | | | M | 1 | | Identifies the recipient of Notifications sent by the SMF. | |  | |
| altNotifIpv4Addrs | | array(Ipv4Addr) | | | O | 1..N | | Alternate or backup IPv4 Address(es) where to send Notifications. | |  | |
| altNotifIpv6Addrs | | array(Ipv6Addr) | | | O | 1..N | | Alternate or backup IPv6 Address(es) where to send Notifications. | |  | |
| altNotifFqdns | | array(Fqdn) | | | O | 1..N | | Alternate or backup FQDN(s) where to send Notifications. | |  | |
| eventSubs | | array(EventSubscription) | | | M | 1..N | | Subscribed events | |  | |
| ImmeRep | | boolean | | | O | 0..1 | | It is included and set to true if the immediate reporting of the current status of the subscribed event, if available is required. | |  | |
| notifMethod | | NotificationMethod | | | O | 0..1 | | If "notifMethod" is not supplied, the default value "ON\_EVENT\_DETECTION" applies. | |  | |
| maxReportNbr | | Uinteger | | | O | 0..1 | | If omitted, there is no limit. | |  | |
| expiry | | DateTime | | | C | 0..1 | | This attribute indicates the expiry time of the subscription, after which the SMF shall not send any event notifications and the subscription becomes invalid. It may be included in an event subscription request and may be included in an event subscription response based on operator policies. If an expiry time was included in the request, then the expiry time returned in the response should be less than or equal to that value. If the expiry time is not included in the response, the NF Service Consumer shall not associate an expiry time for the subscription. | |  | |
| repPeriod | | DurationSec | | | C | 0..1 | | Is supplied for notification Method "periodic". | |  | |
| guami | | Guami | | | C | 0..1 | | The Globally Unique AMF Identifier (GUAMI) shall be provided by an AMF as service consumer. | |  | |
| serviceName | | ServiceName | | | O | 0..1 | | If the NF service consumer is an AMF, it should provide the name of a service produced by the AMF that makes use of the notification about subscribed events. | |  | |
| supportedFeatures | | SupportedFeatures | | | C | 0..1 | | List of Supported features used as described in subclause 5.8.  This parameter shall be supplied by NF service consumer and SMF in the POST request that request the creation of an SMF Notification Subscriptions resource and the related reply, respectively. | |  | |
| sampRatio | | SamplingRatio | | | O | 0..1 | | Indicates the ratio of the random subset to target UEs, event reports only relates to the subset. | |  | |
| grpRepTime | | DurationSec | | | O | 0..1 | | Indicates the time for which the SMF aggregates the event reports detected by the UEs in a group and report them together to the NF service consumer. | |  | |
| NOTE 1: If the event subscription applies for a specific PDU session, the PDU session of a single UE (pduSeId, and gpsi/supi) shall be included; otherwise one and only one of a single UE (gpsi/supi), a group of UEs (groupId), or anyUeInd set to true shall be included.  NOTE 2: If the UDM as NF service consumer subscribes to event (e.g. downlink data delivery status, PDU Session Establishment, PDU Session Release) on behalf of AF/NEF, "notifId" shall be set the same as "referenceId" received from the AF/NEF as defined in subclause 6.4.6.2.4 of 3GPP TS 29.503 [14]. | | | | | | | | | | | |

\*\*\* End of Changes \*\*\*