**3GPP TSG-CT WG4 Meeting #111-eC4-224xxx**

**E-Meeting, 18th – 26th August 2022** *Revision of C4-224152*

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.510** | **CR** | **0734** | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Removing an editor's note | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | SBIProtoc17 | | | | |  | ***Date:*** | | | 2022-08-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Clause 6.1.6.1 contains the following editor's note: "A general solution of NRF handling towards absent attributes (not registered by the NF or not supported by NF with early version) is FFS". CT4 however chose not to address the matter at least in Rel-17 timeframe. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Editor's note is removed from clause 6.1.6.1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Editors' note remains in 3GPP Rel-17 version of the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.1.6.1. | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not alter OpenAPIs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev1: Cover sheet is corrected. | | | | | | | | |

\* \* \* First Change \* \* \* \*

### 6.1.6 Data Model

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nnrf\_NFManagement service-based interface protocol.

Table 6.1.6.1-1: Nnrf\_NFManagement specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| NFProfile | 6.1.6.2.2 | Information of an NF Instance registered in the NRF. |
| NFService | 6.1.6.2.3 | Information of a given NF Service Instance; it is part of the NFProfile of an NF Instance. |
| DefaultNotificationSubscription | 6.1.6.2.4 | Data structure for specifying the notifications the NF service subscribes by default along with callback URI. |
| IpEndPoint | 6.1.6.2.5 | IP addressing information of a given NFService; it consists on, e.g. IP address, TCP port, transport protocol... |
| UdrInfo | 6.1.6.2.6 | Information of an UDR NF Instance. |
| UdmInfo | 6.1.6.2.7 | Information of an UDM NF Instance. |
| AusfInfo | 6.1.6.2.8 | Information of an AUSF NF Instance. |
| SupiRange | 6.1.6.2.9 | A range of SUPIs (subscriber identities), either based on a numeric range, or based on regular-expression matching. |
| IdentityRange | 6.1.6.2.10 | A range of subscriber identities, either based on a numeric range, or based on regular-expression matching. |
| AmfInfo | 6.1.6.2.11 | Information of an AMF NF Instance. |
| SmfInfo | 6.1.6.2.12 | Information of an SMF NF Instance. |
| UpfInfo | 6.1.6.2.13 | Information of an UPF NF Instance. |
| SnssaiUpfInfoItem | 6.1.6.2.14 | Set of parameters supported by UPF for a given S-NSSAI. |
| DnnUpfInfoItem | 6.1.6.2.15 | Set of parameters supported by UPF for a given DNN. |
| SubscriptionData | 6.1.6.2.16 | Information of a subscription to notifications to NRF events, included in subscription requests and responses. |
| NotificationData | 6.1.6.2.17 | Data sent in notifications from NRF to subscribed NF Instances. |
| NFServiceVersion | 6.1.6.2.19 | Contains the version details of an NF service. |
| PcfInfo | 6.1.6.2.20 | Information of a PCF NF Instance. |
| BsfInfo | 6.1.6.2.21 | Information of a BSF NF Instance. |
| Ipv4AddressRange | 6.1.6.2.22 | Range of IPv4 addresses. |
| Ipv6PrefixRange | 6.1.6.2.23 | Range of IPv6 prefixes. |
| InterfaceUpfInfoItem | 6.1.6.2.24 | Information of a given IP interface of an UPF. |
| UriList | 6.1.6.2.25 | Set of URIs following 3GPP hypermedia format (containing a "\_links" attribute). |
| N2InterfaceAmfInfo | 6.1.6.2.26 | AMF N2 interface information |
| TaiRange | 6.1.6.2.27 | Range of TAIs (Tracking Area Identities). |
| TacRange | 6.1.6.2.28 | Range of TACs (Tracking Area Codes). |
| SnssaiSmfInfoItem | 6.1.6.2.29 | Set of parameters supported by SMF for a given S-NSSAI. |
| DnnSmfInfoItem | 6.1.6.2.30 | Set of parameters supported by SMF for a given DNN. |
| NrfInfo | 6.1.6.2.31 | Information of an NRF NF Instance, used in hierarchical NRF deployments. |
| ChfInfo | 6.1.6.2.32 | Information of a CHF NF Instance. |
| PlmnRange | 6.1.6.2.34 | Range of PLMN IDs. |
| SubscrCond | 6.1.6.2.35 | Condition to determine the set of NFs to monitor under a certain subscription in NRF. |
| NfInstanceIdCond | 6.1.6.2.36 | Subscription to a given NF Instance Id. |
| NfTypeCond | 6.1.6.2.37 | Subscription to a set of NFs based on their NF Type. |
| ServiceNameCond | 6.1.6.2.38 | Subscription to a set of NFs based on their support for a given Service Name. |
| AmfCond | 6.1.6.2.39 | Subscription to a set of AMFs, based on AMF Set Id and/or AMF Region Id. |
| GuamiListCond | 6.1.6.2.40 | Subscription to a set of AMFs, based on their GUAMIs. |
| NetworkSliceCond | 6.1.6.2.41 | Subscription to a set of NFs, based on the slices (S-NSSAI and NSI) they support . |
| NfGroupCond | 6.1.6.2.42 | Subscription to a set of NFs based on their Group Id. |
| NotifCondition | 6.1.6.2.43 | Condition (list of attributes in the NF Profile) to determine whether a notification must be sent by NRF. |
| PlmnSnssai | 6.1.6.2.44 | List of network slices (S-NSSAIs) for a given PLMN ID. |
| NwdafInfo | 6.1.6.2.45 | Information of a NWDAF NF Instance. |
| LmfInfo | 6.1.6.2.46 | Information of an LMF NF Instance. |
| GmlcInfo | 6.1.6.2.47 | Information of a GMLC NF Instance. |
| NefInfo | 6.1.6.2.48 | Information of an NEF NF Instance. |
| PfdData | 6.1.6.2.49 | List of Application IDs and/or AF IDs managed by a given NEF Instance. |
| AfEventExposureData | 6.1.6.2.50 | AF Event Exposure data managed by a given NEF Instance. |
| WAgfInfo | 6.1.6.2.51 | Information of the W-AGF endpoints. |
| TngfInfo | 6.1.6.2.52 | Information of the TNGF endpoints. |
| PcscfInfo | 6.1.6.2.53 | Information of a P-CSCF NF Instance. |
| NfSetCond | 6.1.6.2.54 | Subscription to a set of NFs based on their Set Id. |
| NfServiceSetCond | 6.1.6.2.55 | Subscription to a set of NFs based on their Service Set Id. |
| NfInfo | 6.1.6.2.56 | Information of a generic NF Instance. |
| HssInfo | 6.1.6.2.57 | Information of an HSS NF Instance. |
| ImsiRange | 6.1.6.2.58 | A range of IMSIs (subscriber identities), either based on a numeric range, or based on regular-expression matching. |
| InternalGroupIdRange | 6.1.6.2.59 | A range of Group IDs (internal group identities), either based on a numeric range, or based on regular-expression matching. |
| UpfCond | 6.1.6.2.60 | Subscription to a set of NF Instances (UPFs), able to serve a certain service area (i.e. SMF serving area or TAI list). |
| TwifInfo | 6.1.6.2.61 | Addressing information (IP addresses, FQDN) of the TWIF. |
| VendorSpecificFeature | 6.1.6.2.62 | Information about a vendor-specific feature |
| UdsfInfo | 6.1.6.2.63 | Information related to UDSF |
| ScpInfo | 6.1.6.2.65 | Information of an SCP Instance |
| ScpDomainInfo | 6.1.6.2.66 | SCP domain information |
| ScpDomainCond | 6.1.6.2.67 | Subscription to an SCP domain |
| OptionsResponse | 6.1.6.2.68 | Communication options of the NRF |
| NwdafCond | 6.1.6.2.69 | Subscription to a set of NF Instances (NWDAFs), identified by Analytics ID(s), S-NSSAI(s) or NWDAF Serving Area information, i.e. list of TAIs for which the NWDAF can provide analytics. |
| NefCond | 6.1.6.2.70 | Subscription to a set of NF Instances (NEFs), identified by Event ID(s) provided by AF, S-NSSAI(s), AF Instance ID, Application Identifier, External Identifier, External Group Identifier, or domain name. |
| SuciInfo | 6.1.6.2.71 | SUCI information containing Routing Indicator and Home Network Public Key ID. |
| SeppInfo | 6.1.6.2.72 | Information of a SEPP Instance |
| AanfInfo | 6.1.6.2.73 | Information of an AAnF NF Instance. |
| 5GDdnmfInfo | 6.1.6.2.74 | Information of a 5G DDNMF NF Instance. |
| MfafInfo | 6.1.6.2.75 | Information of the MFAF NF Instance. |
| NwdafCapability | 6.1.6.2.76 | Indicates the capability supported by the NWDAF. |
| DccfInfo | 6.1.6.2.80 | Information of a DCCF NF Instance. |
| NsacfInfo | 6.1.6.2.81 | Information of an NSACF NF Instance. |
| NsacfCapability | 6.1.6.2.82 | NSACF service capability. |
| DccfCond | 6.1.6.2.83 | Subscription to a set of NF Instances (DCCFs), identified by NF types, NF Set Id(s) or DCCF Serving Area information, i.e. list of TAIs served by the DCCF. |
| MlAnalyticsInfo | 6.1.6.2.84 | ML Analytics Filter information supported by the Nnwdaf\_MLModelProvision service |
| MbSmfInfo | 6.1.6.2.85 | Information of a MB-SMF NF Instance |
| TmgiRange | 6.1.6.2.86 | Range of TMGIs |
| MbsSession | 6.1.6.2.87 | MBS Session served by an MB-SMF |
| SnssaiMbSmfInfoItem | 6.1.6.2.88 | Parameters supported by an MB-SMF for a given S-NSSAI |
| DnnMbSmfInfoItem | 6.1.6.2.89 | Parameters supported by an MB-SMF for a given DNN |
| TsctsfInfo | 6.1.6.2.91 | Information of a TSCTSF NF Instance. |
| SnssaiTsctsfInfoItem | 6.1.6.2.92 | Set of parameters supported by TSCTSF for a given S-NSSAI. |
| DnnTsctsfInfoItem | 6.1.6.2.93 | Set of parameters supported by TSCTSF for a given DNN. |
| MbUpfInfo | 6.1.6.2.94 | Information of a MB-UPF NF Instance. |
| UnTrustAfInfo | 6.1.6.2.95 | Information of a untrusted AF Instance. |
| TrustAfInfo | 6.1.6.2.96 | Information of a trusted AF Instance |
| SnssaiInfoItem | 6.1.6.2.97 | Set of parameters supported by NF for a given S-NSSAI. |
| DnnInfoItem | 6.1.6.2.98 | Set of parameters supported by NF for a given DNN. |
| CollocatedNfInstance | 6.1.6.2.99 | Information related to collocated NF type(s) and corresponding NF Instance(s) when the NF is collocated with NFs supporting other NF types. |
| ServiceNameListCond | 6.1.6.2.100 | Subscription to a set of NF Instances that offer a service name in the Service Name list. |
| NfGroupListCond | 6.1.6.2.101 | Subscription to a set of NF Instances, identified by a NF Group Identity in the NF Group Identity list. |
| PlmnOauth2 | 6.1.6.2.102 | Per PLMN Oauth2.0 indication. |
| V2xCapability | 6.1.6.2.103 | Indicate the supported V2X Capability by the PCF. |
| NssaafInfo | 6.1.6.2.104 | Information of a NSSAAF NF Instance. |
| ProSeCapability | 6.1.6.2.105 | Indicate the supported ProSe Capability by the PCF. |
| SharedDataIdRange | 6.1.6.2.106 |  |
| SubscriptionContext | 6.1.6.2.107 | Context data related to a created subscription, to be included in notifications sent by NRF. |
| IwmscInfo | 6.1.6.2.108 | Information of a SMS-IWMSC NF Instance. |
| MnpfInfo | 6.1.6.2.109 | Information of an MNPF Instance. |
| NefId | 6.1.6.3.2 | Identity of the NEF. |
| VendorId | 6.1.6.3.2 | Vendor ID of the NF Service instance (Private Enterprise Number assigned by IANA) |
| WildcardDnai | 6.1.6.3.2 | Wildcard DNAI |
| NFType | 6.1.6.3.3 | NF types known to NRF. |
| NotificationType | 6.1.6.3.4 | Types of notifications used in Default Notification URIs in the NF Profile of an NF Instance. |
| TransportProtocol | 6.1.6.3.5 | Types of transport protocol used in a given IP endpoint of an NF Service Instance. |
| NotificationEventType | 6.1.6.3.6 | Types of events sent in notifications from NRF to subscribed NF Instances. |
| NFStatus | 6.1.6.3.7 | Status of a given NF Instance stored in NRF. |
| DataSetId | 6.1.6.3.8 | Types of data sets stored in UDR. |
| UPInterfaceType | 6.1.6.3.9 | Types of User-Plane interfaces of the UPF. |
| ServiceName | 6.1.6.3.11 | Service names known to NRF. |
| NFServiceStatus | 6.1.6.3.12 | Status of a given NF Service Instance of an NF Instance stored in NRF. |
| AnNodeType | 6.1.6.3.13 | Access Network Node Type (gNB, ng-eNB...). |
| ConditionEventType | 6.1.6.3.14 | Indicates whether a notification is due to the NF Instance to start or stop being part of a condition for a subscription to a set of NFs |
| IpReachability | 6.1.6.3.15 | Indicates the type(s) of IP addresses reachable via an SCP. |
| CollocatedNfType | 6.1.6.3.17 | Possible NF types supported by a collocated NF. |

Table 6.1.6.1-2 specifies data types re-used by the Nnrf\_NFManagement service-based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nnrf\_NFManagement service-based interface.

Table 6.1.6.1-2: Nnrf\_NFManagement re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| N1MessageClass | 3GPP TS 29.518 [6] | The N1 message type |
| N2InformationClass | 3GPP TS 29.518 [6] | The N2 information type |
| IPv4Addr | 3GPP TS 29.571 [7] |  |
| IPv6Addr | 3GPP TS 29.571 [7] |  |
| IPv6Prefix | 3GPP TS 29.571 [7] |  |
| Uri | 3GPP TS 29.571 [7] |  |
| Dnn | 3GPP TS 29.571 [7] |  |
| SupportedFeatures | 3GPP TS 29.571 [7] |  |
| Snssai | 3GPP TS 29.571 [7] |  |
| PlmnId | 3GPP TS 29.571 [7] |  |
| Guami | 3GPP TS 29.571 [7] |  |
| Tai | 3GPP TS 29.571 [7] |  |
| NfInstanceId | 3GPP TS 29.571 [7] |  |
| LinksValueSchema | 3GPP TS 29.571 [7] | 3GPP Hypermedia link |
| UriScheme | 3GPP TS 29.571 [7] |  |
| AmfName | 3GPP TS 29.571 [7] |  |
| DateTime | 3GPP TS 29.571 [7] |  |
| Dnai | 3GPP TS 29.571 [7] |  |
| ChangeItem | 3GPP TS 29.571 [7] |  |
| DiameterIdentity | 3GPP TS 29.571 [7] |  |
| AccessType | 3GPP TS 29.571 [7] |  |
| NfGroupId | 3GPP TS 29.571 [7] | Network Function Group Id |
| AmfRegionId | 3GPP TS 29.571 [7] |  |
| AmfSetId | 3GPP TS 29.571 [7] |  |
| PduSessionType | 3GPP TS 29.571 [7] |  |
| AtsssCapability | 3GPP TS 29.571 [7] | Capability to support procedures related to Access Traffic Steering, Switching, Splitting. |
| Nid | 3GPP TS 29.571 [7] |  |
| PlmnIdNid | 3GPP TS 29.571 [7] |  |
| NfSetId | 3GPP TS 29.571 [7] | NF Set ID (see clause 28.12 of 3GPP TS 23.003 [12]) |
| NfServiceSetId | 3GPP TS 29.571 [7] | NF Service Set ID (see clause 28.13 of 3GPP TS 23.003 [12]) |
| GroupId | 3GPP TS 29.571 [7] | Internal Group Identifier |
| RatType | 3GPP TS 29.571 [7] | RAT Type |
| DurationSec | 3GPP TS 29.571 [7] |  |
| RedirectResponse | 3GPP TS 29.571 [7] | Response body of the redirect response message. |
| ExtSnssai | 3GPP TS 29.571 [7] |  |
| AreaSessionId | 3GPP TS 29.571 [7] | Area Session Identifier used for an MBS session with location dependent content |
| MbsSessionId | 3GPP TS 29.571 [7] | MBS Session Identifier |
| MbsServiceArea | 3GPP TS 29.571 [7] | MBS Service Area |
| IpAddr | 3GPP TS 29.571 [7] | IP Address |
| MbsServiceAreaInfo | 3GPP TS 29.571 [7] | MBS Service Area Information for Location dependent MBS session |
| Fqdn | 3GPP TS 29.571 [7] | Fully Qualified Domain Name |
| EventId | 3GPP TS 29.520 [32] | Defined in Nnwdaf\_AnalyticsInfo API. |
| NwdafEvent | 3GPP TS 29.520 [32] | Defined in Nnwdaf\_EventsSubscription API. |
| ExternalClientType | 3GPP TS 29.572 [33] |  |
| LMFIdentification | 3GPP TS 29.572 [33] | LMF Identification |
| AfEvent | 3GPP TS 29.517 [35] | Defined in Naf\_EventExposure API |
| SupportedGADShapes | 3GPP TS 29.572 [33] | Supported GAD Shapes |
| NetworkNodeDiameterAddress | 3GPP TS 29.503 [36] | Diameter Address of a Network Node |

\* \* \* End of Changes \* \* \* \*