**3GPP TSG-CT WG4 Meeting #111-eC4-224402**

**E-Meeting, 18th – 26th August 2022** *Merger of C4-224062 and C4-224166*

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.532** | **CR** | **0027** | **rev** | **1** | **Current version:** | **17.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Change of MBS session authorization |
|  |  |
| ***Source to WG:*** | Huawei, Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5MBS |  | ***Date:*** | 2022-07-19 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Remaining editor's note reads: "it is FFS whether and how to notify a change of MBS session authorization (anyUEInd), i.e. whether this should be defined as an event type".SA2 has not specified in TS 23.247 if and how a change of MBS session authorization would be communicated to MB-SMF. The editor's note needs to be removed. |
|  |  |
| ***Summary of change:*** | The editor's note is removed. |
|  |  |
| ***Consequences if not approved:*** | An editor's note remains in Rel-17 specification. |
|  |  |
| ***Clauses affected:*** | 6.2.6.2.16. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev1: New NOTE is removed. C4-224166 is merged, Nokia, Nokia Shanghai Bell is added as a source and the cover sheet is updated. |

\* \* \* First Change \* \* \* \*

##### 6.2.6.2.16 Type: MbsContextInfo

Table 6.2.6.2.16-1: Definition of type MbsContextInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| startTime | DateTime | O | 0..1 | Start time of the multicast MBS session |  |
| anyUeInd | boolean | O | 0..1 | Indication that the multicast MBS session allows any UE to join.When present, it shall be set as follows:- true: any UE may join- false (default): the MBS session is not open to any UE |  |
| llSsm | Ssm | O | 0..1 | This IE may be present if multicast transport may be used over N19mb.When present, it shall contain the Low Layer Source Specific Multicast Address allocated by the MB-UPF. |  |
| cTeid | Uint32 | O | 0..1 | This IE may be present if multicast transport may be used over N19mb.When present, it shall contain the Common TEID allocated by the MB-UPF. |  |
| mbsServiceArea | MbsServiceArea | C | 0..1 | This IE shall be present for a Local MBS session. |  |
| mbsServiceAreaInfoList | map(MbsServiceAreaInfo) | C | 1..N | This IE shall be present for a location dependent MBS service. When present, one map entry shall be provided for each MBS Service Area served by the MBS session.The key of the map shall be the areaSessionId. |  |

\* \* \* End of Changes \* \* \* \*