**3GPP TSG-CT WG4 Meeting #111-eC4-224424**

**E-Meeting, 18th – 26th August 2022** *Revision of C4-224387*

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **29.518** | **CR** | **0788** | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction to ContextCreateReqData |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5MBS |  | ***Date:*** | 2022-08-10 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)lRel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Step 2 in clause 7.3.1 of TS 23.247 specifies the following, quote:The MB-SMF may use NRF to discover the AMF(s) supporting MBS based on the MBS service area and select the appropriate one(s). Then the MB-SMF sends the Namf\_MBSBroadcast\_ContextCreate (TMGI, N2 SM information ([LL SSM], 5G QoS Profile), MBS service area, [MBS FSA ID(s)]) messages to the selected AMF(s) in parallel if the service type is broadcast service. The MB-SMF may include a maximum response time in the request.If the message would contain the MB-SMF instance ID and MB-SMF service instance ID, the AMF could subscribe to MB-SMF status notifications. |
|  |  |
| ***Summary of change:*** | New attributes 'mbsmfId' and 'mbsmfServiceInstId' are added to 'ContextCreateReqData'. Also, editorials are applied to Table 6.5.6.2.2-1 (French is changed to UK English and extra period is replaced with a whitespace character. |
|  |  |
| ***Consequences if not approved:*** | AMF will not be able to monitor the service status from the NRF. |
|  |  |
| ***Clauses affected:*** | 6.5.6.2.2 A.6. |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** | This contribution introduces backwards compatible corrections to the Namf\_MBSBroadcast API. |
|  |  |
| ***This CR's revision history:*** | Rev1: New 'mbsmfServiceInstId' attribute is added to 'ContextCreateReqData'. Cover sheet is updated. |

\* \* \* First Change \* \* \* \*

6.5.6.2.2 Type: ContextCreateReqData

**Table 6.5.6.2.2-1: Definition of type ContextCreateReqData**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute name** | **Data type** | **P** | **Cardinality** | **Description** |
| mbsSessionId | MbsSessionId | M | 1 | MBS Session ID |
| mbsServiceArea | MbsServiceArea | C | 1 | MBS Service AreaThis IE shall be present if this is a Local broadcast MBS session.(NOTE 1) |
| mbsServiceAreaInfoList  | array(MbsServiceAreaInfo) | C | 1..N | List of MBS service areas and their related Area Session IDs.This IE shall be present if this is a Location dependent broadcast MBS service.(NOTE 1) |
| n2MbsSmInfo | N2MbsSmInfo | M | 1 | This IE shall be present and shall contain N2 MBS Session Management related information (see clause 6.5.6.4). |
| notifyUri | Uri | M | 1 | This IE shall contain the notification URI where to be notified about the status change of the broadcast MBS session context. |
| maxResponseTime | DurationSec | O | 0..1 | Maximum response time (in seconds) to receive information about the completion of the Broadcast MBS session establishment. |
| snssai  | Snssai | M | 1 | This IE shall be included to indicate the S-NSSAI of the MBS session. (NOTE 2). |
| mbsmfId | NfInstanceId | O | 0..1 | This IE may be present to contain the NF Instance ID of the MB-SMF.  |
| mbsmfServiceInstId | string | O | 0..1 | This IE may be present to contain the NF Service Instance ID within the NF Instance of the MB-SMF. |
| NOTE 1: Either the mbsServiceAreaInfoList IE or the mbsServiceArea IE shall be present.NOTE 2: If an MB-SMF does not receive the S-NSSAI from the NEF/MBSF, the MB-SMF shall include a pre-configured default SNSSAI. |

\* \* \* 2nd Change \* \* \* \*

# A.6 Namf\_MBSBroadcast API

openapi: 3.0.0

info:

 version: 1.0.0

 title: Namf\_MBSBroadcast

 description: |

 AMF MBSBroadcast Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

## Skipped for clarity ##

#

# STRUCTURED DATA TYPES

#

 ContextCreateReqData:

 description: Data within ContextCreate Request

 type: object

 properties:

 mbsSessionId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

 mbsServiceAreaInfoList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceAreaInfo'

 minItems: 1

 mbsServiceArea:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceArea'

 n2MbsSmInfo:

 $ref: '#/components/schemas/N2MbsSmInfo'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 maxResponseTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 mbsmfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 mbsmfServiceInstId:

 type: string

 required:

 - mbsSessionId

 - n2MbsSmInfo

 - notifyUri

 - snssai

 oneOf:

 - required: [ mbsServiceArea ]

 - required: [ mbsServiceAreaInfoList ]

## Skipped for clarity ##

\* \* \* End of Changes \* \* \* \*