**3GPP TSG- Meeting # *68***

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.2.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **2** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps | **x** | ME | **x** | Radio Access Network | **x** | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | and cl. 3.8 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | C6 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Wrong test case number in applicability table  Wrong implementation of C055 in applicability table  Duplication of O\_GERAN in newly added conditions C055 and C056  Wrong timer name in step e) of cl. 13.2.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Correct errors in spec | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.8, 13.2.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

3.8 Applicability table

**Table B.1: Applicability of tests**

| **Item** | **Description** | **Tested feature defined in Release** | **Test sequence(s)** | **R99 ME** | **Rel-4 ME** | **Rel-5 ME** | **Rel-6 ME** | **Rel-7 ME** | **Rel-8 ME** | **Rel-9 ME** | **Rel-10 ME** | **Rel-11 ME** | **Rel-12 ME** | **Rel-13 ME** | **Rel-14-ME** | **Network Dependency** | **Support** | **Additional test case execution recommendation** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | [………….] |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 124 | UE recognising the priority order of the User controlled PLMN selector over the Operator controlled PLMN selector list – E-UTRAN in NB-S1 mode | Rel-14 | 7.3.6 | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | C022  AND  C046 | NB System Simulator |  |  |
| 125 | UE recognising the priority order of the Operator controlled PLMN selector list using the ACT preference - E-UTRAN in NB-S1/ E-UTRAN in WB-S1 mode | Rel-14 | 7.3.7 | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | C027  AND  C046 | E-UTRAN System Simulator  and  NB System Simulator |  |  |
| 126 | UE recognising the priority order of the Operator controlled PLMN selector list using the ACT preference - E-UTRAN in NB-S1 mode/ GSM | Rel-14 | 7.3.8 | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | C046 AND C055 | NB System Simulator  and  System Simulator |  |  |
| 127 | UE recognising the priority order of the Operator controlled PLMN selector list using the ACT preference - E-UTRAN in WB-S1 mode/GSM | Rel-14 | 7.3.9 | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | N/A | C027 AND  C055 | E-UTRAN and  System Simulator |  |  |

**Table B.1: Applicability of tests (continued)**

|  |  |  |
| --- | --- | --- |
|  | [……….] |  |
| C022 | IF A.1/17 THEN M ELSE N/A | -- O\_EFPLMNwACT\_numerical entry |
|  | [………..] |  |
| C027 | IF (A.1/20 OR A.1/21) THEN M ELSE N/A | -- pc\_eFDD OR pc\_eTDD |
|  | [……….] |  |
| C046 | IF A.1/37 THEN M ELSE N/A | -- pc\_NB |
| C047 | IF (A.1/3 OR (A.1/4 AND NOT A.1/38)) THEN M ELSE N/A | -- O\_UTRAN OR (O\_GERAN AND NOT O\_PLMN\_specific\_PS\_attempt\_counters) |
| C048 | IF A.1/3 THEN M ELSE N/A | -- O\_UTRAN |
| C049 | IF A.1/3 OR A.1/4 THEM M ELSE N/A | -- O\_UTRAN OR O\_GERAN |
| C050 | IF A.1/15 AND (A.1/20 OR A.1/21) THEN M ELSE N/A | -- O\_ACL AND (pc\_eFDD OR pc\_eTDD) |
| C051 | ..IF (A.1/20 OR A.1/21 OR A.1/37) AND A.1/39 THEN M ELSE N/A | -- (pc\_eFDD OR pc\_eTDD OR pc\_NB) AND O\_PSM\_DEAC\_UICC |
| C052 | IF (A.1/20 OR A.1/21 OR A.1/37) AND A.1/40 THEN M ELSE N/A | -- (pc\_eFDD OR pc\_eTDD OR pc\_NB) AND O\_eDRX\_DEAC\_UICC |
| C053 | IF (A.1/20 OR A.1/21 OR A.1/37) AND A.1/41 THEN M ELSE N/A | -- (pc\_eFDD OR pc\_eTDD OR pc\_NB) AND O\_PSM\_ SUSPEND\_UICC |
| C054 | IF (A.1/20 OR A.1/21 OR A.1/37) AND A.1/42 THEN M ELSE N/A | -- (pc\_eFDD OR pc\_eTDD OR pc\_NB) AND O\_eDRX\_ SUSPEND\_UICC |
| C055 | IF A.1/4 THEN M ELSE N/A | -- O\_GERAN |
| O.1 | IF C002 THEN "Expected Sequence A" M ELSE IF C001 THEN "Expected Sequence B" M |  |

[……]

13.2 UICC interface in PSM handling for E-UTRAN – PSM not accepted by E-USS/NB-SS

[….]

13.2.4.2 Procedure

a) The UE is switched on.

b) The UE requests RRC Connection and transmits an *ATTACH REQUEST* message to the E-USS/NB-SS including T3324 set to T3324\_V.

c) The E-USS/NB-SS sends the *ATTACH ACCEPT* message contains a T3324 set to “deactivated”. It shall not contain the eDRX parameters.

d) After receipt of the *AttachComplete* during registration from the UE, the E-USS/NB-SS sends *RRCConnectionRelease/RRCConnectionRelease-NB*, to the UE

e) After the time period T3324\_V has passed, the E-USS/NB-SS transmits *Paging/Paging-NB* to the UE using the S-TMSI.

[…………]