{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":91,"n_cols":32,"rows_kept":91,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Secretary Remarks","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["C6-150401","Meeting Agenda","WG Chairman","Xavier Piednoir",32337,"agenda","","Decision","","","3","3","Agenda and organisational issues",0,"revised","2015-08-04T08:00:00.913","2015-08-13T10:38:55.253","","","","","","","","","","","","","","",""]
["C6-150402","Call for IPRs and Statement of anti-trust compliance","MCC","Xavier Piednoir",32337,"other","","Decision","","","5","3.2","IPR",0,"noted","2015-08-04T08:00:00.923","2015-08-17T16:17:28.897","","","","","","","","","","","","","","",""]
["C6-150403","Draft Report of CT6 meeting #76","MCC","Xavier Piednoir",32337,"report","","Decision","","","6","3.3","Report of previous CT6 meeting",0,"revised","2015-08-04T08:00:00.930","2015-08-17T00:38:52.643","","","","","","","","","","","","","","",""]
["C6-150404","Approved Report of CT6 meeting #76","3GPP CT6","Xavier Piednoir",32337,"report","","Decision","","","6","3.3","Report of previous CT6 meeting",0,"approved","2015-08-04T08:00:00.937","2015-09-17T09:58:10.483","","","","","","","","","","","","","","",""]
["C6-150405","Action list before CT6 #77","MCC","Xavier Piednoir",32337,"other","","Decision","","","13","5.4","Review of action list",0,"revised","2015-08-04T08:00:00.947","2015-08-13T14:32:24.820","","","","","","","","","","","","","","",""]
["C6-150406","Action list after CT6 #77","3GPP CT6","Xavier Piednoir",32337,"other","","Decision","","","13","5.4","Review of action list",0,"noted","2015-08-04T08:00:00.953","2015-09-17T09:01:56.593","","","","","","","","","","","","","","",""]
["C6-150407","Status of CT6 specifications and rapporteurs","MCC","Xavier Piednoir",32337,"other","","Decision","","","14","5.5","Status of CT6 specifications, rapporteurs & WIs",0,"revised","2015-08-04T08:00:00.960","2015-09-17T09:01:56.763","","","","","","","","","","","","","","",""]
["C6-150408","Updated status of CT6 specifications and rapporteurs","3GPP CT6","Xavier Piednoir",32337,"other","","Decision","","","14","5.5","Status of CT6 specifications, rapporteurs & WIs",0,"noted","2015-08-04T08:00:00.967","2015-09-17T09:01:56.967","","","","","","","","","","","","","","",""]
["C6-150409","Meetings schedule","MCC","Xavier Piednoir",32337,"other","","Decision","","","60","10","Meeting plan",0,"revised","2015-08-04T08:00:00.973","2015-08-13T14:38:43.617","","","","","","","","","","","","","","",""]
["C6-150410","Updated meetings schedule","3GPP CT6","Xavier Piednoir",32337,"other","","Decision","","","60","10","Meeting plan",0,"noted","2015-08-04T08:00:00.983","2015-09-17T09:01:57.153","","","","","","","","","","","","","","",""]
["C6-150411","Meeting Agenda with document allocation","WG Chairman","Xavier Piednoir",32337,"agenda","","Decision","","","4","3.1","Agreement of the agenda and the scheduling",0,"revised","2015-08-04T08:00:00.990","2015-08-13T10:38:55.423","","C6-150490","","","","","","","","","","","","",""]
["C6-150412","Status report of SCP activities after SCP #69","ETSI TC SCP Liaison Officer","Xavier Piednoir",32337,"other","","Decision","","","59","9","Report on ETSI TC SCP activity and review of approved ETSI TC SCP change requests",0,"noted","2015-08-04T08:00:00.997","2015-09-17T09:01:57.343","","","","","","","","","","","","","","",""]
["C6-150413","Chairman's report from CT Plenary #68","WG Chairman","Xavier Piednoir",32337,"other","","Decision","","","10","5.1","Report from TSG plenary meetings",0,"noted","2015-08-04T08:00:01.007","2015-09-17T09:01:57.543","","","","","","","","","","","","","","",""]
["C6-150414","Correction to Bearer parameters for UTRAN and EUTRAN","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Several octets in the \"Bearer parameters for UTRAN Packet Service with extended parameters / HSDPA / E-UTRAN\" refer to parameters in 27.007 that are encoded as strings or that can have maximum value that exceed what can be represented in this object.\nMoreover, \"EPS quality of service\" information element, defined in TS 24.301 clause 9.9.4.3, was updated with extended-2 values for maximum and guaranteed bitrates in Rel.11 (CR 1373, C1-121580). This causes that maximum size of the element increased from 11 to 15 octets. The increased definition cannot be represented in the Bearer description TLV for \"Bearer parameters for E-UTRAN / mapped UTRAN packet service\".","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-05T00:53:24.587","2015-08-07T21:14:19.247","","","Rel-13","31.111","13.0.0","TEI13","0627","","F","CP-150563","","","","",""]
["C6-150415","TS 31.124, Rel-12 content replacement by reference to TS 31.124, Rel-13","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","TS 31.124 Rel-12 shall reference to the next release which covers the tests for all releases in a single document","","49","7.7.1","TEI 12 (TEI12)",0,"agreed","2015-08-05T00:56:04.153","2015-08-07T21:16:59.370","","","Rel-12","31.124","12.4.0","TEI12","0421","","F","CP-150560","","","","",""]
["C6-150416","Addition of Rel.13 column to applicability table","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Applicability table does not contain column for Rel.13 ME","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-05T01:00:19.943","2015-08-07T21:16:59.557","","C6-150465","Rel-13","31.124","13.0.0","TEI13","0422","","F",null,"","","","",""]
["C6-150417","Typo in the Option A.1/74 for Class E: Terminal supports UDP, Terminal in Server Mode","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","Item 74 in the table A.1 wrongly indicates \"Class E: Terminal supports UDP, UICC in Server Mode\", while it applies to \"Class E: Terminal supports UDP, Terminal in Server Mode\".","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-05T01:04:09.173","2015-08-07T21:18:56.347","","","Rel-13","31.124","13.0.0","TEI13","0423","","F","CP-150562","","","","",""]
["C6-150418","LS to 3GPP CT6 on Need for enhanced USAT Testing","GCF","Paul Jolivet",16261,"LS in","","Decision","","","17","6.2","Incoming liaison statements / inputs from other groups",0,"noted","2015-08-05T13:59:10.617","2015-08-05T14:22:10.263","","","","","","","","","","",null,null,null,null,"C6-150489"]
["C6-150419","ePDG Identifier configuration","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","SA2 CR#1373 has concluded in 23.402 on the use of ePDG Identifier configuration in the ePDG static selection procedure. The USIM need provide a configuration file to store the ePDG Identifer configuration information accordingly.\nThe CR provides ePDG Identifier Configuration support by the USIM.","","49","7.7.1","TEI 12 (TEI12)",0,"postponed","2015-08-05T14:22:37.030","2015-08-10T15:56:10.783","C6-150239","C6-150552, C6-150571","Rel-12","31.102","12.8.1","TEI12","0630","1","F",null,"","","","",""]
["C6-150420","ePDG Selection Information","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","SA2 has concluded in CR#1376 to TS 23.402 on the use of ePDG Selection Information in the ePDG selection procedure. The USIM need provide a configuration file to store the ePDG selection information accordingly.\nThe CR provide the corresponding EF to store ePDG Selection information.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-05T14:31:57.993","2015-08-10T15:56:10.997","","C6-150461","Rel-13","31.102","13.0.0","TEI13","0636","","B",null,"","","","",""]
["C6-150421","ePDG Identifier configuration","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","SA2 CR#1373 has concluded in 23.402 on the use of ePDG Identifier configuration in the ePDG static selection procedure. The USIM need provide a configuration file to store the ePDG Identifer configuration information accordingly.\nProvide ePDG Identifier Configuration support by the USIM.","","49","7.7.1","TEI 12 (TEI12)",0,"postponed","2015-08-05T14:44:36.823","2015-08-21T01:37:47.043","","C6-150553, C6-150565, C6-150572","Rel-13","31.102","13.0.0","TEI12","0637","","A",null,"","","","",""]
["C6-150422","Alignment of Provide Local Information for Timing Advance to E-UTRAN radio technology","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","Timing advance information is available in the ME when it is connected to GERAN or E-UTRAN. However, the Provide Local Information USAT specification restricted the availability of the information to GERAN as the information was not avaialble in UTRAN. It is proposed to align the availability of the information to the support of E-UTRAN technology.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-05T15:00:21.697","2015-08-10T15:59:07.287","C6-150238","C6-150466","Rel-13","31.111","13.0.0","TEI13","0436","1","B",null,"","","","",""]
["C6-150423","Clarification to the applicability of the UE retry wait time value or behaviour","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","CT1 has approved changes in TS 24.368 that change the description of the SM_RetryWaitTime and SM_RetryAtRATChange for more clarity (see document CP-150329).","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-05T22:35:15.863","2015-08-07T21:20:51.420","","","Rel-13","31.102","13.0.0","TEI13","0638","","F","CP-150563","","","","",""]
["C6-150424","Replacement of EF LAUNCH SCWS with EF LAUNCH PAD","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","ETSI SCP has approved changes in TS 102 221 to have the same functionality and features to display a Smart Card Web Server launch pad as currently described in 3GPP TS 31.102. In order to avoid problems for technical implementations to handle to conflicting sources of launch pad information (as described in document C6-104626), the EF LAUNCH SCWS in the USIM is removed and reference to EF LAUNCH PAD is introduced.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-05T23:02:19.727","2015-08-07T21:22:27.090","","C6-150467","Rel-13","31.101","12.2.0","TEI13","0082","","C",null,"","","","",""]
["C6-150425","Replacement of EF LAUNCH SCWS with EF LAUNCH PAD","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","ETSI SCP has approved changes in TS 102 221 to have the same functionality and features to display a Smart Card Web Server launch pad as currently described in 3GPP TS 31.102. In order to avoid problems for technical implementations to handle to conflicting sources of launch pad information (as described in document C6-104626), the EF LAUNCH SCWS in the USIM is removed and reference to EF LAUNCH PAD is introduced.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-05T23:03:48.267","2015-08-07T21:22:27.263","","C6-150468","Rel-13","31.102","13.0.0","TEI13","0639","","C",null,"","","","",""]
["C6-150426","Update of EF-GBABP when key material is discarded","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","According to TS 33.220 clasue 5.3.3: \"GBA keys in UICC do not need to be deleted when the ME is powered down\". This indicates that UICC might retain the key material or discard it.\nAnyway, if the key material is discarded and EF-GBABP is not updated, the ME is not aware of it and would unnecessarily attempt to perform an AUTHENTICATE command with GBA security context (NAF Derivation Mode). This could be avoided if the UICC had deleted the content of EF-GBABP when key material was deleted.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-05T23:07:56.360","2015-08-07T21:23:57.070","","C6-150555, C6-150573","Rel-13","31.102","13.0.0","TEI13","0640","","C",null,"","","","",""]
["C6-150427","Update of EF-GBABP when key material is discarded","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","According to TS 33.220 clasue 5.3.3: \"GBA keys in UICC do not need to be deleted when the ME is powered down\". This indicates that UICC might retain the key material or discard it.\nAnyway, if the key material is discarded and EF-GBABP is not updated, the ME is not aware of it and would unnecessarily attempt to perform an AUTHENTICATE command with GBA security context (NAF Derivation Mode). This could be avoided if the UICC had deleted the content of EF-GBABP when key material was deleted.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-05T23:09:47.033","2015-08-07T21:23:57.240","","C6-150556, C6-150574","Rel-13","31.103","13.0.0","TEI13","0096","","C",null,"","","","",""]
["C6-150428","Alignment of UICC polling interval with eDRX cycle","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","eDRX feature is introduced to reduce the amount of power for specific classes of devices. In those cases, it is desirable to also extend the UICC polling interval to avoid unnecessary polling while the device has negotiated an extended DRX cycle with the network.","","52","7.8","Rel-13",0,"revised","2015-08-05T23:13:35.900","2015-08-07T21:33:23.387","","C6-150470","Rel-13","31.101","12.2.0","eDRX-CT","0083","","C",null,"","","","",""]
["C6-150429","New Work Item on Extended DRX cycle for Power Consumption Optimization","QUALCOMM Incorporated","Michele Berionne",45196,"WID new","","Decision","New Work Item on Extended DRX cycle for Power Consumption Optimization","","55","7.9","New Work Items / Study Items",0,"revised","2015-08-05T23:20:51.457","2015-08-07T21:33:23.203","","C6-150473","Rel-13","","","","","","","","","","","",""]
["C6-150430","Discussion paper on specific_x00B_network availability","QUALCOMM Incorporated","Michele Berionne",45196,"discussion","","Decision","Discussion paper on specific_x00B_ network availability","","53","7.8.1","TEI 13 (TEI13)",0,"noted","2015-08-05T23:22:55.977","2015-08-07T21:39:21.053","","","","","","","","","","","","","","",""]
["C6-150431","Testing for ProSe USIM","QUALCOMM Incorporated","Michele Berionne",45196,"discussion","","Decision","Discussion paper on testing aspects for USIM with ProSe support","","50","7.7.2","CT6 part of CT aspects of Proximity-based Services (ProSe-CT)",0,"noted","2015-08-05T23:37:31.437","2015-08-07T21:40:39.033","","","","","","","","","","","","","","",""]
["C6-150432","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences","Comprion GmbH","Achim Lobbert",49073,"CR","","Decision","This CR adds the following REFRESH test case sequences to TS 31.124:\nSeq 2.1 REFRESH, UICC Reset for IMSI Changing procedure\nSeq 2.3 REFRESH, 3G Session Reset for IMSI Changing procedure\nSeq 2.x REFRESH, reject UICC Reset for IMSI Change procedure during CS call\nSeq 2.y REFRESH, UICC Reset for IMSI Change procedure during PDN Connection\nSeq 2.z REFRESH, 3G Session Reset for IMSI Change procedure during PDN Connection","","52","7.8","Rel-13",0,"revised","2015-08-07T14:59:05.513","2015-08-07T15:30:36.160","","C6-150462","Rel-13","31.124","13.0.0","TEI12","0424","","B",null,"","","","",""]
["C6-150433","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences for E-UTRAN","Comprion GmbH","Achim Lobbert",49073,"CR","","Decision","LS S-15-161r1 from GCF SG to 3GPP TSG CT6 asking for additional USAT Confirmance Criteria to cover existing REFRESH command qualifiers according to current market requirements. Up to now no test case was defined for testing REFRESH command qualifiers when the terminal is connected to E-UTRAN.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-07T15:03:07.947","2015-08-07T15:30:36.337","","C6-150463","Rel-13","31.124","13.0.0","TEI12","0425","","B",null,"","","","",""]
["C6-150434","USAT Testing Enhancement by addition of new test case sequence 1.x for REFRESH command qualifier \"USIM Initialization and Full File change Notification\" when roaming between different countries","Comprion GmbH, Vodafone GmbH","Achim Lobbert",49073,"CR","","Decision","This CR adds the following test sequence  to TS 31.124, test case 27.22.4.7.1:\nSeq 1.x REFRESH, USIM Initialization and Full File Change Notification when roaming between different countries.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-07T15:07:03.590","2015-08-07T15:30:36.510","","C6-150557, C6-150575","Rel-13","31.124","13.0.0","TEI13","0426","","B",null,"","","","",""]
["C6-150435","CR 31.124 R13 USAT Correction of technical handling of features made optional by TR 31.901 within applicability table and terminal profile.","Comprion GmbH","Achim Lobbert",49073,"CR","","Decision","Features made optional by TR 31.901 are corrected to be handled within table A.1 following above concept to be used for conditions within applicability table B.1 and terminal profile table E.1.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-07T15:09:58.720","2015-08-07T15:30:35.930","","C6-150472","Rel-13","31.124","13.0.0","TEI13","0427","","F",null,"","","","",""]
["C6-150436","UICC interface in Power Saving Mode (PSM)","QUALCOMM Incorporated","Michele Berionne",45196,"discussion","","Decision","Discussion paper on power consumption of the UICC interface with regards to the Power Saving Mode (PSM)","","53","7.8.1","TEI 13 (TEI13)",0,"noted","2015-08-07T21:48:45.310","2015-08-07T22:05:36.010","","","","","","","","","","","","","","",""]
["C6-150437","UICC interface in Power Saving Mode (PSM)","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The power consumption of the UICC in idle mode can become significant after long periods of time, as described in document C6-150436. For this reason, it is desirable to be able to deactivate the UICC while the UE is in PSM.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-07T22:04:21.840","2015-08-07T22:05:36.197","","C6-150464","Rel-13","31.102","13.0.0","TEI13","0641","","B",null,"","","","",""]
["C6-150438","Correction to PLI, Inter-frequency UTRAN Measurements test case","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The validation of the network measurement report in the PROVIDE LOCAL INFORMATION, Inter-frequency UTRAN Measurements test case is not correct in case of odd value of UTRA-CarrierRSSI.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-07T22:07:52.877","2015-08-07T22:15:07.977","","C6-150474","Rel-13","31.124","13.0.0","TEI13","0428","","F",null,"","","","",""]
["C6-150439","Correction to PLI, Inter-frequency UTRAN Measurements test case","QUALCOMM Incorporated","Michele Berionne",45196,"discussion","","Decision","","","53","7.8.1","TEI 13 (TEI13)",0,"noted","2015-08-07T22:08:58.250","2015-08-07T22:15:08.180","","","Rel-13","","","","","","","","","","","",""]
["C6-150440","Relaxing the mandatory clause & Making features optional","BlackBerry UK Limited","Adrian Buckley",26735,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-08-07T22:34:17.420","2015-08-07T22:40:23.997","","C6-150475","Rel-13","31.121","12.3.0","Red_UCe","0200","","C",null,"","","","",""]
["C6-150441","New commands to suspend and resume the UICC","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","The power consumption of the UICC in idle mode can become significant over long periods of time for devices that have very strict power requirements. For this reason, it would be beneficial to be able to power down the UICC in specific circumstances (for example, while in PSM mode). In this cases, it is desirable that ME can resume the previous UICC session after waking up, without having to perform a complete re-initialization.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-07T22:36:30.467","2015-08-07T22:37:26.900","","C6-150558, C6-150576","Rel-13","31.101","12.2.0","TEI13","0084","","B",null,"","","","",""]
["C6-150442","Precedence between EF NASconfig and the NAS Configuration MO","Intel","Robert Zaus",10799,"other","","Decision","","","39","7.5.7","CT6 part of Stage 3 for Network Improvements for Machine-Type Communication",0,"noted","2015-08-10T14:10:15.593","2015-08-11T11:29:57.607","","","","","","","","","","","","","","",""]
["C6-150443","Correction of EF NASconfig","Intel","Robert Zaus",10799,"CR","","Decision","","","39","7.5.7","CT6 part of Stage 3 for Network Improvements for Machine-Type Communication",0,"postponed","2015-08-10T14:10:15.607","2015-08-11T07:40:14.840","","C6-150548, C6-150577","Rel-10","31.102","10.11.0","NIMTC-CN","0642","","F",null,"","","","",""]
["C6-150444","Correction of EF NASconfig","Intel","Robert Zaus",10799,"CR","","Decision","","","39","7.5.7","CT6 part of Stage 3 for Network Improvements for Machine-Type Communication",0,"postponed","2015-08-10T14:10:15.763","2015-08-11T07:40:15.030","","C6-150549, C6-150578","Rel-11","31.102","11.8.0","NIMTC-CN","0643","","A",null,"","","","",""]
["C6-150445","Correction of EF NASconfig","Intel","Robert Zaus",10799,"CR","","Decision","","","39","7.5.7","CT6 part of Stage 3 for Network Improvements for Machine-Type Communication",0,"postponed","2015-08-10T14:10:15.873","2015-08-11T07:40:15.217","","C6-150550, C6-150579","Rel-12","31.102","12.8.1","NIMTC-CN","0644","","A",null,"","","","",""]
["C6-150446","Correction of EF NASconfig","Intel","Robert Zaus",10799,"CR","","Decision","","","39","7.5.7","CT6 part of Stage 3 for Network Improvements for Machine-Type Communication",0,"postponed","2015-08-10T14:10:15.997","2015-08-11T07:40:15.403","","C6-150551, C6-150570, C6-150615, C6-150616, C6-150617","Rel-13","31.102","13.0.0","NIMTC-CN","0645","","A",null,"","","","",""]
["C6-150447","Provide Local Information [Access Technology] test scenario with change of Access Technology during a call.","Gemalto N.V.","Ly Thanh Phan",42268,"CR","","Decision","This CR provide the test scenario to cover these cases to ensure valid and current Access Technology information is provided to the USAT application when a PLI[Access Technology] command is performed by the ME.","","49","7.7.1","TEI 12 (TEI12)",0,"postponed","2015-08-10T16:03:49.687","2015-08-10T16:09:09.960","","C6-150554, C6-150580","Rel-12","31.124","12.4.0","TEI12","0429","","C",null,"","","","",""]
["C6-150448","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Paul Jolivet",16261,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"not pursued","2015-08-11T16:58:45.637","2015-08-11T17:33:42.937","C6-150253","","Rel-8","31.122","8.0.1","TEI8","0052","1","F",null,"","","","",""]
["C6-150449","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Paul Jolivet",16261,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"not pursued","2015-08-11T17:03:59.397","2015-08-11T17:33:43.107","C6-150254","","Rel-9","31.122","9.2.0","TEI8","0053","1","A",null,"","","","",""]
["C6-150450","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Paul Jolivet",16261,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"not pursued","2015-08-11T17:06:17.413","2015-08-11T17:33:43.293","C6-150255","","Rel-10","31.122","10.0.0","TEI8","0054","1","A",null,"","","","",""]
["C6-150451","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Paul Jolivet",16261,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"not pursued","2015-08-11T17:08:06.783","2015-08-11T17:33:43.497","C6-150256","","Rel-11","31.122","11.1.0","TEI8","0055","1","A",null,"","","","",""]
["C6-150452","Specify the status condition returned  if search pattern can not be found in any of the records","China Mobile","Paul Jolivet",16261,"CR","","Decision","","","25","7.3.1","TEI 8 (TEI8)",0,"postponed","2015-08-11T17:10:31.367","2015-08-11T17:33:43.667","C6-150257","C6-150544, C6-150581","Rel-12","31.122","12.0.0","TEI8","0056","1","A",null,"","","","",""]
["C6-150453","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Paul Jolivet",16261,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"postponed","2015-08-11T17:20:15.460","2015-08-11T17:33:43.857","C6-150285","C6-150545, C6-150582","Rel-10","31.130","10.4.0","TEI8","0068","3","F",null,"","","","",""]
["C6-150454","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Paul Jolivet",16261,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"postponed","2015-08-11T17:23:46.043","2015-08-11T17:33:44.027","C6-150286","C6-150546, C6-150583","Rel-11","31.130","11.0.0","TEI8","0069","3","A",null,"","","","",""]
["C6-150455","Missing rule for SMS_PP envelope response handling","OBERTHUR TECHNOLOGIES","Paul Jolivet",16261,"CR","","Decision","","","33","7.5.1","TEI 10 (TEI10)",0,"postponed","2015-08-11T17:25:09.967","2015-08-11T17:33:44.193","C6-150287","C6-150547, C6-150584","Rel-12","31.130","12.0.0","TEI8","0070","3","A",null,"","","","",""]
["C6-150456","WID on \"CT aspects of Support of Emergency services over WLAN – phase 1\"","Alcatel-Lucent, Alcatel-Lucent Shanghai Bell /Jennifer","Jennifer Liu",43418,"WID new","","Decision","","","55","7.9","New Work Items / Study Items",0,"endorsed","2015-08-12T18:16:13.117","2015-08-12T18:22:45.933","","","Rel-13","","","","","","","","","","","",""]
["C6-150457","Reply LS on SCWS Launch Pad and Launch SCWS","ETSI SCP","Xavier Piednoir",32337,"LS in","","Decision","","","17","6.2","Incoming liaison statements / inputs from other groups",0,"noted","2015-08-13T08:55:03.590","2015-08-13T08:59:31.940","","","Rel-13","","","","","","",""]
["C6-150458","LS on the acceptance of TS 102 230-2","ETSI SCP","Xavier Piednoir",32337,"LS in","","Decision","","","17","6.2","Incoming liaison statements / inputs from other groups",0,"noted","2015-08-13T09:01:45.763","2015-08-13T09:03:34.837","","","Rel-9","","","","","","",""]
["C6-150459","New WID on Mission Critical Push To Talk over LTE protocol aspects","Samsung R&D Institute UK","Ricky Kaura",36916,"WID new","","Decision","WID for MCPTT only submitted for information.","","55","7.9","New Work Items / Study Items",0,"noted","2015-08-14T18:50:32.607","2015-08-14T19:00:48.773","","","Rel-13","","","","","","","","","","","",""]
["C6-150460","Provide Local Information requests for network details","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"withdrawn","2015-08-17T16:39:28.143","2015-08-17T16:42:47.397","C6-150283","","Rel-12","31.111","12.8.0","TEI12","0423","2","C",null,"","","","",""]
["C6-150461","ePDG Selection Information","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","SA2 has concluded in CR#1376 to TS 23.402 on the use of ePDG Selection Information in the ePDG selection procedure. The USIM need provide a configuration file to store the ePDG selection information accordingly.\nThe CR provide the corresponding EF to store ePDG Selection information.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-17T22:45:04.557","2015-08-17T22:46:11.053","C6-150420","C6-150559, C6-150585","Rel-13","31.102","13.0.0","TEI13","0636","1","B",null,"","","","",""]
["C6-150462","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences","Comprion GmbH, Vodafone GmbH","Xavier Piednoir",32337,"CR","","Decision","This CR adds the following REFRESH test case sequences to TS 31.124:\nSeq 2.1 REFRESH, UICC Reset for IMSI Changing procedure\nSeq 2.3 REFRESH, 3G Session Reset for IMSI Changing procedure\nSeq 2.x REFRESH, reject UICC Reset for IMSI Change procedure during CS call\nSeq 2.y REFRESH, UICC Reset for IMSI Change procedure during PDN Connection\nSeq 2.z REFRESH, 3G Session Reset for IMSI Change procedure during PDN Connection","","52","7.8","Rel-13",0,"revised","2015-08-18T17:23:48.617","2015-09-17T09:01:57.733","C6-150432","C6-150481","Rel-13","31.124","13.0.0","TEI13","0424","1","B",null,"","","","",""]
["C6-150463","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences for E-UTRAN","Comprion GmbH","Xavier Piednoir",32337,"CR","","Decision","LS S-15-161r1 from GCF SG to 3GPP TSG CT6 asking for additional USAT Confirmance Criteria to cover existing REFRESH command qualifiers according to current market requirements. Up to now no test case was defined for testing REFRESH command qualifiers when the terminal is connected to E-UTRAN.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-18T18:12:02.710","2015-09-17T09:01:58.027","C6-150433","C6-150482","Rel-13","31.124","13.0.0","TEI13","0425","1","B",null,"","","","",""]
["C6-150464","UICC interface in Power Saving Mode (PSM)","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","The power consumption of the UICC in idle mode can become significant after long periods of time, as described in document C6-150436. For this reason, it is desirable to be able to deactivate the UICC while the UE is in PSM.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-18T22:12:31.110","2015-08-18T22:22:04.860","C6-150437","","Rel-13","31.102","13.0.0","TEI13","0641","1","B","CP-150563","","","","",""]
["C6-150465","Addition of Rel.13 column to applicability table","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","Applicability table does not contain column for Rel.13 ME","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-18T22:23:47.977","2015-08-18T22:24:10.547","C6-150416","","Rel-13","31.124","13.0.0","TEI13","0422","1","B","CP-150562","","","","",""]
["C6-150466","Alignment of Provide Local Information for Timing Advance to E-UTRAN radio technology","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","Timing advance information is available in the ME when it is connected to GERAN or E-UTRAN. However, the Provide Local Information USAT specification restricted the availability of the information to GERAN as the information was not avaialble in UTRAN. It is proposed to align the availability of the information to the support of E-UTRAN technology.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-18T23:32:56.160","2015-08-20T18:55:46.620","C6-150422","C6-150487","Rel-13","31.111","13.0.0","TEI13","0436","2","B",null,"","","","",""]
["C6-150467","Replacement of EF LAUNCH SCWS with EF LAUNCH PAD","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","ETSI SCP has approved changes in TS 102 221 to have the same functionality and features to display a Smart Card Web Server launch pad as currently described in 3GPP TS 31.102. In order to avoid problems for technical implementations to handle to conflicting sources of launch pad information (as described in document C6-104626), the EF LAUNCH SCWS in the USIM is removed and reference to EF LAUNCH PAD is introduced.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-18T23:43:27.537","2015-08-18T23:58:39.897","C6-150424","","Rel-13","31.101","12.2.0","TEI13","0082","1","B","CP-150563","","","","",""]
["C6-150468","Replacement of EF LAUNCH SCWS with EF LAUNCH PAD","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","ETSI SCP has approved changes in TS 102 221 to have the same functionality and features to display a Smart Card Web Server launch pad as currently described in 3GPP TS 31.102. In order to avoid problems for technical implementations to handle to conflicting sources of launch pad information (as described in document C6-104626), the EF LAUNCH SCWS in the USIM is removed and reference to EF LAUNCH PAD is introduced.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-19T00:02:03.177","2015-08-19T00:02:32.317","C6-150425","","Rel-13","31.102","13.0.0","TEI13","0639","1","C","CP-150563","","","","",""]
["C6-150469","Alignment of UICC polling interval with eDRX cycle","Qualcomm Incorporated","Michele Berionne",45196,"CR","","Decision","eDRX feature is introduced to reduce the amount of power for specific classes of devices. In those cases, it is desirable to also extend the UICC polling interval to avoid unnecessary polling while the device has negotiated an extended DRX cycle with the network.","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-19T15:32:29.920","2015-08-19T15:41:55.213","","C6-150560, C6-150586","Rel-13","31.102","13.0.0","eDRX-CT","0646","","B",null,"","","","",""]
["C6-150470","Alignment of UICC polling interval with eDRX cycle","QUALCOMM Incorporated","Michele Berionne",45196,"CR","","Decision","eDRX feature is introduced to reduce the amount of power for specific classes of devices. In those cases, it is desirable to also extend the UICC polling interval to avoid unnecessary polling while the device has negotiated an extended DRX cycle with the network.","","52","7.8","Rel-13",0,"revised","2015-08-19T15:34:58.913","2015-08-19T15:41:55.387","C6-150428","C6-150479","Rel-13","31.101","12.2.0","eDRX-CT","0083","1","C",null,"","","","",""]
["C6-150471","Change the number of EFs at the MF level","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-08-19T15:57:41.980","2015-08-19T16:08:34.273","","C6-150476","Rel-13","31.102","13.0.0","TEI12","0647","","F",null,"","","","",""]
["C6-150472","CR 31.124 R13 USAT Correction of technical handling of features made optional by TR 31.901 within applicability table and terminal profile.","Comprion GmbH","Xavier Piednoir",32337,"CR","","Decision","Features made optional by TR 31.901 are corrected to be handled within table A.1 following above concept to be used for conditions within applicability table B.1 and terminal profile table E.1.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-19T17:34:53.110","2015-08-19T17:36:30.563","C6-150435","","Rel-13","31.124","13.0.0","TEI13","0427","1","F","CP-150562","","","","",""]
["C6-150473","New Work Item on Extended DRX cycle for Power Consumption Optimization","QUALCOMM Incorporated","Michele Berionne",45196,"WID new","","Decision","New Work Item on Extended DRX cycle for Power Consumption Optimization","","55","7.9","New Work Items / Study Items",0,"endorsed","2015-08-19T17:37:56.503","2015-08-19T17:38:53.117","C6-150429","","Rel-13","","","","","","","","","","","",""]
["C6-150474","Correction to PLI, Inter-frequency UTRAN Measurements test case","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","The validation of the network measurement report in the PROVIDE LOCAL INFORMATION, Inter-frequency UTRAN Measurements test case is not correct in case of odd value of UTRA-CarrierRSSI.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-19T18:19:04.627","2015-09-17T09:01:58.263","C6-150438","","Rel-13","31.124","13.0.0","TEI13","0428","1","F","CP-150562","","","","",""]
["C6-150475","Relaxing the mandatory clause & Making features optional","BlackBerry UK Limited","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"revised","2015-08-19T18:58:08.433","2015-09-17T09:01:58.590","C6-150440","C6-150480","Rel-13","31.121","12.3.0","Red_UCe","0200","1","C",null,"","","","",""]
["C6-150476","Change the number of EFs at the MF level","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"revised","2015-08-19T19:08:28.887","2015-08-19T19:09:33.690","C6-150471","C6-150477","Rel-12","31.102","12.8.1","TEI12","0647","1","F",null,"","","","",""]
["C6-150477","Alignment of EFs at the MF level with TS 31.101","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"agreed","2015-08-19T19:43:57.807","2015-08-19T19:49:15.170","C6-150476","","Rel-12","31.102","12.8.1","TEI12","0647","2","F","CP-150561","","","","",""]
["C6-150478","Alignment of EFs at the MF level with TS 31.101","China Mobile","Xavier Piednoir",32337,"CR","","Decision","","","49","7.7.1","TEI 12 (TEI12)",0,"agreed","2015-08-19T19:46:14.320","2015-08-19T19:49:15.357","","","Rel-13","31.102","13.0.0","TEI12","0648","","A","CP-150561","","","","",""]
["C6-150479","Alignment of UICC polling interval with eDRX cycle","QUALCOMM Incorporated","Xavier Piednoir",32337,"CR","","Decision","eDRX feature is introduced to reduce the amount of power for specific classes of devices. In those cases, it is desirable to also extend the UICC polling interval to avoid unnecessary polling while the device has negotiated an extended DRX cycle with the network.","","52","7.8","Rel-13",0,"postponed","2015-08-19T22:09:48.463","2015-08-19T22:11:13.780","C6-150470","C6-150519, C6-150561, C6-150587","Rel-13","31.101","12.2.0","eDRX-CT","0083","2","C",null,"","","","",""]
["C6-150480","Relaxing the mandatory clause & Making features optional","BlackBerry UK Limited","Xavier Piednoir",32337,"CR","","Decision","","","54","7.8.2","Review of dedicated 3GPP UICC features (Red_UCe)",0,"agreed","2015-08-19T22:29:29.907","2015-09-17T09:01:58.823","C6-150475","","Rel-13","31.121","12.3.0","Red_UCe","0200","2","C","CP-150564","","","","",""]
["C6-150481","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences","Comprion GmbH, Vodafone GmbH","Xavier Piednoir",32337,"CR","","Decision","This CR adds the following REFRESH test case sequences to TS 31.124:\nSeq 2.1 REFRESH, UICC Reset for IMSI Changing procedure\nSeq 2.3 REFRESH, 3G Session Reset for IMSI Changing procedure\nSeq 2.x REFRESH, reject UICC Reset for IMSI Change procedure during CS call\nSeq 2.y REFRESH, UICC Reset for IMSI Change procedure during PDN Connection\nSeq 2.z REFRESH, 3G Session Reset for IMSI Change procedure during PDN Connection","","52","7.8","Rel-13",0,"revised","2015-08-20T16:03:24.357","2015-08-20T16:16:41.917","C6-150462","C6-150484","Rel-13","31.124","13.0.0","TEI13","0424","2","B",null,"","","","",""]
["C6-150482","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences for E-UTRAN","Comprion GmbH","Xavier Piednoir",32337,"CR","","Decision","LS S-15-161r1 from GCF SG to 3GPP TSG CT6 asking for additional USAT Confirmance Criteria to cover existing REFRESH command qualifiers according to current market requirements. Up to now no test case was defined for testing REFRESH command qualifiers when the terminal is connected to E-UTRAN.","","53","7.8.1","TEI 13 (TEI13)",0,"revised","2015-08-20T16:05:16.677","2015-08-20T18:40:57.740","C6-150463","C6-150486","Rel-13","31.124","13.0.0","TEI13","0425","2","B",null,"","","","",""]
["C6-150483","Emergency ePDG identifier configuration","Gemalto","Xavier Piednoir",32337,"CR","","Decision","","","53","7.8.1","TEI 13 (TEI13)",0,"postponed","2015-08-20T16:25:51.827","2015-08-20T16:29:39.260","","C6-150562, C6-150588","Rel-13","31.102","13.0.0","TEI13, SEW1-CT","0649","","F",null,"","","","",""]
["C6-150484","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences","Comprion GmbH, Vodafone GmbH","Xavier Piednoir",32337,"CR","","Decision","This CR adds the following REFRESH test case sequences to TS 31.124:\nSeq 2.1 REFRESH, UICC Reset for IMSI Changing procedure\nSeq 2.3 REFRESH, 3G Session Reset for IMSI Changing procedure\nSeq 2.x REFRESH, reject UICC Reset for IMSI Change procedure during CS call\nSeq 2.y REFRESH, UICC Reset for IMSI Change procedure during PDN Connection\nSeq 2.z REFRESH, 3G Session Reset for IMSI Change procedure during PDN Connection","","52","7.8","Rel-13",0,"agreed","2015-08-20T17:28:55.477","2015-08-20T17:30:04.647","C6-150481","","Rel-13","31.124","13.0.0","TEI13","0424","3","B","CP-150562","","","","",""]
["C6-150485","Reply LS on need for Enhanced USAT Testing","3GPP CT6","Xavier Piednoir",32337,"LS out","","Decision","","","18","6.3","Outgoing liaison statements",0,"revised","2015-08-20T18:22:18.667","2015-09-17T09:01:59.027","","C6-150488","","","","","","","","","C6-150418","GCF Steering Group"]
["C6-150486","USAT Testing Enhancement by addition of REFRESH with IMSI changing procedure test sequences for E-UTRAN","Comprion GmbH","Xavier Piednoir",32337,"CR","","Decision","LS S-15-161r1 from GCF SG to 3GPP TSG CT6 asking for additional USAT Confirmance Criteria to cover existing REFRESH command qualifiers according to current market requirements. Up to now no test case was defined for testing REFRESH command qualifiers when the terminal is connected to E-UTRAN.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-20T18:40:19.270","2015-08-20T18:40:57.910","C6-150482","","Rel-13","31.124","13.0.0","TEI13","0425","3","B","CP-150562","","","","",""]
["C6-150487","Alignment of Provide Local Information for Timing Advance to E-UTRAN radio technology","Gemalto N.V.","Xavier Piednoir",32337,"CR","","Decision","Timing advance information is available in the ME when it is connected to GERAN or E-UTRAN. However, the Provide Local Information USAT specification restricted the availability of the information to GERAN as the information was not avaialble in UTRAN. It is proposed to align the availability of the information to the support of E-UTRAN technology.","","53","7.8.1","TEI 13 (TEI13)",0,"agreed","2015-08-20T18:57:11.237","2015-08-20T19:03:31.437","C6-150466","","Rel-13","31.111","13.0.0","TEI13","0436","3","B","CP-150563","","","","",""]
["C6-150488","Reply LS on need for Enhanced USAT Testing","3GPP CT6","Xavier Piednoir",32337,"LS out","","Decision","","","18","6.3","Outgoing liaison statements",0,"revised","2015-08-20T19:27:16.300","2015-08-20T19:33:34.113","C6-150485","C6-150489","","","","","","","","","C6-150418","GCF SG","GCF CAG"]
["C6-150489","Reply LS on need for Enhanced USAT Testing","3GPP CT6","Xavier Piednoir",32337,"LS out","","Decision","","","18","6.3","Outgoing liaison statements",0,"approved","2015-08-20T19:36:42.373","2015-08-20T19:40:16.997","C6-150488","","","","","","","","","","C6-150418","GCF SG","GCF CAG"]
["C6-150490","Meeting Agenda with document allocation and document status","WG Chairman","Xavier Piednoir",32337,"agenda","","Decision","","","4","3.1","Agreement of the agenda and the scheduling",0,"noted","2015-08-20T20:28:35.397","2015-09-17T09:01:59.230","C6-150411","","","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","reserved","A","Decision"]
["Work Plan","available","B","Agreement"]
["LS in","revised","C","Approval"]
["LS out","agreed","D","Information"]
["pCR","conditionally agreed","E","Discussion"]
["draftCR","approved","F","Action"]
["CR","conditionally approved",null,"Endorsement"]
["CR pack","partially approved",null,"Presentation"]
["ToR","treated"]
["WID new","endorsed"]
["WID revised","replied to"]
["SID new","merged"]
["SID revised","not pursued"]
["WI status report","postponed"]
["WI exception request","noted"]
["TS or TR cover","not concluded"]
["draft TS","withdrawn"]
["draft TR","reissued"]
["report"]
["discussion"]
["response"]
["other"]