[103-e-NR-Rel-16-V2X-02] Email discussion/approval regarding location of PSFCH/PSSCH/PSCCH/2nd SCI mapping and PSCCH precoding

* Issue PS-2-1: To clarify starting symbol and location for PSFCH
* Issue PS-2-2: To clarify time-domain location of PSSCH
* Issue PS-2-3: To clarify time-domain and frequency-domain location of PSCCH

till 10/29, with a potential CR by 11/4 – Jeongho (Samsung)

# **Issue PS-2-1. To clarify starting symbol and location for PSFCH**

Six contributions [LGE], [Intel], [Sharp], [ASUSTek], [NTT DCM], [Qualcomm] discuss on this topic, which is related to the yellow-highlighted part below in TS38.211.

|  |
| --- |
| 8.3.4.2 PSFCH format 0  8.3.4.2.1 Sequence generation  The sequence shall be generated according to  where is given by clause 6.3.2.2 with the following exceptions:  - is given by clause 16.3 of [5, TS 38.213];  - is given by clause 16.3 of [5, TS 38.213];  - is the OFDM symbol number in the PSFCH transmission where corresponds to the first OFDM symbol of the PSFCH transmission;  - is the index of the OFDM symbol in the slot that corresponds to the first OFDM symbol of the PSFCH transmission in the slot given by [5, TS 38.213];  - and with given by the higher-layer parameter *sl-PSFCH-HopID* if configured; otherwise, .  - with given by the higher-layer parameter *sl-PSFCH-HopID* if configured; otherwise, .  8.3.4.2.2 Mapping to physical resources  The sequence shall be multiplied with the amplitude scaling factor in order to conform to the transmit power specified in [5, TS 38.213] and mapped in sequence starting with to resource elements assigned for transmission according to clause 16.3 of [5, TS 38.213] in increasing order of first the index over the assigned physical resources, and then the index on antenna port.  The resource elements used for the PSFCH in the first OFDM symbol in the mapping operation above, including any DM-RS, PT-RS, or CSI-RS occurring in the first OFDM symbol, shall be duplicated in the immediately preceding OFDM symbol. |

* Alt 1. Describe PSFCH starting at symbol *startSLsymbols* + *lengthSLsymbols* - 2 in TS38.214 [LG]
* Alt 2. Describe as “The first OFDM symbol of the PSFCH transmission 𝑙′ is defined as 𝑙′ = startSLsymbols + *lengthSLsymbols* – 2.” in Clause 16.3 of TS38.213 [Intel], [ASUSTeK], [NTT DCM]
* Alt 3. Change the above yellow-highlighted to “ is the index of the OFDM symbol in the slot that corresponds to the last but one OFDM symbol available for SL transmission in the slot” in Clause 8.3.4.2.1 of TS38.211 [Sharp]
* Alt 4. Clarify that there is only one PSFCH symbol in Clause 8.2.1 of TS38.211 and describe as “In a slot with PSFCH transmission occasion, PSFCH resources are in the OFDM symbol that is two symbols after the last OFDM symbol with PSSCH resources in that slot.” in Clause 16.3 of TS38.213. [Qualcomm]

Please provide your views and reason.

|  |  |
| --- | --- |
| **Company** | **Views** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# **Issue PS-2-2. To clarify time-domain location of PSSCH**

Two contributions [Sharp], [LG] discuss on this topic, which is related to the yellow-highlighted part below in TS38.214.

|  |
| --- |
| 8.1.2.1 Resource allocation in time domain  The UE shall transmit the PSSCH in the same slot as the associated PSCCH.  The minimum resource allocation unit in the time domain is a slot.  The UE shall transmit the PSSCH in consecutive symbols within the slot, subject to the following restrictions:  - The UE shall not transmit PSSCH in symbols which are not configured for sidelink. A symbol is configured for sidelink, according to higher layer parameters *startSLsymbols* and *lengthSLsymbols*, where *startSLsymbols* is the symbol index of the first symbol of *lengthSLsymbols* consecutive symbols configured for sidelink.  - Within the slot, PSSCH resource allocation starts at symbol *startSLsymbols+1.*  - The UE shall not transmit PSSCH in symbols which are configured for use by PSFCH, if PSFCH is configured in this slot.  - The UE shall not transmit PSSCH in the last symbol configured for sidelink.  - The UE shall not transmit PSSCH in the symbol immediately preceding the symbols which are configured for use by PSFCH, if PSFCH is configured in this slot. |

* [LG] proposes to describe “The UE shall not transmit PSSCH in symbols which are configured for use by PSFCH starting at symbol *startSLsymbols* + *lengthSLsymbols* - 2, if PSFCH is configured in this slot” (Same as Alt 1 of Issue PS-2-1 above)
* [Sharp] proposes that, the last bullet is changed into “The UE shall not transmit PSSCH in the two consecutive symbols immediately preceding the symbol(s) which are configured for use by PSFCH, if PSFCH is configured in this slot.”

Please provide your views and reason including whether the change is needed or not.

|  |  |
| --- | --- |
| **Company** | **Views** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# **Issue PS-2-3. To clarify time-domain and frequency-domain location of PSCCH**

Two contributions [ZTE, Sanechips], [ASUSTeK] discuss on this topic, which is related to the yellow-highlighted part below in TS38.213.

|  |
| --- |
| 16.4 UE procedure for transmitting PSCCH  A UE can be provided a number of symbols in a resource pool, by *timeResourcePSCCH*, starting from a second symbol that is available for SL transmissions in a slot, and a number of PRBs in the resource pool, by *frequencyResourcePSCCH*, for a PSCCH transmission with a SCI format 1-A. |

* [ZTE, Sanechips] proposes to change the above as
  + A UE can be provided a number of symbols in a resource pool, by *timeResourcePSCCH*, starting from symbol *startSLsymbols+1* ~~a second symbol that is available for SL transmissions~~ in a slot, and a number of PRBs in the resource pool, by *frequencyResourcePSCCH,* starting from the lowest PRB of the lowest sub-channel of the associated PSSCH, for a PSCCH transmission with a SCI format 1-A.
* [ASUSTeK] proposes three options for the first symbol of PSCCH.
  + Option 1: Add “The first OFDM symbol of a PSCCH is at the same symbol as the first OFDM symbol of its associated PSSCH” in Clause 8.2.1 of TS38.211.
  + Option 2: Add “The first OFDM symbol of a PSCCH is the OFDM symbol immediately next to the OFDM symbol indicated by *sl-StartSymbol*.” in Clause 8.3.2.3 of TS38.211.
  + Option 3: Add “The first OFDM symbol of a PSCCH is at symbol *sl-StartSymbol*+1.” in Clause 8.3.2.3 of TS38.211.

Please provide your views and reason including whether the change is needed or not.

|  |  |
| --- | --- |
| **Company** | **Views** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Reference

1. R1-2007610 Correction on sidelink PT-RS sequence generation Huawei, HiSilicon
2. R1-2007772 Discussion on essential corrections in physical layer structure LG Electronics
3. R1-2007809 Remaining issues on physical layer structure for NR sidelink CATT
4. R1-2007921 Remaining issues of NR sidelink physical layer structure ZTE, Sanechips
5. R1-2007934 Remaining opens of sidelink physical structure for NR V2X design Intel Corporation
6. R1-2008129 Text Proposals on Physical Layer Structures for NR Sidelink Samsung
7. R1-2008230 Draft TP on physical structure for NR sidelink OPPO
8. R1-2008381 Remaining issue on physical layer structure and procedure for sidelink in NR V2X Panasonic Corporation
9. R1-2008387 Remaining issues on physical layer structure for NR sidelink Sharp
10. R1-2008429 Remaining Issue of Sidelink Physical Layer Structure Apple
11. R1-2008496 Maintenance for PSFCH and PSCCH symbol on NR sidelink ASUSTeK
12. R1-2008529 Maintenance for sidelink physical layer structure NTT DOCOMO, INC.
13. R1-2008604 Remaining Issues in Physical Layer Structure Qualcomm Incorporated
14. R1-2008665 Remaining issues on physical layer structure for NR sidelink vivo
15. R1-2008750 Discussion paper on the remaining issues in Rel. 16 for NR V2X Ericsson