**3GPP TSG RAN WG1 Meeting #103-E R1-** **200xxxx**

**e-Meeting, October 26th – November 13th, 2020**

**Source: Moderator (Intel Corporation)**

**Title: Discussion on [103-e-NR-Rel-16-V2X-04]**

**Agenda item: 7.2.4**

**Document for:** **Discussion and Decision**

Introduction

This contribution provides discussion on critical issues for the thread [103-e-NR-Rel-16-V2X-04].

[103-e-NR-Rel-16-V2X-04] Email discussion/approval regarding e-evaluation procedure for periodic resource reservations

* Issue M2-1: Fix undefined UE behaviour for the case of re-evaluation performed during periodic reservation process
* Issue M2-7: Fix the issue of unreachable pre-emption event condition due to prior exclusion of slots related to non-monitored slots in the sensing window

till 10/30, with a potential CR by 11/4 – Sergey (Intel)

Outcome summary

Text proposal

1st round discussion

## Issue M2-1: Fix undefined UE behaviour for the case of re-evaluation performed during periodic reservation process

It is currently uncertain in specification whether a UE should perform re-evaluation procedure only before SCIs of the first period after the re-selection, or before ant SCI regardless of the periodic occasion.

In the last meeting the issue was discussed but no final decision was made. The following was one of the latest proposals:

|  |
| --- |
| **Updated Proposal*** If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure at least for resource(s) in the first period after the initial resource re-selection trigger or for resources in non-initial resource re-selection triggered by pre-emption
	+ Allow discussion in the next meeting whether re-evaluation in other than the first period is feasible and can be allowed for the UE implementation
	+ Note, this is intended to be captured in MAC specification
	+ Note, the initial resource re-selection trigger refers to the initial (re-)selection triggered according to clause 5.22.1.2 of TS 38.321, except resource re-selection triggered by re-evaluation and pre-emption
 |

This option was not supported by a few sources since it precludes re-evaluation every period. However, it was argued that if ‘sl-ReselectAfter’ is configured to 0 or a smaller value, then it may be already possible to do re-evaluation/re-selection when there is no packet transmission in a period.

Another issue found with re-evaluation every period is self-blocking due to step 5) execution. Similar to Issue M2-7, the resource being re-evaluated overlaps with the slot which should be excluded in step 5). In this case, after execution of steps 1)-7), the resource will not be in S\_A, even if there was no collision.

In order to facilitate decision in this meeting, the following set of questions is presented, based on the following two options:

**Option 1:**

* If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure only for resource(s) in the first period after the initial resource re-selection trigger or for resources in non-initial resource re-selection triggered by pre-emption
	+ Note, this is intended to be captured in MAC specification as a restriction when and which resource for re-evaluation can be passed to PHY
	+ Note, the initial resource re-selection trigger refers to the initial (re-)selection triggered according to clause 5.22.1.2 of TS 38.321, except resource re-selection triggered by re-evaluation and pre-emption

**Option 2:**

* If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure for resource(s) in every period by the following procedure
	+ During re-evaluation check for resources indicated by a prior SCI with a period, step 5) in 8.1.4 of 38.214 is omitted during re-evaluation check
	+ During re-evaluation check for resources indicated by a prior SCI with a period, in step 6)-c) in 8.1.4 of 38.214, j is let to be ‘1 to Cresel-1’ for re-evaluation, i.e. collision checking is skipped for the nearest period
	+ If the resource is not in the identified resource set, then re-evaluation is indicated to MAC layer
	+ MAC layer resets SL\_RESOURCE\_RESELECTION\_COUNTER following agreed procedures
	+ In SCI, which was supposed to reserve the re-evaluated resource with a period, the reservation period is set to 0

**Q1-1: Does the above description of Option 1 capture the intention of performing re-evaluation only for resource in the first period? Please answer even if you don’t support Option 1.**

|  |  |  |
| --- | --- | --- |
| **Source** | **Short answer** | **Comments** |
| LG Electronics | Yes |  |
| Qualcomm | No | If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure only for resource(s) in the first period after the initial resource re-selection trigger or for resources that has not been signalled in the immediate last or current SPS period.The resource may not be reserved by the immediate last SPS period due to transmission drop (congestion control, prioritization, etc.), feedback not triggered, or pre-emption in the immediate last SPS. |
| NTT DOCOMO | Yes |  |
| Panasonic | Yes |  |
| Vivo | Yes |  |
| ZTE | Yes |  |
| Apple | Yes |  |
| Sharp | Yes |  |
| OPPO | Yes and No | Generally, agree with Option 1’s wording and we also see QC’s point that resources in the immediate last period may be dropped due to prioritization and congestion control causing the resources in the current period being un-reserved. We suggest to modify the main bullet of Option 1 as:“If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure only for resource(s) in the first period after the initial resource re-selection trigger, for resources in non-initial resource re-selection triggered by pre-emption, or for resources in the current period that has not been signalled in the immediate last” |
| Samsung | Yes |  |
| CATT | Yes |  |
| Huawei/HiSilicon | Yes with minor update | Technically, after re-valuation, the UE can still perform re-evaluation, it’s up to UE implementation. But it seems this case is not captured in Option 1. So maybe in Option 1, in the last part of the main bullet, we need to change “pre-emption” to “pre-emption/re-evaluation”? |
| Futurewei | Yes |  |
| Nokia, NSB | Yes |  |

**Based on the comments it seems the description of Option 1 is mostly accurate. For the comments on the skipped immediate previous period and current period, it seems there was no such intention in Option 1. The proposal from Qualcomm and OPPO creates another option.**

**Q1-2: Does the above description of Option 2 capture the intention of performing re-evaluation in every period? Please answer even if you don’t support Option 2.**

|  |  |  |
| --- | --- | --- |
| **Source** | **Short answer** | **Comments** |
| LG Electronics | Difficult to understand the exact behaviour of Option 2 with the current description. | At least the following comments should be clarified:* What does the sentence of “collision checking is skipped for the nearest period” mean? Is this correct understanding that even though the re-evaluation check for the resources within the current period is performed assuming these resource are periodically reserved “Cresel-1” times, but the resource re-selection can be triggered by this check is limited to the resources within the current period?
* What’s the target behaviour/technical motivation with the sentence of “MAC layer resets SL\_RESOURCE\_RESELECTION\_COUNTER following agreed procedures”?

FL comment:“Collision checking is skipped for the nearest period” is intended to say that in the current/nearest period corresponding to j = 0, the resources have been already reserved by prior SCI in immediate previous period. Thus, these resources could not be re-evaluated.“MAC layer resets SL\_RESOURCE\_RESELECTION\_COUNTER following agreed procedures” means that re-selection due to re-evaluation resets the reselection counter since is equal to the change of resources due to full re-selection. |
| Qualcomm | No | During re-evaluation check for resources indicated by a prior SCI with a period, in step 6)-c) in 8.1.4 of 38.214, j is let to be ‘1’ for re-evaluation, i.e. collision checking is performed for the immediate next periodThe second last is not needed. It’s up to UE to do a full resource selection, or just transmit next period using per packet scheduling and then switch back to current resource in the next-next period. |
| NTT DOCOMO | Yes |  |
| Panasonic | Yes |  |
| Vivo | No | To us, it is not necessary to change steps in 214, even we may accept the re-evaluation check to periodic resource. So, the proposal should eliminate RAN1 spec. change.Our suggestion for progress as following:1. We do not support cross-period check, which has been discussed multiple rounds without consensus.2. We prefer a simple solution directly addressing companies’ concern who do not support option 1. To my best understanding, re-evaluation is only applied to resources which is regarded as occupied resource from proximity-UE perspective. Based on 214, the following resource is un-occupied resource from proximity-UE as commented by QC ‘resources that has not been signalled in the immediate last or current SPS period’. We agree that those resources can be re-evaluation. Based on the discussion, we suggest following proposal (red colored part is changed based on agreement for pre-emption check) for option 2 for further discussion. * If periodic reservation is in use by a UE, the UE perform re-evaluation check for resources provided by MAC layer to L1, according to specified procedures
	+ L1 expects that MAC layer provides resources intended for transmission of one TB, which can fit to resource selection window of current TB of the UE, and for which the relevant priority is available
	+ Re-evaluation check is not applied to the resources that have been signaled in the immediate last or current period
	+ If a resource is indicated for re-evaluation, a re-selection for the resource is triggered based on the specified step 1 and step 2 procedures,
		- with details up to UE implementations, including whether/how to set the reservation period in the re-selected resource
 |
| ZTE | Partially Yes (See comment) | We agree with most bullets of option 2 except last bullet. From our understanding, once UE triggered resource reslection due to re-evaluation, it is up to UE implementation to select either the next period resource or the set of following periods resources. It is not preferred to add the restriction to say UE can only reselect resource for one period due to re-evaluation. So the last bullet is suggested to be removed. |
| Sharp | No | We share similar view as Qualcomm. |
| OPPO | Same as LGE | In addition to LGE’s questions:As for “In SCI, which was supposed to reserve the re-evaluated resource with a period, the reservation period is set to 0”, does it mean that UE can re-select a resource in upcoming period when UE performs re-evaluation check in current period? But UE can only select a resource within a selection window and the selection window is defined and covers only the current period.We may have more questions after. |
| Huawei/HiSilicon | Unclear about Option 2 | In Option 2, we are unclear about the 2nd sub-bullet and 4th sub-bullet, i.e., why we need “j is let to be ‘1 to Cresel-1’ for re-evaluation” and “MAC layer resets SL\_RESOURCE\_RESELECTION\_COUNTER”?**FL comment:****See reply to LGE**And we think the 1st sub-bullet is against previous agreement (copied below). According to the cyan part of the following agreements in RAN1#98b, the re-evaluation is performed before transmission of SCI with reservation.Agreements:* Resource (re-)selection procedure supports re-evaluation of Step 1 and Step 2 before transmission of SCI with reservation
	+ The re-evaluation of the (re-)selection procedure for a resource reservation signalled in a moment ‘m’ is not required to be triggered at moment > ‘m – T3’ (i.e. resource reselection processing time needs to be ensured)
	+ FFS condition to change resource(s) from previous iteration to resource(s) from current iteration
	+ FFS relationship of T1 and T3, if any
	+ FFS whether to handle it differently for blind and feedback-based retransmission resources
 |
| Futurewei |  | We do not fully understand what the second bullet wants to capture:* + During re-evaluation check for resources indicated by a prior SCI with a period, in step 6)-c) in 8.1.4 of 38.214, j is let to be ‘1 to Cresel-1’ for re-evaluation, i.e. collision checking is skipped for the nearest period

Generally speaking, option 2 is more complicated and not as clear as option 1 |
| Nokia, NSB | Not sure | I need to think about this option a bit more. |

**Based on the comments, it seems the intention of modifying j to start from 1 is not clear to everyone. Similar situation is with some other sub-bullets, i.e. the realization of Option 2 is not yet stable.**

**Q1-3: Based on essentiality, spec impact, and backward compatibility which option (or any other alternative) should be implemented?**

|  |  |  |
| --- | --- | --- |
| **Source** | **Short answer** | **Comments** |
| LG Electronics | Option 1 |  |
| Qualcomm | Option 1 + Option 2  | The options as described is not exclusive. Re-evaluation for each period is needed anyway for reason explained in Q1-1. |
| NTT DOCOMO | Option 1 | Once periodic resources are reserved is signalled by TX UE, RX UE and surrounding UE(s) would exclude them at their own step 6. So from resource utilization perspective, it is important that a TX UE utilizes their reserved resources as much as possible.  |
| Panasonic | Option 1+ UE implementation  | We think it’s necessary to perform re-evaluation for the 1st period but not every period. It may up to implementation whether a UE needs to drop the entire periodic reservations when meet certain numbers of failures. Therefore, the “at least for resource(s) in the first period …” with the current proposal is ok to us. |
| vivo |  | Not necessary to down-select in-between, which has been done in previous meeting, however failed. It is suggested to compromise to a simple solution. |
| ZTE | Option 2 + UE implementation | For periodic traffic, if re-evaluation is limited to the first period, then the resource conflict cannot be avoided in the subsequent periods even if some resource collisions are detected. Therefore, we support option 2. In addition, it is up to UE implementation to reselect either the next period or the set of following periods resource(s). |
| Apple | Option 1 + UE implementation |  |
| Sharp | Option 1 | We support to keep the re-evaluation as it was defined “pre-selected resource(s)” in the agreements. |
| OPPO | Option 1 | Option 2 will lead to so much modifications of the spec. And it violates at least the definition of selection window. |
| Samsung | Option 1 |  |
| CATT | Option 1 |  |
| Huawei/HiSilicon | Option 1 | Option 2 leads to too many specification changes, and the benefits are unclear. |
| Futurewei | Option 1 |  |

**Based on the views, it seems Option 1 has majority support. There is also an interesting compromise from vivo which can be checked for support.**

**Q1-4: Any other compromise proposals / comments helping to resolve the outstanding issue?**

|  |  |
| --- | --- |
| **Source** | **Comments** |
| Ericsson | We are not sure that everyone is discussing the same thing. In our view, it is at least necessary to be able to re-evaluate/re-select for the upcoming period. Consider a UE using Mode2 with a reservation period:* At time n, it selects resources n+k, n+k+P, n+k+2P, n+k+3P, …
* At time n+k+j\*P, it reserves resource n+k+(j+1)\*P for j = {0,1,2,…}

Being able to to reselect resources for the coming period consist of:* Prior to the transmission in resource n+k, the UE should re-evaluate the selected but-not-yet-reserved resource n+k+P.
	+ If resource n+k+P is available, go ahead and reserve it.
	+ If not, reselect.
* Prior to the transmission in resource n+k+(j+1)\*P, the UE should re-evaluate the selected but-not-yet-reserved resource n+k+(j+2)\*P.
	+ If resource n+k+(j+2)\*P is available, go ahead and reserve it.
	+ If not, reselect.
* In general (for j={0,1,2,…}), prior to the transmission in resource n+k+j\*P, the UE should re-evaluate the selected but-not-yet-reserved resource n+k+(j+1)\*P.
	+ If resource n+k+(j+1)\*P is available, go ahead and reserve it.
	+ If not, reselect.

We would also be fine with UEs being able to make changes further ahead in time, but the preceding behaviour is the minimum that we think is necessary.**FL comment: In my understanding, your example describes Option 2** |
| vivo | As commented above |
| OPPO | Based on the example of Ericsson, we think that, prior to the transmission in resource n+k, UE performs re-evaluation. During the regular Step 1 of re-evaluation, UE will check whether there is a collision on resource n+k+P because j is up to Cresel-1. If the collision exists, UE will re-select a resource from the selection window in the current period to replace resource n+k. The corresponding resources in upcoming periods (n+k+P,n+k+2p…) will be changed due to the re-selection of n+k. Hope both interpretations can make this issue more clearly. |
| Qualcomm 2 | To further clarify, there are 2 types of re-evaluation here.1/ Re-evaluation for the purpose of using the resource for transmission in the current period: this should be done every period for the resources in this period that has not been reserved by current period or immediately previous period.2/ Re-evaluation for the purpose of signalling SPS reservation for the next period: this should be done every period for the resources in the next SPS period. We think that Ericsson description of the procedure correctly capture our intention. Once a collision is detected, the UE should not signal SPS reservation period for the next SPS period. It is up to UE to use per packet scheduling for the next period and switch back to the SPS grant for the one after that, or reselect the whole SPS grant from next period. |

## Issue M2-7: Fix the issue of unreachable pre-emption event condition due to prior exclusion of slots related to non-monitored slots in the sensing window

In NR SL Mode-2, when pre-emption enabled a UE performs pre-emption checking with both aperiodic and periodic traffic. In case of periodic reservation is enabled in the pool, a UE checks for pre-emption event by comparing RSRP and priority. However, the procedure of resource identification performed by the UE also includes step 5) which excludes slots in the selection window related to slots not monitored in the sensing window, with the set of periodicities configured in the resource pool.

Even if only one period is configured, a UE can face the issue that pre-emption condition is never reached even if there are collisions. This is illustrated in Figure 1 from [1].



Figure 1. Reserved resource with period P during pre-emption

In order to avoid the issue, step 5) may need to be modified for the case when executed during pre-emption checking it does not exclude the reserved resource subject to pre-emption.

**Q2-1: Do you agree that the issue is valid and need to be resolved?**

|  |  |  |
| --- | --- | --- |
| **Source** | **Short answer** | **Comments** |
| LG Electronics | Not critical (i.e., further agreement is not necessary) | Even in Figure 1, according to the current specification, there could be a case that a UE performing the pre-emption checking triggers the resource re-selection of periodically reserved resource if such resource is overlapped with other UE’s resource (e.g., aperiodic resource selection) with a priority satisfying the pre-emption condition, which is identified in a slot different from the location of its periodically reserved resource. |
| Ericsson | OK to correct or clarify | The following agreement is ambiguous:Agreements:* The procedure to check whether a reserved resource to be signaled in slot ‘m’ should be re-selected due to pre-emption:
	+ A regular Step 1 (as in 8.1.4 in 38.214) of the resource (re-)selection procedure is performed
	+ If the reserved resource is still in the identified candidate resource set after the Step 1 execution, then Step 2 for reselection of the reserved resource(s) is not triggered
	+ If the reserved resource is NOT in the identified candidate resource set after the Step 1 execution
		- If the resource is excluded by comparison with the RSRP measurement for an SCI associated with a priority which can trigger pre-emption, then Step 2 for reselection of the reserved resource(s) is triggered
		- If the resource is excluded by comparison with the RSRP measurement for an SCI associated with a priority which cannot trigger pre-emption, then Step 2 for reselection of the reserved resource(s) is not triggered

In our understanding, the case discussed here does not fit into any of the two highlighted sub-bullets. In fact if a resource is excluded in Step 5, then it will not be checked in Step 6.We do not think that a procedure that forces a UE to reselect resources always is reasonable or supported by agreements. |
| Qualcomm | Yes | This is an issue for both pre-emption and re-evaluation. |
| NTT DOCOMO | Yes | We agree with Ericsson’s points that “In fact if a resource is excluded in Step 5, then it will not be checked in Step 6.We do not think that a procedure that forces a UE to reselect resources always is reasonable or supported by agreements”.  |
| Panasonic | Yes |  |
| vivo | No | What if the pre-empting UE sends SCI in the non-monitored slots. Then the pre-empting UE cannot be detect. The benefit of the change is not easy to be justified. |
| ZTE | Yes | For pre-emption, there is not available priority of the resources excluded in step 5, so here this step is not necessary. |
| Apple | Yes |  |
| Sharp | Yes | We share the view as Ericsson and DCM. |
| OPPO | Yes | Same as QC |
| Samsung | Yes | We share the view as Ericsson |
| CATT | YEs | When performing sensing based resource exclusion operations for periodic service, the selected and reserved resource(s) would be excluded in Step 5) but there is no RSRP measurements and priority value in the hypothetical SCI format 1-A. then in Step 6), the excluded resource(s) would not be checked. Because of the absent of RX priority, the reselection cannot be triggered during the pre-emption check. So we think it should be clarified and resolved. |
| Huawei/HiSilicon | Yes | If a resource is already excluded in step 5, it will not be checked in step 6. So it’s unclear whether this resource is actually pre-empted or not.  |
| Futurewe | Yes | Not absolutely critical to fix, but okay to address |
| Nokia, NSB | Yes | OK to fix even though it is doubtful if this is critical/essential. |

**Based on the comments, it seems the issue can be acknowledged.**

**Q2-2: If you think the issue is valid, what solution can be applied?**

* **Examples:**
	+ **Skip step 5) during pre-emption check**
	+ **Do not include TX period when executing step 5)**
	+ **Swap step 5) and step 6)**
	+ **Etc.**

|  |  |
| --- | --- |
| **Source** | **Comments** |
| Qualcomm | Skip step 5) for pre-emption and re-evaluation. |
| NTT DOCOMO | Do not include TX period when executing step 5. Resources not corresponding to the periodic resource (i.e. resources being checked pre-emption) should be excluded at step 5 as it currently is.  |
| Panasonic | Do not include TX period when executing step 5. |
| ZTE | For both pre-emption and re-evaluation, skip step 5) |
| Apple | Do not include Tx period when executing step 5) |
| Sharp | Swap step 5 and step 6 is preferred. Since current step 5 assumes the worst case of collision, without performing it, the pre-emption check could be not thorough enough. |
| OPPO | Do not include Tx period when executing step 5) |
| Samsung | We propose to remove step 5) in Mode 2 procedure. In addition to issue M2-7, with step 5), a UE might exclude candidate resources for resource selection unnecessarily and result in performance degradation especially when short reservation periodicity is configured at higher layer. |
| CATT | Skip step 5) during pre-emption check |
| Huawei/HiSilicon | We support solution similar to 2nd sub-bullet, i.e., “Do not include TX period when executing step 5)”.If resources subject to pre-emption check have already been periodically reserved, the period associated with the reservation is excluded from the periodicity values allowed by the higher layer parameter *sl-ResourceReservePeriodList* when executing step 5). |
| Futurewei | Skip step 5)  |
| Nokia, NSB | Skip step 5 |

Skip step 5):

 6

Do not include TX period in step 5)

 5

Swap 5) and 6)

 1

It seems skipping of step 5) has slight majority. Furthermore, excluding only the TX period from step 5) still has similar issues e.g. if other periods are integer multiple of the TX period (i.e. P / n, where n is integer). Having this in mind, skipping of step 5) is proposed for pre-emption.

**Proposal 2**

* **When resource identification procedure is performed to check for pre-emption, step 5) in section 8.1.4 of TS 38.214 is not executed**

2nd round discussion

## Issue M2-1: Fix undefined UE behaviour for the case of re-evaluation performed during periodic reservation process

FL observations

* Based on the comments it seems the description of Option 1 is mostly accurate. For the comments on the skipped immediate previous period and current period, it seems there was no such intention in Option 1. The proposal from Qualcomm and OPPO creates another option, which is similar to the suggested by vivo as a compromise.
* Based on the comments, it seems the intention of modifying j to start from 1 is not clear to everyone. Similar situation is with some other sub-bullets, i.e. the realization of Option 2 is not yet stable.
	+ j was supposed to start from 1 since the case of 0 is the current period, and in usual case these resources are signalled by the immediate previous period SCI, that is why those could not be re-evaluated.
	+ The intention of re-setting SL\_RES\_RESEL\_COUNTER is to capture that re-evaluation in this case terminates the SPS process
* Based on the views, it seems Option 1 has majority support. There is also an interesting compromise from vivo which can be checked for support.

Further, almost unchanged Option 1 (as per explanation above), slightly modified Option 2, and a new Option 3 are presented aiming for another round of technical discussion.

**Option 1:**

* If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure only for resource(s) in the first period after the initial resource re-selection trigger or for resources in non-initial resource re-selection triggered by pre-emption/re-evaluation
	+ Note, this is intended to be captured in MAC specification as a restriction when and which resource for re-evaluation can be passed to PHY
	+ Note, the initial resource re-selection trigger refers to the initial (re-)selection triggered according to clause 5.22.1.2 of TS 38.321, except resource re-selection triggered by re-evaluation and pre-emption

**Option 2:**

* If periodic reservation is in use by a UE selecting resources, the UE performs re-evaluation procedure for resource(s) in every period by the following procedure
	+ During re-evaluation check for resources indicated by a prior SCI with a period, step 5) in 8.1.4 of 38.214 is omitted during re-evaluation check
	+ During re-evaluation check for resources indicated by a prior SCI with a period, in step 6)-c) in 8.1.4 of 38.214, j is let to be ‘1 ~~to Cresel-1~~’ for re-evaluation~~, i.e. collision checking is skipped for the nearest period~~, i.e. collision checking is performed for the immediate next period
	+ If the resource is not in the identified resource set, then re-evaluation is indicated to MAC layer
	+ ~~MAC layer resets SL\_RESOURCE\_RESELECTION\_COUNTER following agreed procedures~~
	+ In SCI, which was supposed to reserve the re-evaluated resource with a period, the reservation period is set to 0

**Option 3:**

* If periodic reservation is in use by a UE, the UE performs re-evaluation check for resources provided by MAC layer to L1, according to specified procedures
	+ L1 expects that MAC layer provides resources intended for transmission of one TB, which can fit to resource selection window of current TB of the UE, and for which the relevant priority is available
	+ Re-evaluation check is not applied to the resources that have been signalled in the immediate last or current period
	+ If a resource is indicated for re-evaluation, a re-selection for the resource is triggered based on the specified step 1 and step 2 procedures,
		- with details up to UE implementations, including whether/how to set the reservation period in the re-selected resource

**Proposal 1**

* TBD based on further technical discussion

|  |  |
| --- | --- |
| **Source** | **Comments** |
| QC | We support Option 2 + Option 3 |
|  |  |

## Issue M2-7: Fix the issue of unreachable pre-emption event condition due to prior exclusion of slots related to non-monitored slots in the sensing window

FL observations

* Based on the comments, it seems the issue can be acknowledged.
* Regarding the solution, the following “votes” distribution is observed
	+ Skip step 5):
		- 6
	+ Do not include TX period in step 5) or similar solution
		- 5
	+ Swap 5) and 6)
		- 1

It seems skipping of step 5) has slight majority. Furthermore, excluding only the TX period from step 5) still has similar issues e.g. if other periods are integer multiple of the TX period (i.e. P / n, where n is integer). Having this in mind, skipping of step 5) is proposed for pre-emption.

**Proposal 2**

* When resource identification procedure is performed to check for pre-emption, step 5) in section 8.1.4 of TS 38.214 is not executed

|  |  |
| --- | --- |
| **Source** | **Comments** |
| QC | Skipping step 5 for pre-emption. |
|  |  |

References

**Contributions identified by FL to contain Mode-2 related issues:**

1. [R1-2007612](file:///C%3A%5C%5CUsers%5C%5Cwanshic%5C%5COneDrive%20-%20Qualcomm%5C%5CDocuments%5C%5CStandards%5C%5C3GPP%20Standards%5C%5CMeeting%20Documents%5C%5CTSGR1_103%5C%5CDocs%5C%5CR1-2007612.zip) Remaining details of sidelink resource allocation mode 2 Huawei, HiSilicon
2. [R1-2007774](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007774.zip) Discussion on essential corrections in resource allocation for Mode 2 LG Electronics
3. [R1-2007811](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007811.zip) Remaining issues on Mode 2 resource allocation in NR V2X CATT
4. [R1-2007923](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007923.zip) Remaining issues in mode 2 ZTE, Sanechips
5. [R1-2007935](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007935.zip) Corrections related to Mode-2 resource allocation Intel Corporation
6. [R1-2007986](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007986.zip) Remaining issues on resource allocation mode 2 for NR V2X ETRI
7. [R1-2008081](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008081.zip) Maintenance for mode 2 resource allocation NEC
8. [R1-2008096](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008096.zip) Remaining issues in NR sidelink mode 2 resource allocation Spreadtrum Communications
9. [R1-2008131](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008131.zip) Draft CR on Mode 2 for NR Sidelink Samsung
10. [R1-2008132](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008132.zip) Draft CR on Sidelink Physical Duration to Logical Slot Conversion Samsung
11. [R1-2008236](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008236.zip) Remaining open issues and corrections for mode 2 RA OPPO
12. [R1-2008389](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008389.zip) Remaining issues on resource allocation mode 2 for NR sidelink Sharp
13. [R1-2008431](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008431.zip) Remaining Issues of Mode 2 Resource Allocation Apple
14. [R1-2008531](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008531.zip) Maintenance for resource allocation mechanism mode 2 NTT DOCOMO, INC.
15. [R1-2008606](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008606.zip) Remaining Issues in Mode 2 Resource Allocation Qualcomm Incorporated
16. [R1-2008633](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008633.zip) Remaining issues for Mode 2 resource allocation in NR V2X ASUSTeK
17. [R1-2008667](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008667.zip) Remaining issues on mode 2 resource allocation mechanism vivo
18. [R1-2008750](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008750.zip) Discussion paper on the remaining issues in Rel. 16 for NR V2X Ericsson
19. [R1-2008752](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008752.zip) Draft\_CR\_TS38.212 Ericsson

**Other Rel.16 NR V2X contributions**

1. [R1-2007610](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007610.zip) Correction on sidelink PT-RS sequence generation Huawei, HiSilicon
2. [R1-2007611](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007611.zip) Remaining details of sidelink resource allocation mode 1 Huawei, HiSilicon
3. [R1-2007613](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007613.zip) Remaining details of physical layer procedures for sidelink Huawei, HiSilicon
4. [R1-2007772](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007772.zip) Discussion on essential corrections in physical layer structure LG Electronics
5. [R1-2007773](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007773.zip) Discussion on essential corrections in resource allocation for Mode 1 LG Electronics
6. [R1-2007775](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007775.zip) Discussion on essential corrections in sidelink synchronization mechanism LG Electronics
7. [R1-2007776](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007776.zip) Discussion on essential corrections in physical layer procedure LG Electronics
8. [R1-2007779](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007779.zip) A remaining issue on UE procedures for reporting HARQ-ACK on uplink Fujitsu
9. [R1-2007780](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007780.zip) A remaining issue on simultaneous transmissions of uplink and PUSCH carrying sidelink HARQ-ACK Fujitsu
10. [R1-2007809](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007809.zip) Remaining issues on physical layer structure for NR sidelink CATT
11. [R1-2007810](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007810.zip) Remaining issues on Mode 1 resource allocation in NR V2X CATT
12. [R1-2007812](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007812.zip) Remaining issues on sidelink synchronization mechanism in NR V2X CATT
13. [R1-2007813](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007813.zip) Remaining issues on physical layer procedures for NR V2X CATT
14. [R1-2007921](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007921.zip) Remaining issues of NR sidelink physical layer structure ZTE, Sanechips
15. [R1-2007922](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007922.zip) Remaining issues in Mode-1 ZTE, Sanechips
16. [R1-2007924](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007924.zip) Remaining issues of synchronization ZTE, Sanechips
17. [R1-2007925](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007925.zip) Remaining issues in PHY procedures for Rel-16 sidelink ZTE, Sanechips
18. [R1-2007934](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007934.zip) Remaining opens of sidelink physical structure for NR V2X design Intel Corporation
19. [R1-2007936](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007936.zip) Corrections related to Mode-1 resource allocation Intel Corporation
20. [R1-2007987](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2007987.zip) Physical layer procedures for sidelink ETRI
21. [R1-2008095](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008095.zip) Remaining issues in NR sidelink mode 1 resource allocation Spreadtrum Communications
22. [R1-2008097](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008097.zip) Remaining issues on sidelink physical layer procedure Spreadtrum Communications
23. [R1-2008129](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008129.zip) Text Proposals on Physical Layer Structures for NR Sidelink Samsung
24. [R1-2008130](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008130.zip) Draft CR on PUCCH Power Control for NR Sidelink Mode 1 Scheduling Samsung
25. [R1-2008133](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008133.zip) Draft CR on Physical Layer Procedures for NR Sidelink Samsung
26. [R1-2008230](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008230.zip) Draft TP on physical structure for NR sidelink OPPO
27. [R1-2008231](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008231.zip) Text proposal of mode 1 for NR sidelink OPPO
28. [R1-2008232](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008232.zip) Text proposal of physical layer procedure for NR sidelink OPPO
29. [R1-2008237](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008237.zip) Corrections for FDM-based semi-static power split for in-device coexistence OPPO
30. [R1-2008334](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008334.zip) Correction on sidelink timing definition Huawei, HiSilicon
31. [R1-2008381](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008381.zip) Remaining issue on physical layer structure and procedure for sidelink in NR V2X Panasonic Corporation
32. [R1-2008387](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008387.zip) Remaining issues on physical layer structure for NR sidelink Sharp
33. [R1-2008388](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008388.zip) Remaining issues on resource allocation mode 1 for NR sidelink Sharp
34. [R1-2008390](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008390.zip) Remaining issues on synchronization mechanism for NR sidelink Sharp
35. [R1-2008391](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008391.zip) Remaining issues on physical layer procedures for NR sidelink Sharp
36. [R1-2008428](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008428.zip) Remaining Issues of Physical Layer Procedures Apple
37. [R1-2008429](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008429.zip) Remaining Issue of Sidelink Physical Layer Structure Apple
38. [R1-2008430](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008430.zip) Remaining Issues of Mode 1 Resource Allocation Apple
39. [R1-2008496](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008496.zip) Maintenance for PSFCH and PSCCH symbol on NR sidelink ASUSTeK
40. [R1-2008497](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008497.zip) Remaining issues on sidelink power control ASUSTeK
41. [R1-2008498](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008498.zip) Miscellaneous issues of SL HARQ-ACK reporting on PUCCH ASUSTeK
42. [R1-2008529](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008529.zip) Maintenance for sidelink physical layer structure NTT DOCOMO, INC.
43. [R1-2008530](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008530.zip) Maintenance for resource allocation mechanism mode 1 NTT DOCOMO, INC.
44. [R1-2008532](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008532.zip) Maintenance for sidelink physical layer procedure NTT DOCOMO, INC.
45. [R1-2008533](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008533.zip) Maintenance for sidelink-related collision NTT DOCOMO, INC.
46. [R1-2008604](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008604.zip) Remaining Issues in Physical Layer Structure Qualcomm Incorporated
47. [R1-2008605](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008605.zip) Remaining Issues in Mode 1 Resource Allocation Qualcomm Incorporated
48. [R1-2008665](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008665.zip) Remaining issues on physical layer structure for NR sidelink vivo
49. [R1-2008666](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008666.zip) Remaining issues on mode 1 resource allocation mechanism vivo
50. [R1-2008668](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008668.zip) Remaining issues on sidelink synchronization mechanism vivo
51. [R1-2008669](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008669.zip) Remaining issues on physical layer procedure for NR sidelink vivo
52. [R1-2008721](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008721.zip) Remaining issues on physical layer procedures for sidelink KT Corp.
53. [R1-2008751](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008751.zip) Draft\_CR\_TS38.211 Ericsson
54. [R1-2008753](file:///C%3A%5CUsers%5Cwanshic%5COneDrive%20-%20Qualcomm%5CDocuments%5CStandards%5C3GPP%20Standards%5CMeeting%20Documents%5CTSGR1_103%5CDocs%5CR1-2008753.zip) Draft\_CR\_TS38.213 Ericsson

1. [R1-2008754](file:///C%3A%5C%5CUsers%5C%5Cwanshic%5C%5COneDrive%20-%20Qualcomm%5C%5CDocuments%5C%5CStandards%5C%5C3GPP%20Standards%5C%5CMeeting%20Documents%5C%5CTSGR1_103%5C%5CDocs%5C%5CR1-2008754.zip) Draft\_CR\_TS38.214 Ericsson