**3GPP TSG-RAN WG1 Meeting #104-eR1-21xxxxx**

**e-Meeting, October 26th – November 13th, 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.211** | **CR** | **DRAFT** | **rev** | **-** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on DM-RS presence with PDSCH mapping type B |
|  |  |
| ***Source to WG:*** | Moderator (Lenovo) |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_unlic-Core |  | ***Date:*** | 2021-02-01 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Incomplete and incorrect description for DM-RS with PDSCH mapping type B for several PDSCH durations. |
|  |  |
| ***Summary of change:*** | 1. Correct assumption on additional single-symbol DM-RS presence for PDSCH duration of 5 symbols;
2. Correct assumption on front-loaded DM-RS presence for PDSCH duration of 5-13 symbols;
3. Correct assumption on DM-RS presence after the 12th symbol for PDSCH duration of 12-13 symbols;
4. Correct assumption on DM-RS presence for PDSCH duration other than 2, 5, 7 symbols;
 |
|  |  |
| ***Consequences if not approved:*** | Incomplete and incorrect UE assumption on presence of DM-RS symbols with PDSCH mapping type B. |
|  |  |
| ***Clauses affected:*** | 7.4.1.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

##### 7.4.1.1.2 Mapping to physical resources

< Unchanged parts are omitted >

For PDSCH mapping type B

- if the PDSCH duration OFDM symbols for normal cyclic prefix or OFDM symbols for extended cyclic prefix, and the front-loaded DM-RS of the PDSCH allocation collides with resources reserved for a search space set associated with a CORESET,  shall be incremented such that the first DM-RS symbol occurs immediately after the CORESET and until no collision with any CORESET occurs, and

- if the PDSCH duration is 2 symbols, the UE is not expected to receive a DM-RS symbol beyond the second symbol;

- if the PDSCH duration is 5 symbols and if one additional single-symbol DM-RS is configured, the UE only expects the additional DM-RS to be transmitted on the 5th symbol when the front-loaded DM-RS symbol is in the 1st symbol of the PDSCH duration, otherwise the UE should expect that the additional DM-RS is not transmitted;

- if the PDSCH duration is 7 symbols for normal cyclic prefix or 6 symbols for extended cyclic prefix:

- if one additional single-symbol DM-RS is configured, the UE only expects the additional DM-RS to be transmitted on the 5th or 6th symbol when the front-loaded DM-RS symbol is in the 1st or 2nd symbol, respectively, of the PDSCH duration, otherwise the UE should expect that the additional DM-RS is not transmitted;

- if the PDSCH duration OFDM symbols, the UE is not expected to receive the front-loaded DM-RS beyond the 4th symbol;

- if the PDSCH duration is 12 or 13 symbols, the UE is not expected to receive DM-RS mapped to symbol 12 or later in the slot;

- for all values of the PDSCH duration other than 2, 5, and 7 symbols, the UE is not expected to receive DM-RS beyond the :th symbol;

- if the PDSCH duration is less than or equal to 4 OFDM symbols, only single-symbol DM-RS is supported.

- if the higher-layer parameter *lte-CRS-ToMatchAround*, *lte-CRS-PatternList1*, or *lte-CRS-PatternList2* is configured, the PDSCH duration symbols for normal cyclic prefix, the subcarrier spacing configuration , single-symbol DM-RS is configured, and at least one PDSCH DM-RS symbol in the PDSCH allocation collides with a symbol containing resource elements as indicated by the higher-layer parameter *lte-CRS-ToMatchAround*, *lte-CRS-PatternList1*, or *lte-CRS-PatternList2*, then shall be incremented by one in all slots.

< Unchanged parts are omitted >