**3GPP TSG RAN WG1 #104-e R1-210xxxx**

**e-Meeting, January 25th – February 5th, 2021**

**Agenda item:** 8.1.1

**Source:** Moderator (Samsung)

**Title:** Moderator summary#5 for multi-beam enhancement: Round 3

**Document for:** Discussion and Decision

## Introduction

In this summary, the term “item 1” refers to the first item in the Rel.17 NR FeMIMO WID, i.e. multi-beam enhancement:

|  |
| --- |
| * Enhancement on multi-beam operation, mainly targeting FR2 while also applicable to FR1:   + Identify and specify features to facilitate more efficient (lower latency and overhead) DL/UL beam management to support higher intra- and L1/L2-centric inter-cell mobility and/or a larger number of configured TCI states:     1. Common beam for data and control transmission/reception for DL and UL, especially for intra-band CA     2. Unified TCI framework for DL and UL beam indication     3. Enhancement on signaling mechanisms for the above features to improve latency and efficiency with more usage of dynamic control signaling (as opposed to RRC)   + Identify and specify features to facilitate UL beam selection for UEs equipped with multiple panels, considering UL coverage loss mitigation due to MPE, based on UL beam indication with the unified TCI framework for UL fast panel selection |

## Summary and proposals

The summary and proposals are based on the content of the previous FL summaries R1-2101185 (preparation) and R1-2101856 (round 1).

### Issue 1 (Rel.17 unified TCI framework)

Table 1 Summary: issue 1

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 1.11 | TCI State pool for CA  Alt1: Shared among CCs  Alt2: Individually configured per CC | **Alt1 (14)**: Spreadtrum, Xiaomi, ZTE, vivo, MTK, Intel, Sony, NTT Docomo, Samsung, Qualcomm, Lenovo/MoM, Ericsson (UL TCI), IDC  **Alt2 (12)**: OPPO, Nokia/NSB, CMCC, Huawei/HiSi, CATT, APT, TCL, Ericsson (DL TCI), Futurewei, LG  **QCL Type-A implicitly determined based on CC:** Intel, Samsung, MTK, CATT, ZTE |
| 1.12 | For separate TCI, UL TCI state pool  Alt1: Shared pool with joint/DL TCI state  Alt2: Separate pool | **Alt1 (12)**: Spreadtrum, Xiaomi, ZTE, CATT, vivo, MTK, Intel, Convida, Qualcomm, Samsung, CATT, NTT Docomo  **Alt2 (15)**: Futurewei, OPPO, Lenovo/MoM, Nokia/NSB, CMCC, Ericsson, Huawei/HiSi, AT&T, Sony, Lenovo/MoM, APT |

|  |
| --- |
| Previous agreements:   * FFS: TCI state pool for CA   + Opt-1: sharing a single RRC TCI state pool for the set of configured CCs, e.g., cell-group TCI state pool, or reuse TCI state pool for PDSCH in a reference cell; A CC ID for QCL-Type A RS is absent in a TCI state, and the CC ID for QCL-Type A RS is determined according to a target CC of the TCI state.     - FFS: Whether it is possible that a single TCI state in the pool includes all source RSs from different CCs   + Opt-2: configuring RRC TCI state pool per individual CC |

|  |
| --- |
| Action: Please answer the questions below.   1. TCI state pool for CA (for common signaling of TCI state ID across CCs):    1. Since QCL Type-A reference must be CC-specific (unlike QCL Type-D), Alt1 can work only if QCL Type-A reference can be inferred via other means, e.g. “implicitly determined based on CC” (there might be other means). Could Alt1 proponents explain how QCL Type-A reference be obtained?    2. For UL TX spatial reference, is there any advantage of Alt2 over Alt1 (since Alt1 seems a natural choice)? 2. TCI state pool for separate DL/UL TCI: Considering the supported source RS types for joint TCI are a subset of those for UL-only TCI (since joint TCI applies to both DL and UL),    1. How would Alt1 overcome this limitation (otherwise the choice of UL TCI source RS types for Alt1 would be limited to that of joint TCI)?    2. Is there any advantage of Alt1 over Alt2 that justifies the potential drawback in 2a?   Goal: Finalize the proposal to be ready for endorsement |

|  |
| --- |
| **Proposal 1.1**: On Rel.17 unified TCI framework:  ... |

Table 2 Inputs: issue 1

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | Please provide inputs for the questions |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 2 (L1/L2-centric inter-cell mobility)

Table 3 Summary: issue 2

|  |  |  |
| --- | --- | --- |
| **#** | **Issue** | **Companies’ views** |
| 2.5 | Source RS type(s) applicable for L1/L2-centric inter-cell mobility  Note: currently there is no agreement on supported source RS type(s) for L1/L2-centric inter-cell mobility | SSB:   * **Yes**: * **No**:   CSI-RS for mobility:   * **Yes**: Lenovo/MoM, Huawei/HiSi, LGE, Sony. CATT, ZTE * **No**: Samsung, Qualcomm, Intel, MTK, Apple, OPPO, Nokia/NSB, Futurewei   CSI-RS for tracking:   * **Yes**: Samsung, ZTE, Futurewei, Huawei/HiSi * **No**: Qualcomm, Intel, MTK, OPPO, Nokia/NSB   CSI-RS for BM:   * **Yes**: Futurewei * **No**: |

|  |
| --- |
| Previous agreement (RAN1#103-e)   * The following enhancement scope is assumed:   + Facilitating measurement and reporting of non-serving RSs via incorporating non-serving cell info with some TCI(s), along with the necessary measurement and reporting scheme(s)     - FFS: Detailed/exact method(s)     - FFS: Whether this also implies the support of beam indication (TCI state update along with the necessary TCI state activation) for TCI(s) associated with non-serving cell RS(s)     - FFS: Metric for the measurement and reporting, e.g. L1-RSRP or L3-RSRP or time- or spatial-domain-filtered L1-RSRP     - FFS: Beam-level event-driven mechanism, using serving cell RS and/or non-serving cell RS   + … |

|  |
| --- |
| Action: Interested companies are encouraged to share their views on the following questions:   1. Supporting beam indication (TCI state update along with the necessary TCI state activation) for TCI(s) associated with non-serving cell RS(s) – yes or no? 2. If #1 is affirmative, what type(s) of source RS shall be supported for providing:    1. QCL information for UE-dedicated PDSCH/PDCCH reception?    2. UL TX spatial filter information for PUSCH/PUCCH?   Goal: Finalize the proposal to be ready for endorsement |

|  |
| --- |
| **Proposal 2.1**: On Rel.17 multi beam measurement/reporting enhancements for L1/L2-centric inter-cell mobility:  ... |

Table 4 Inputs: issue 2

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | Please provide answers to the questions |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 3 (beam indication signaling medium)

Table 5 Summary: issue 3

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **Issue** | **Companies’ views** | **Moderator notes** |
| 3.1 | Beam application time definition:  Alt1: Measured from DCI reception  Alt2: Measured from ACK transmission | **Alt1 (DCI) (7):** Spreadtrum, Xiaomi, Ericsson, CATT, MTK, NEC, Samsung  **Alt2 (ACK) (17):** IDC, Lenovo/MoM, Fujitsu, Nokia/NSB, CMCC, Apple, Huawei/HiSi, ZTE, vivo, Intel, Sony, Qualcomm, NTT Docomo, APT  **Alt1 and Alt 2:** OPPO (Since Alt1 considers the requirement of UE and Alt2 considers the requirement of gNB side), LG (Alt1 for DL assignment/PDSCH of the DCI, Alt2 else) | |

|  |
| --- |
| Previous agreement (RAN1#103-e):  On Rel.17 DCI-based beam indication:   * Regarding application time of the beam indication: if beam indication is received, down-select from the following:   + Alt1: the first slot that is at least X ms or Y symbols after the DCI with the joint or separate DL/UL beam indication   + Alt2: the first slot that is at least X ms or Y symbols after the acknowledgment of the joint or separate DL/UL beam indication   + FFS: whether any existing timing defined for DCI based TCI/spatial relation update can be used for X/Y * FFS: When to apply the minimum indication delay (e.g., when the newly indicated beam is different with the previously indicated beam) |

From round-2B discussion, the following proposal for refining Alt1 was made (Qualcomm, Spreadtrum: reworded from UE perspective):

* Alt1: the first slot that is at least X ms or Y symbols after the DCI with the joint or separate DL/UL beam indication
  + The UE may assume that the (gNB-)configured application time is after the acknowledgement.

Some companies also commented that the decision on beam application time (BAT) should be dependent on the decision whether an additional DCI format for beam indication is supported or not.

|  |
| --- |
| **Proposal 3.1**: On Rel.17 DCI-based beam indication, regarding application time of the beam indication: if beam indication is received, down-select (no later than RAN1#105-e) from the following:   * Alt1A: the first slot that is at least X ms or Y symbols after the DCI with the joint or separate DL/UL beam indication * Alt1B: the first slot that is at least X ms or Y symbols after the DCI with the joint or separate DL/UL beam indication   + In addition, the UE may assume that the (gNB-)configured application time is after the acknowledgement * Alt2: the first slot that is at least X ms or Y symbols after the acknowledgment of the joint or separate DL/UL beam indication * FFS: whether any existing timing defined for DCI based TCI/spatial relation update can be used for X/Y   FFS: When to apply the minimum indication delay (e.g., when the newly indicated beam is different with the previously indicated beam) |

|  |
| --- |
| Action: Interested companies are encouraged to provide their inputs on the proposal.  Goal: Finalize the proposal for endorsement |

Table 6 Inputs: issue 3

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | Proposal 3.1 is essentially the previous agreement with Alt1B added and a deadline for decision. The new part is highlighted in blue |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 4 (MP-UE)

Table 7 Summary: issue 4

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **Issue** | **Companies’ views** | **Moderator notes** |
| 4.1 | Entity pertaining to an UL panel for the purpose of UE-initiated panel selection (of one) and activation (of ≥1)  Note: support for UE-initiated panel selection/activation was agreed (but spec support is still FFS – see 4.2) | Alternatives:   * Newly defined panel ID(s): Lenovo/MoM (study), LGE, Xiaomi, NTT Docomo, Qualcomm, Spreadtrum, ZTE, Huawei/HiSi (virtual concept without mandating physical UE panel implementation), IDC, APT, CMCC   + Not needed: AT&T, CATT, Ericsson, OPPO, Nokia/NSB * SSBRI(s)/CRI(s) or CSI-RS resource set ID(s): IDC, Samsung, MTK(SSBRI(s)/CRI(s)), Xiaomi, CATT * SRI(s) or SRS resource set ID(s): vivo, Qualcomm, Xiaomi, Sony (SRS resource set ID(s)), Fraunhofer IIS/HHI, Huawei/HiSi, APT * Antenna port group: Apple, Qualcomm, Nokia/NSB | |

|  |
| --- |
| Previous agreement (RAN1#102-e):   * The following assumptions are used:   1. In terms of RF functionality, a UE panel comprises a collection of TXRUs that is able to generate one analog beam (one beam may correspond to two antenna ports if dual-polarized array is used) |

Regardless of whether a newly defined panel ID is needed or not, (from the above summary) there are two main categories on what constitutes a panel:

* A group of antenna ports
* A group of RS resources (abstraction of “analog beam”)
  + For beam indication, the RS is a measurement RS
  + For CSI/beam reporting, the RS is a source RS for UL TX spatial filter information

|  |
| --- |
| Action: Interested companies are encouraged to provide their inputs on the following alternatives:   * Alt1. A panel entity corresponds to a group of antenna ports * Alt2. A panel entity corresponds to a group RS resources   + For beam indication, the RS is a measurement RS   + For CSI/beam reporting, the RS is a source RS for UL TX spatial filter information   Goal: Finalize the proposal to be ready for endorsement |

|  |
| --- |
| **Proposal 4.1**: On Rel.17 enhancement for facilitating fast uplink panel selection,   * … |

Table 8 Inputs: issue 4

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | Please provide answers to the question |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 5 (MPE mitigation)

|  |
| --- |
| Latest version of proposal 5.1 (FL):  **Proposal 5.1**: On Rel.17 enhancements to facilitate MPE mitigation:   * Decide in RAN1#104bis-e whether the following combinations should be further studied (not necessarily, but can be, in one reporting instance):   + {Rel.16 P-MPR based (beam/panel-level)} + {A}, where A is either Opt 2 or Opt3 or Opt4   + {SSBRI(s)/CRI(s) and/or panel indication} + {A}, where A is either Opt1 or Opt2 or both (Opt1 and Opt2) or Opt4 * Option 1: L1-RSRP [L1-SINR] associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)   + FFS: How panel-level L1-RSRP [L1-SINR] is calculated if L1-RSRP [L1-SINR] is associated with panel   + FFS: Whether/how to include MPE effect in L1-RSRP [L1-SINR], e.g. by using scaled or modified L1-RSRP [L1-SINR]   + FFS: Whether/how to enhance existing beam reporting format to support Option 1 * Option 2: Virtual PHR or a modified version associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured) * Option 3: Virtual PHR or a modified version associated with each activated UL TCI or, if applicable, joint TCI * Option 4: No additional report   Intel’s version of proposal 5.1:  **Proposal 5.1**: On Rel.17 enhancements to facilitate MPE mitigation:   * Decide in RAN1#104bis-e whether the following ~~combinations~~ should be further studied (not necessarily, but can be, in one reporting instance):   + {Rel.16 P-MPR based (beam/panel-level)} + {A}, where A is either Opt1A, Opt1B, or Opt1C:     - Option 1A: Virtual PHR or a modified version associated with each activated UL TCI or, if applicable, joint TCI     - Option 1B: {SSBRI(s)/CRI(s) and/or panel indication}     - Option 1C: No additional reporting quantity   + {SSBRI(s)/CRI(s) and/or panel indication} + {A}, where A is either Opt2A, Opt2B, Opt2A+ Opt2B, or Option 2C     - Option 2A: L1-RSRP [L1-SINR] associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)       * FFS: How panel-level L1-RSRP [L1-SINR] is calculated if L1-RSRP [L1-SINR] is associated with panel       * FFS: Whether/how to include MPE effect in L1-RSRP [L1-SINR], e.g. by using scaled or modified L1-RSRP [L1-SINR]       * FFS: Whether/how to enhance existing beam reporting format to support Option 1     - Option 2B: Virtual PHR or a modified version associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)     - Option 2C: No additional reporting quantity |

Intel’s version disseminates each reporting format more clearly. We will use that as a starting point for this round and refine it while being mindful of the latest FL version (in terms of content):

|  |
| --- |
| **Proposal 5.1**: On Rel.17 enhancements to facilitate MPE mitigation, decide in RAN1#104bis-e whether the following should be further studied (not necessarily, but can be, in one reporting instance):   * {Rel.16 P-MPR based (beam/panel-level)} + {A}, where A is either Opt1A, Opt1B, or Opt1C:   + Option 1A: Virtual PHR or a modified version associated with each activated UL TCI or, if applicable, joint TCI   + Option 1B: {SSBRI(s)/CRI(s) and/or panel indication}   + Option 1C: No additional reporting quantity * {SSBRI(s)/CRI(s) and/or panel indication} + {A}, where A is either Opt2A, Opt2B, Opt2A+ Opt2B, or Option 2C   + Option 2A: L1-RSRP [L1-SINR] associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)     - FFS: How panel-level L1-RSRP [L1-SINR] is calculated if L1-RSRP [L1-SINR] is associated with panel     - FFS: Whether/how to include MPE effect in L1-RSRP [L1-SINR], e.g. by using scaled or modified L1-RSRP [L1-SINR]     - FFS: Whether/how to enhance existing beam reporting format to support Option 1   + Option 2B: Virtual PHR or a modified version associated with each of the reported SSBRI(s)/CRI(s) and/or panel indication (if configured)   + Option 2C: No additional reporting quantity |

|  |
| --- |
| Action: Interested companies are encouraged to provide their inputs on the proposal  Goal: Finalize the proposal to be ready for endorsement |

Table 9 Inputs: issue 5

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | 5.1: Using the latest Intel’s version |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

### Issue 6 (beam refinement/tracking)

This is the status after the second GTW (online) session 01/29/2021.

|  |
| --- |
| **Possible Agreement**  On Rel.17 enhancements based on the unified TCI framework, perform study and, if needed, specify the following:   * Beam management with reduced DL signaling to reduce latency * Reducing activation delay of TCI states and PL-RSs (including other WGs, e.g. RAN4)   + On RAN4-related matters, assessment/study phase can be done in RAN1. If RAN4-based enhancements are found necessary, a LS to RAN4 will be sent (to prepare RAN4 work)   Note: Given its dependence on the maturity of and lower priority compared to other issues (1 to 5), when to start the work and how much work is done on issue 6 should depend on the progress on the other issues.  **Objected by** Huawei/HiSi  **Support by** Futurewei (clarify 2nd bullet), MTK, Samsung, OPPO, Apple, Intel, NTT Docomo, Qualcomm (clarify 2nd bullet), Ericsson, IDC, Spreadtrum (after other issues progress enough), Xiaomi, Nokia/NSB (clarify 2nd bullet), Convida (after other issues progress enough), Lenovo/MoM, CATT, ZTE, NEC, Sony, Verizon Wireless, KT Corporation |