**3GPP TSG RAN WG1 #110bis-e R1-22xxxxx**

**e-Meeting, October 10th – 19th, 2022**

Agenda Item: 7.2

Source: Google

Title: Summary on email discussion 110bis-e-NR-R16-04

Document for: Discussion/Decision

# Introduction

In this contribution, we provided a summary on email discussion 110bis-e-NR-R16-04, which is about the draft CR R1-2208870 with the following proposed changes:

|  |
| --- |
| 6 Link recovery procedures A UE can be provided, for each BWP of a serving cell, a set  of periodic CSI-RS resource configuration indexes by *failureDetectionResourcesToAddModList* and a set  of periodic CSI-RS resource configuration indexes and/or SS/PBCH block indexes by *candidateBeamRSList* or *candidateBeamRSListExt* or *candidateBeamRSSCellList* for radio link quality measurements on the BWP of the serving cell. If the UE is not provided  by *failureDetectionResourcesToAddModList* for a BWP of the serving cell, the UE determines the set  to include periodic CSI-RS resource configuration indexes with same values as the RS indexes in the RS sets indicated by *TCI-State* for respective CORESETs that the UE uses for monitoring PDCCH and, if there are two RS indexes in a TCI state, the set  includes RS indexes configured with *qcl-Type* set to 'typeD' for the corresponding TCI states. The UE expects the set  to include up to two RS indexes. The UE expects single port RS in the set . For the SCell, the UE expects single-port or two-port CSI-RS with frequency density equal to 1 or 3 REs per RB in the set . |

The reason for the change is as follows:

|  |  |
| --- | --- |
| ***Reason for change:*** | In Rel-16, SCell BFR was introduced and the following sentence is defined to restrict the configuration for CBD RS configuration. However, there is no such sentence defined in Rel-15 spec, where PCell BFR is supported. It is unclear whether the following sentence is also applied to PCell BFR.  “The UE expects single-port or two-port CSI-RS with frequency density equal to 1 or 3 REs per RB in the set .” |
|  |  |
| ***Summary of change:*** | Clarify that the restriction on CBD RS configuration is for Rel-16 SCell BFR only. |
|  |  |
| ***Consequences if not approved:*** | It is unclear whether the restriction on CBD RS configuration in Rel-16 spec is also applied to PCell BFR. |

# Discussion

**Q1: Is the sentence “The UE expects single-port or two-port CSI-RS with frequency density equal to 1 or 3 REs per RB in the set .” in Rel-16 spec (not in Rel-15 spec) applied to spCell BFR?**

|  |  |  |
| --- | --- | --- |
| Company | Y or N? | Comments |
| Samsung | N | The sentence is for Rel-16 only. |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: If “No” to the Q1, do you agree with the proposed CR?**

|  |  |  |
| --- | --- | --- |
| Company | Y or N? | Comments |
| Samsung | Y | We support the CR. |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3: If “Yes” to the Q1, how can UE distinguish whether it is communicating with a Rel-15 or Rel-16 gNB? Incorrect configuration may cause some additional UE behavior.**

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |