**3GPP TSG-RAN WG1 Meeting #101-e *R1-200xxxx***

**E-meeting, 25 May – 5 June, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.212** | **CR** | **xx** | **rev** |  | **Current version:** | **16.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Corrections for NR IAB |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_IAB-Core |  | ***Date:*** | 2020-06-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | 1. Reference on soft resources to TS 38.473 is missing
2. The maximum size of DCI format 2\_5 is in brackets
 |
|  |  |
| ***Summary of change:*** | 1. Change Clause [x.x] to Clause 9.3.1.
2. Remove the bracket of [128].
 |
|  |  |
| ***Consequences if not approved:*** | 1. The reference of soft resources to TS 38.473 is not accurate
2. The maximum size of DCI format 2\_5 is not defined
 |
|  |  |
| ***Clauses affected:*** | 7.3.1, 7.3.1.3.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **N** |  Other core specifications  |   |
| ***affected:*** |  | **N** |  Test specifications |  |
| ***(show related CRs)*** |  | **N** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### 7.3.1 DCI formats

The DCI formats defined in table 7.3.1-1 are supported.

Table 7.3.1-1: DCI formats

|  |  |
| --- | --- |
| **DCI format** | **Usage** |
| 0\_0 | Scheduling of PUSCH in one cell |
| 0\_1 | Scheduling of one or multiple PUSCH in one cell, or indicating downlink feedback information for configured grant PUSCH (CG-DFI) |
| 0\_2 | Scheduling of PUSCH in one cell |
| 1\_0 | Scheduling of PDSCH in one cell |
| 1\_1 | Scheduling of PDSCH in one cell, and/or triggering one shot HARQ-ACK codebook feedback |
| 1\_2 | Scheduling of PDSCH in one cell |
| 2\_0 | Notifying a group of UEs of the slot format, available RB sets, COT duration and search space set group switching |
| 2\_1 | Notifying a group of UEs of the PRB(s) and OFDM symbol(s) where UE may assume no transmission is intended for the UE |
| 2\_2 | Transmission of TPC commands for PUCCH and PUSCH |
| 2\_3 | Transmission of a group of TPC commands for SRS transmissions by one or more UEs |
| 2\_4 | Notifying a group of UEs of the PRB(s) and OFDM symbol(s) where UE cancels the corresponding UL transmission from the UE |
| 2\_5 | Notifying the availability of soft resources as defined in Clause 9.3.1 of [10, TS 38.473] |
| 2\_6 | Notifying the power saving information outside DRX Active Time for one or more UEs |
| 3\_0 | Scheduling of NR sidelink in one cell |
| 3\_1 | Scheduling of LTE sidelink in one cell |

< Unchanged parts are omitted >

7.3.1.3.6 Format 2\_5

DCI format 2\_5 is used for notifying the availability of soft resources as defined in Clause 9.3.1 of [10, TS 38.473]

The following information is transmitted by means of the DCI format 2\_5 with CRC scrambled by AI-RNTI:

- Availability indicator 1, Availability indicator 2, …, Availability indicator *N*.

The size of DCI format 2\_5 with CRC scrambled by AI-RNTI is configurable by higher layers up to 128 bits, according to Clause 14 of [5, TS 38.213].

< Unchanged parts are omitted >